=============================================================================
List of generated methods in project: pokus1

THIS TEXT DESCRIPTION IS GENERATED BY THE TOOL. DO NOT MODIFY IT.
=============================================================================

Module "AS1"       (bean AsynchroSerial)
   - AS1_Enable -Enables the bean - it starts the send and receive functions. Events may be generated 
                ("DisableEvent"/"EnableEvent").
   - AS1_Disable -Disables the bean - it stops the send and receive functions. No events will be generated.
   - AS1_RecvChar -If any data is received, this method returns one character, otherwise it returns an error code (it does not 
                wait for data). This method is enabled only if the receiver property is enabled.  [Note:] Because the preferred 
                method to handle error and break exception in the interrupt mode is to use events <OnError> and <OnBreak> the 
                return value ERR_RXEMPTY has higher priority than other error codes. As a consequence the information about an 
                exception in interrupt mode is returned only if there is a valid character ready to be read. Version specific 
                information for Freescale 56800 derivatives ]   DMA mode:  If DMA controller is available on the selected CPU 
                and the receiver is configured to use DMA controller then this method only sets the selected DMA channel. Then 
                the status of the DMA transfer can be checked using GetCharsInRxBuf method. See an example of a typical usage 
                for details about the communication using DMA.
   - AS1_SendChar -Sends one character to the channel. If the bean is temporarily disabled (Disable method) SendChar method 
                only stores data into an output buffer. In case of a zero output buffer size, only one character can be stored. 
                Enabling the bean (Enable method) starts the transmission of the stored data. This method is available only if 
                the transmitter property is enabled.  Version specific information for Freescale 56800 derivatives ]   DMA mode:
                If DMA controller is available on the selected CPU and the transmitter is configured to use DMA controller then 
                this method only sets selected DMA channel. Then the status of the DMA transfer can be checked using 
                GetCharsInTxBuf method. See an example of a typical usage for details about communication using DMA.

Module "AS2"       (bean AsynchroSerial)
   - AS2_Enable -Enables the bean - it starts the send and receive functions. Events may be generated 
                ("DisableEvent"/"EnableEvent").
   - AS2_Disable -Disables the bean - it stops the send and receive functions. No events will be generated.
   - AS2_RecvChar -If any data is received, this method returns one character, otherwise it returns an error code (it does not 
                wait for data). This method is enabled only if the receiver property is enabled.  [Note:] Because the preferred 
                method to handle error and break exception in the interrupt mode is to use events <OnError> and <OnBreak> the 
                return value ERR_RXEMPTY has higher priority than other error codes. As a consequence the information about an 
                exception in interrupt mode is returned only if there is a valid character ready to be read. Version specific 
                information for Freescale 56800 derivatives ]   DMA mode:  If DMA controller is available on the selected CPU 
                and the receiver is configured to use DMA controller then this method only sets the selected DMA channel. Then 
                the status of the DMA transfer can be checked using GetCharsInRxBuf method. See an example of a typical usage 
                for details about the communication using DMA.
   - AS2_SendChar -Sends one character to the channel. If the bean is temporarily disabled (Disable method) SendChar method 
                only stores data into an output buffer. In case of a zero output buffer size, only one character can be stored. 
                Enabling the bean (Enable method) starts the transmission of the stored data. This method is available only if 
                the transmitter property is enabled.  Version specific information for Freescale 56800 derivatives ]   DMA mode:
                If DMA controller is available on the selected CPU and the transmitter is configured to use DMA controller then 
                this method only sets selected DMA channel. Then the status of the DMA transfer can be checked using 
                GetCharsInTxBuf method. See an example of a typical usage for details about communication using DMA.

Module "Cpu"       (bean MCF52233_80_LQFP)
   - Cpu_EnableInt -Enables all maskable interrupts. This method sets the interrupt level mask group in the SR register by 
                value = 0.
   - Cpu_DisableInt -Disables all maskable interrupts. This method sets the interrupt level mask group in the SR register by 
                value = 7.
   - Cpu_SetIntLevel -Sets the interrupt level mask in the SR register. Interrupt requests are inhibited for all priority 
                levels less than or equal to current level, except edge-sensitive level 7 request, which cannot be masked.
   - Cpu_Delay100US -This method realizes software delay. The length of delay is at least 100 microsecond multiply input 
                parameter [us100]. As the delay implementation is not based on real clock, the delay time may be increased by 
                interrupt service routines processed during the delay. The method is independent on selected speed mode.

===================================================================================
