### Legends

Acronym | Verbose Description
--- | ---
CLK | Global Clock
DG | DataGATE
DGE | DataGATE Enable
GCK0 | Global clock zero
GCK1 | Global clock one
GCK2 | Global clock two
GND | Dedicated Ground Pin
GSR | Global set-reset
GTS0 | Global tristate zero (output enable)
GTS1 | Global tristate one (output enable)
GTS2 | Global tristate two (output enable)
GTS3 | Global tristate three (output enable)
HSTL | High speed Tranciever Logic
I/O | Input/Output
INIT | Initial state
ISP | The use of the JTAG port to program the chip while it is powered in a system.
JTAG | IEEE Standard 1149 (JTAG) boundary-scan test standard.
KPR | Unused I/O with weak keeper (leave unconnected)
NC | Not Connected, unbonded pin
PGND | Programmable ground pin
PROHIBITED | User reserved pin
R | Reset
S | Set
-S | Schmitt trigger input (used with VREF input). Schmitt Trigger 1.5 Volts input only. All inputs set to SCHMITT15IN are automatically configured as schmitt-trigger. LVCMOS15 is allowed only on output-only pins. SCHMITT15IN can be used on any type of pad; output requirements are same as for LVCMOS15.
TCK | One of four terminals required by (JTAG) IEEE Std 1149 or IEEE Std 1532. Test operations of the device are synchronous to TCK. Data is captured on the rising edge of TCK and outputs change on the falling edge of TCK. An internal pull-up forces TCK to a high level if left unconnected.
TDI | One of four terminals required by (JTAG) IEEE Std 1149 or IEEE Std 1532. It is the serial input for shifting data through the instruction register or selected data register. An internal pull-up forces TDI to a high level if left unconnected.
TDO | One of four terminals required by (JTAG) IEEE Std 1149 or IEEE Std 1532. It is the serial output for shifting data through the instruction register or selected data register. An internal pull-up forces TDI to a high level when it is not driven from an external source.
TIE | Unused I/O floating -- must tie to VCC, GND or other signal
TMS | One of four terminals required by (JTAG) IEEE Std 1149 or IEEE Std 1532. It directs the device through its Test Access Port controller states. An internal pull-up forces TDI to a high level when it is not driven from an external source. TMS also provides the optional test reset signal of IEEE Std 1149 or IEEE Std 1532.
VAUX | JTAG port auxiliary supply voltage
LVCMOS15 | External Output supply voltage for LVCMOS15
LVCMOS18 | External I/O supply voltage for LVCMOS18
LVCMOS25 | External I/O supply voltage for LVCMOS25
LVCMOS33 | External I/O supply voltage for LVCMOS33
LVTTL | Low Voltage Transistor Transistor Logic 3.3Volts
SCHMITT15IN | Schmitt Trigger 1.5 Volts input only. All inputs set to SCHMITT15IN are automatically configured as schmitt-trigger. LVCMOS15 is allowed only on output-only pins. SCHMITT15IN can be used on any type of pad; output requirements are same as for LVCMOS15.
SSTL | Stub Switched Tranceiver Logic
VCCIO | External power for Inputs/Outputs
VCCIO-1.5 | External I/O supply voltage for LVCMOS15, HSTL_I
VCCIO-1.8 | External I/O supply voltage for LVCMOS18
VCCIO-2.5 | External I/O supply voltage for LVCMOS25, SSTL2_I
VCCIO-3.3 | External I/O supply voltage for LVTTL, LVCMOS33, SSTL3_I
VCC | Dedicated Power Pin, Internal supply voltage for the device
VREF-[iostd] | Reference voltage for indicated input/output standard
*VREF-[iostd] | Reference voltage pin selected by software
WPU | Unused I/O with Internal Weak Pull Up (leave unconnected)
WPD | Unused I/O with Internal Weak Pull Down (leave unconnected)