### Device Usage Page (device_usage_statistics.html)

This HTML page displays the device usage statistics that will be sent to Xilinx. The file also contains predefined XML tags used to simplify processing.
Please verify the contents are okay to send to Xilinx!

Software Version and Target Device
Product Version: | ISE:9.2i | Target Family: | spartan3
OS Platform: | LIN | Target Device: | xc3s200
Project ID (random number) | 28692.1 | Target Package: | pq208
Date Generated | Po ?en 2 12:48:15 2008 | Target Speed: | -4

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Comparators=8 10-bit comparator greatequal=1 10-bit comparator less=2 12-bit comparator greatequal=1 12-bit comparator lessequal=1 16-bit comparator equal=1 16-bit comparator less=1 4-bit comparator less=1 Registers=86 Flip-Flops=86 Counters=4 10-bit up counter=2 16-bit up counter=1 4-bit up counter=1 | MiscellaneousStatistics AVG_LUT_FAN_IN=2.423100 AVG_SIG_FANOUT=1.900000 FOUR_LOAD_SIG=12 LUT=156 MAX_SIG_FANOUT=17 PK_NUM_4_INPUT_LUTS=156 PK_NUM_BONDED_IOBS=52 PK_NUM_CYINIT=42 PK_NUM_CYMUX=80 PK_NUM_EQUIV_GATES=2 PK_NUM_IOB_FFS=24 PK_NUM_JTAG_GATES=52 PK_NUM_LUTLESS_IOB_FFS=12 PK_NUM_LUTLESS_SLICE_FFS=80 PK_NUM_SLICELS=110 PK_NUM_SLICES=110 PK_NUM_SLICE_FFS=102 PK_NUM_TOTAL_LUTLESS_REGISTERS=92 PK_NUM_XBZ_GCLKS=2 PK_NUM_XOR=36 SINGLE_LOAD_SIG=101 THREE_LOAD_SIG=1 TWO_LOAD_SIG=36 | NetStatistics NumNets_Active=277 NumNets_Gnd=1 NumNets_Vcc=1 NumNodesOfType_Active_CLKPIN=78 NumNodesOfType_Active_CNTRLPIN=124 NumNodesOfType_Active_DOUBLE=548 NumNodesOfType_Active_DUMMY=397 NumNodesOfType_Active_DUMMYESC=29 NumNodesOfType_Active_GLOBAL=42 NumNodesOfType_Active_HFULLHEX=7 NumNodesOfType_Active_HLONG=2 NumNodesOfType_Active_HUNIHEX=36 NumNodesOfType_Active_INPUT=489 NumNodesOfType_Active_IOBOUTPUT=28 NumNodesOfType_Active_OMUX=211 NumNodesOfType_Active_OUTPUT=200 NumNodesOfType_Active_PREBXBY=47 NumNodesOfType_Active_VFULLHEX=37 NumNodesOfType_Active_VLONG=12 NumNodesOfType_Active_VUNIHEX=31 NumNodesOfType_Vcc_CNTRLPIN=2 NumNodesOfType_Vcc_INPUT=10 NumNodesOfType_Vcc_PREBXBY=7 NumNodesOfType_Vcc_VCCOUT=10 | SiteSummary BUFGMUX=2 BUFGMUX_GCLKMUX=2 BUFGMUX_GCLK_BUFFER=2 IOB=52 IOB_DELAY=1 IOB_IFF1=1 IOB_INBUF=28 IOB_OFF1=23 IOB_OUTBUF=36 IOB_PAD=52 SLICEL=110 SLICEL_CYMUXF=42 SLICEL_CYMUXG=38 SLICEL_F=81 SLICEL_FFX=49 SLICEL_FFY=53 SLICEL_G=75 SLICEL_GNDF=22 SLICEL_GNDG=19 SLICEL_XORF=18 SLICEL_XORG=18

Configuration Data
BUFGMUX_GCLKMUX DISABLE_ATTR=[LOW:2] IOB_IFF1 IFF1_INIT_ATTR=[INIT0:1] IFF1_SR_ATTR=[SRLOW:1] IFFATTRBOX=[ASYNC:1] LATCH_OR_FF=[FF:1] | IOB_OFF1 LATCH_OR_FF=[FF:23] OFF1_INIT_ATTR=[INIT0:23] OFF1_SR_ATTR=[SRLOW:11] OFFATTRBOX=[ASYNC:11] IOB_PAD DRIVEATTRBOX=[12:36] IOATTRBOX=[LVCMOS33:52] SLEW=[SLOW:36] | SLICEL_FFX FFX_INIT_ATTR=[INIT0:48] [INIT1:1] FFX_SR_ATTR=[SRLOW:49] LATCH_OR_FF=[FF:49] SYNC_ATTR=[ASYNC:49] SLICEL_FFY FFY_INIT_ATTR=[INIT0:53] FFY_SR_ATTR=[SRLOW:53] LATCH_OR_FF=[FF:53] SYNC_ATTR=[ASYNC:53] |

Pin Data
BUFGMUX I0=2 O=2 S=2 BUFGMUX_GCLKMUX I0=2 OUT=2 S=2 BUFGMUX_GCLK_BUFFER IN=2 OUT=2 IOB I=27 ICLK1=1 IQ1=1 O1=36 OCE=23 OTCLK1=23 PAD=52 REV=10 SR=12 T1=12 IOB_DELAY IN=1 OUT=1 IOB_IFF1 CK=1 D=1 Q=1 SR=1 | IOB_INBUF IN=28 OUT=28 IOB_OFF1 CE=23 CK=23 D=23 Q=23 REV=10 SR=11 IOB_OUTBUF IN=36 OUT=36 TRI=12 IOB_PAD PAD=52 SLICEL BX=28 BY=26 CE=36 CIN=35 CLK=54 COUT=38 F1=81 F2=71 F3=23 F4=10 G1=75 G2=74 G3=29 G4=15 SR=31 X=29 XB=1 XQ=49 Y=25 YQ=53 | SLICEL_CYMUXF 0=42 1=42 OUT=42 S0=42 SLICEL_CYMUXG 0=38 1=38 OUT=38 S0=38 SLICEL_F A1=81 A2=71 A3=23 A4=10 D=81 SLICEL_FFX CE=32 CK=49 D=49 Q=49 SR=27 SLICEL_FFY CE=35 CK=53 D=53 Q=53 SR=31 | SLICEL_G A1=75 A2=74 A3=29 A4=15 D=75 SLICEL_GNDF 0=22 SLICEL_GNDG 0=19 SLICEL_XORF 0=18 1=18 O=18 SLICEL_XORG 0=18 1=18 O=18

Tool Usage
Command Line History xst -ise <ise_file> -intstyle ise -ifn <fname>.xst -ofn <fname>.syr ngdbuild -ise <ise_file> <fname>.ngd map -ise <ise_file> -intstyle ise -p xc3s200-pq208-4 -cm area -pr b -k 4 -c 100 -o <fname>.ncd <fname>.ngd <fname>.pcf par -ise <ise_file> -w -intstyle ise -ol std -t 1 <fname>.ncd <fname>.ncd <fname>.pcf trce -ise <ise_file> -intstyle ise -e 3 -s 4 -xml <design> <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf bitgen -ise <ise_file> -intstyle ise -f <fname>.ut <fname>.ncd