   CPAR00CZE Site Information Form (site log)
     International GNSS Service
     See Instructions at:
       https://files.igscb.org/pub/station/general/sitelog_instr.txt


0.   Form

     Prepared by (full name)  : Jan Reznicek
     Date Prepared            : 2022-02-01
     Report Type              : UPDATE
     If Update:
      Previous Site Log       : cpar00cze_20181006.log
      Modified/Added Sections : 3.15, 3.16


1.   Site Identification of the GNSS Monument

     Site Name                : Pardubice
     Four Character ID        : CPAR
     Monument Inscription     : 
     IERS DOMES Number        : 11527M001
     CDP Number               : (A4)
     Monument Description     : Steel pole
       Height of the Monument : 1.4 m
       Monument Foundation    : Roof of reinforced concrete building
       Foundation Depth       : (m)
     Marker Description       : Center of hole in steel plate
     Date Installed           : 2005-01-11
     Geologic Characteristic  : (BEDROCK/CLAY/CONGLOMERATE/GRAVEL/SAND/etc)
       Bedrock Type           : (IGNEOUS/METAMORPHIC/SEDIMENTARY)
       Bedrock Condition      : (FRESH/JOINTED/WEATHERED)
       Fracture Spacing       : (0 cm/1-10 cm/11-50 cm/51-200 cm/over 200 cm)
       Fault zones nearby     : (YES/NO/Name of the zone)
         Distance/activity    : (multiple lines)
     Additional Information   : Antenna is aproximately 21.5m above ground
                              : level.


2.   Site Location Information

     City or Town             : Pardubice
     State or Province        : Pardubice Region
     Country                  : Czechia
     Tectonic Plate           : EURASIAN
     Approximate Position (ITRF)
       X coordinate (m)       : 3949919.120
       Y coordinate (m)       : 1116467.150
       Z coordinate (m)       : 4865832.520
       Latitude (N is +)      : +500222.37
       Longitude (E is +)     : +0154659.69
       Elevation (m,ellips.)  : 283.3
     Additional Information   : (multiple lines)


3.   GNSS Receiver Information

3.1  Receiver Type            : LEICA GRX1200PRO
     Satellite System         : GPS
     Serial Number            : 453661
     Firmware Version         : 1.52
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2005-01-11
     Date Removed             : 2005-02-08
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.2  Receiver Type            : LEICA GRX1200PRO
     Satellite System         : GPS
     Serial Number            : 453661
     Firmware Version         : 2.12
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2005-02-08
     Date Removed             : 2006-06-05
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.3  Receiver Type            : LEICA GRX1200PRO
     Satellite System         : GPS
     Serial Number            : 453661
     Firmware Version         : 4.00
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2006-06-05
     Date Removed             : 2007-07-31
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.4  Receiver Type            : LEICA GRX1200PRO
     Satellite System         : GPS
     Serial Number            : 453661
     Firmware Version         : 5.50
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2007-07-31
     Date Removed             : 2008-02-06
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.5  Receiver Type            : LEICA GRX1200PRO
     Satellite System         : GPS
     Serial Number            : 453661
     Firmware Version         : 5.62
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2008-02-06
     Date Removed             : 2009-09-04
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.6  Receiver Type            : LEICA GRX1200PRO
     Satellite System         : GPS
     Serial Number            : 453661
     Firmware Version         : 7.53/2.125
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2009-09-04
     Date Removed             : 2010-05-18
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.7  Receiver Type            : LEICA GRX1200PRO
     Satellite System         : GPS
     Serial Number            : 453661
     Firmware Version         : 7.80/2.125
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2010-05-18
     Date Removed             : 2010-06-21
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.8  Receiver Type            : LEICA GRX1200PRO
     Satellite System         : GPS
     Serial Number            : 453661
     Firmware Version         : 8.00/2.125
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2010-06-21
     Date Removed             : 2011-11-10
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.9  Receiver Type            : LEICA GRX1200+GNSS
     Satellite System         : GPS+GLO
     Serial Number            : 457127
     Firmware Version         : 8.20/4.007
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2011-11-10
     Date Removed             : 2015-01-14T10:00Z
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.10 Receiver Type            : LEICA GRX1200+GNSS
     Satellite System         : GPS+GLO
     Serial Number            : 457127
     Firmware Version         : 9.20/6.404
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2015-01-14T10:00Z
     Date Removed             : 2017-04-24T00:00Z
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.11 Receiver Type            : LEICA GRX1200+GNSS
     Satellite System         : GPS+GLO+GAL+SBAS
     Serial Number            : 457127
     Firmware Version         : 9.20/6.404
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2017-04-24T00:00Z
     Date Removed             : 2018-01-06
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.12 Receiver Type            : LEICA GRX1200+GNSS
     Satellite System         : GPS+GLO+GAL+SBAS
     Serial Number            : 457127
     Firmware Version         : 9.20/6.405
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2018-01-06
     Date Removed             : 2018-01-18
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.13 Receiver Type            : LEICA GRX1200+GNSS
     Satellite System         : GPS+GLO+GAL+BDS
     Serial Number            : 457127
     Firmware Version         : 9.20/6.405
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2018-01-19
     Date Removed             : 2018-01-20
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.14 Receiver Type            : LEICA GRX1200+GNSS
     Satellite System         : GPS+GLO+GAL+BDS+SBAS
     Serial Number            : 457127
     Firmware Version         : 9.20/6.405
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2018-01-20
     Date Removed             : 2018-10-04
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.15 Receiver Type            : LEICA GR30
     Satellite System         : GPS+GLO+GAL+BDS+QZSS+SBAS
     Serial Number            : 1706461
     Firmware Version         : 4.31/7.403
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2018-10-04
     Date Removed             : 2022-02-17T22:30Z
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.16 Receiver Type            : LEICA GR30
     Satellite System         : GPS+GLO+GAL+BDS+QZSS+SBAS
     Serial Number            : 1706461
     Firmware Version         : 4.52/7.711
     Elevation Cutoff Setting : 0 deg
     Date Installed           : 2022-02-17T22:45Z
     Date Removed             : CCYY-MM-DDThh:mmZ
     Temperature Stabiliz.    : (deg C) +/- (deg C)
     Additional Information   : (multiple lines)

3.x  Receiver Type            : (A20, from rcvr_ant.tab; see instructions)
     Satellite System         : (GPS+GLO+GAL+BDS+QZSS+IRNSS+SBAS)
     Serial Number            : (A20, but note the first A5 is used in SINEX)
     Firmware Version         : (A11)
     Elevation Cutoff Setting : (deg)
     Date Installed           : (CCYY-MM-DDThh:mmZ)
     Date Removed             : (CCYY-MM-DDThh:mmZ)
     Temperature Stabiliz.    : (none or tolerance in degrees C)
     Additional Information   : (multiple lines)


4.   GNSS Antenna Information

4.1  Antenna Type             : LEIAT504        LEIS
     Serial Number            : 102546
     Antenna Reference Point  : BPA
     Marker->ARP Up Ecc. (m)  :   0.0651
     Marker->ARP North Ecc(m) :   0.0000
     Marker->ARP East Ecc(m)  :   0.0000
     Alignment from True N    : 0 deg
     Antenna Radome Type      : LEIS
     Radome Serial Number     : 
     Antenna Cable Type       : (vendor & type number)
     Antenna Cable Length     : (m)
     Date Installed           : 2005-01-11
     Date Removed             : 2011-10-25
     Additional Information   : (multiple lines)

4.2  Antenna Type             : LEIAR25.R4      LEIT
     Serial Number            : 10401009
     Antenna Reference Point  : BPA
     Marker->ARP Up Ecc. (m)  :   0.0656
     Marker->ARP North Ecc(m) :   0.0000
     Marker->ARP East Ecc(m)  :   0.0000
     Alignment from True N    : 0 deg
     Antenna Radome Type      : LEIT
     Radome Serial Number     : 
     Antenna Cable Type       : (vendor & type number)
     Antenna Cable Length     : (m)
     Date Installed           : 2011-10-25
     Date Removed             : CCYY-MM-DDThh:mmZ
     Additional Information   : (multiple lines)

4.x  Antenna Type             : (A20, from rcvr_ant.tab; see instructions)
     Serial Number            : (A*, but note the first A5 is used in SINEX)
     Antenna Reference Point  : (BPA/BCR/XXX from "antenna.gra"; see instr.)
     Marker->ARP Up Ecc. (m)  : (F8.4)
     Marker->ARP North Ecc(m) : (F8.4)
     Marker->ARP East Ecc(m)  : (F8.4)
     Alignment from True N    : (deg; + is clockwise/east)
     Antenna Radome Type      : (A4 from rcvr_ant.tab; see instructions)
     Radome Serial Number     : 
     Antenna Cable Type       : (vendor & type number)
     Antenna Cable Length     : (m)
     Date Installed           : (CCYY-MM-DDThh:mmZ)
     Date Removed             : (CCYY-MM-DDThh:mmZ)
     Additional Information   : (multiple lines)


5.   Surveyed Local Ties

5.x  Tied Marker Name         : 
     Tied Marker Usage        : (SLR/VLBI/LOCAL CONTROL/FOOTPRINT/etc)
     Tied Marker CDP Number   : (A4)
     Tied Marker DOMES Number : (A9)
     Differential Components from GNSS Marker to the tied monument (ITRS)
       dx (m)                 : (m)
       dy (m)                 : (m)
       dz (m)                 : (m)
     Accuracy (mm)            : (mm)
     Survey method            : (GPS CAMPAIGN/TRILATERATION/TRIANGULATION/etc)
     Date Measured            : (CCYY-MM-DDThh:mmZ)
     Additional Information   : (multiple lines)


6.   Frequency Standard

6.1  Standard Type            : INTERNAL 
       Input Frequency        : (if external)
       Effective Dates        : 2005-01-11/CCYY-MM-DD
       Notes                  : (multiple lines)

6.x  Standard Type            : (INTERNAL or EXTERNAL H-MASER/CESIUM/etc)
       Input Frequency        : (if external)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Notes                  : (multiple lines)


7.   Collocation Information

7.x  Instrumentation Type     : (GPS/GLONASS/DORIS/PRARE/SLR/VLBI/TIME/etc)
       Status                 : (PERMANENT/MOBILE)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Notes                  : (multiple lines)


8.   Meteorological Instrumentation

8.1.x  Humidity Sensor Model  : 
       Manufacturer           : 
       Serial Number          : 
       Data Sampling Interval : (sec)
       Accuracy (% rel h)     : (% rel h)
       Aspiration             : (UNASPIRATED/NATURAL/FAN/etc)
       Height Diff to Ant     : (m)
       Calibration date       : (CCYY-MM-DD)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Notes                  : (multiple lines)

8.2.x  Pressure Sensor Model  : 
       Manufacturer           : 
       Serial Number          : 
       Data Sampling Interval : (sec)
       Accuracy               : (hPa)
       Height Diff to Ant     : (m)
       Calibration date       : (CCYY-MM-DD)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Notes                  : (multiple lines)

8.3.x  Temp. Sensor Model     : 
       Manufacturer           : 
       Serial Number          : 
       Data Sampling Interval : (sec)
       Accuracy               : (deg C)
       Aspiration             : (UNASPIRATED/NATURAL/FAN/etc)
       Height Diff to Ant     : (m)
       Calibration date       : (CCYY-MM-DD)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Notes                  : (multiple lines)

8.4.x  Water Vapor Radiometer : 
       Manufacturer           : 
       Serial Number          : 
       Distance to Antenna    : (m)
       Height Diff to Ant     : (m)
       Calibration date       : (CCYY-MM-DD)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Notes                  : (multiple lines)

8.5.x  Other Instrumentation  : (multiple lines)


9.   Local Ongoing Conditions Possibly Affecting Computed Position

9.1.x  Radio Interferences    : (TV/CELL PHONE ANTENNA/RADAR/etc)
       Observed Degradations  : (SN RATIO/DATA GAPS/etc)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Additional Information : (multiple lines)

9.2.x  Multipath Sources      : (METAL ROOF/DOME/VLBI ANTENNA/etc)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Additional Information : (multiple lines)

9.3.x  Signal Obstructions    : (TREES/BUILDINGS/etc)
       Effective Dates        : (CCYY-MM-DD/CCYY-MM-DD)
       Additional Information : (multiple lines)


10.  Local Episodic Effects Possibly Affecting Data Quality

10.x  Date                    : (CCYY-MM-DD/CCYY-MM-DD)
      Event                   : (TREE CLEARING/CONSTRUCTION/etc)


11.  On-Site, Point of Contact Agency Information

     Agency                   : Land Survey Office
                              : Geodetic Control Department
     Preferred Abbreviation   : ZU
     Mailing Address          : Pod Sidlistem 9
                              : Praha 8 - Kobylisy
                              : Czechia
     Primary Contact
       Contact Name           : Jan Reznicek
       Telephone (primary)    : +420 284 041 530
       Telephone (secondary)  : 
       Fax                    : +420 284 041 625
       E-mail                 : jan.reznicek@cuzk.cz
     Secondary Contact
       Contact Name           : Miluse Snajdrova
       Telephone (primary)    : +420 284 041 533
       Telephone (secondary)  : 
       Fax                    : +420 284 041 625
       E-mail                 : miluse.snajdrova@cuzk.cz
     Additional Information   : Additional Contacts
                              : Name:   Lubos Nedorost
                              : E-mail: lubos.nedorost@cuzk.cz
                              : 




12.  Responsible Agency (if different from 11.)

     Agency                   : (multiple lines)
     Preferred Abbreviation   : (A10)
     Mailing Address          : (multiple lines)
     Primary Contact
       Contact Name           : 
       Telephone (primary)    : 
       Telephone (secondary)  : 
       Fax                    : 
       E-mail                 : 
     Secondary Contact
       Contact Name           : 
       Telephone (primary)    : 
       Telephone (secondary)  : 
       Fax                    : 
       E-mail                 : 
     Additional Information   : (multiple lines)


13.  More Information

     Primary Data Center      : BEV
     Secondary Data Center    : BKG
     URL for More Information : 
     Hardcopy on File
       Site Map               : (Y or URL)
       Site Diagram           : (Y or URL)
       Horizon Mask           : (Y or URL)
       Monument Description   : (Y or URL)
       Site Pictures          : (Y or URL)
     Additional Information   : (multiple lines)
     Antenna Graphics with Dimensions

LEIAT504      LEIS

                         +-------+                          <-- 0.1393
                       /     +     \
                      |      +      |
    +-----------------+-------------+------------------+    <-- 0.1012 TCR
    |                                                  |
    |                                                  |
    |                                                  |
    |                                                  |
  +-+--------------------------------------------------+-+
  +-------------------+-------------+--------------------+  <-- 0.0345 BCR
                      |             |
                      |             |
                      +------x------+                       <-- 0.000  BPA=ARP

  <--                      0.3794                      -->


LEIAR25.R4      LEIT from 2011-10-26
                       +-------+                          <--  0.1995
                      /
                +---+-------------+---+                   <--  0.1606  TCR
                |                     |
             |---------------------------|
          |---------------------------------|
       |---------------------------------------|
    +---------------------------------------------+
    |                                             |
    |                                             |
  +-+---------------------------------------------+-+
  +-----------------+-------------+-----------------+     <--  0.0320  BCR
                    |             |
                    |             |
                    +------x------+                       <--  0.0000  BPA=ARP

  <--                    0.3802                   -->



ARP: Antenna Reference Point
L1 : L1 Phase Center                   L2 : L2 Phase Center
TCR: Top of Chokering                  BCR: Bottom of Chokering
TGP: Top of Ground Plane               BGP: Bottom of Ground Plane
TPA: Top of Preamplifier               BPA: Bottom of Preamplifier
TOP: Top of Pole