WORKSTATION: A02-0831C
DATE: Monday, May 24, 2010
TIME: 11:08:03 AM
OPERATOR: Olivik
NUMBER OF TESTS: 13
RESULT: passed

InitializeTestSuite
    INFO    Log initialized
    INFO    Microsoft Windows XP (Build 2600)
    INFO    Service Pack 3.0
    INFO    USBCommandVerifier.dll ver 1.3.3.3
    INFO    TestServices.dll ver 1.3.3.5
    INFO    StackSwitcher.dll ver 1.3.3.3
DeviceDescriptorTest_DeviceConfigured | Passed
    INFO

    ===============

    Now Starting Test: Device Descriptor Test (Configuration Index 0)

    INFO    Start time: 11:07:17

    INFO    Device descriptor length : 12
    INFO    Device descriptor type : 1
    INFO    Major version : 2
    INFO    Minor version : 0
    INFO    Each interface specifies its own device class type
    INFO    Device sub class : 0
    INFO    Device protocol : 0
    INFO    Device MaxPacketSize0 : 8
    ABORT   Create file on 'usb.if' failed
    WARNING Failed to get vendor information for VendorID : 4d8
    INFO    Device ProductID : feec
    INFO    Device BCD : 1
    INFO    ENGLISH_US           language string descriptor is : Lukas Olivik, UREL FEKT VUT Brno
    INFO    ENGLISH_US           language string descriptor is : Rotacni ovladac k PC
    INFO    Device Serial Number String : 0
    INFO    Number of configurations device supports : 1
    INFO    Stop time: 11:07:18
    INFO    Stopping Test [ Device Descriptor Test (Configuration Index 0):
         Number of: Fails (0); Aborts (1); Warnings (1) ]
DeviceDescriptorTest_DeviceAddressed | Passed
    INFO

    ===============

    Now Starting Test: Device Descriptor Test (Configuration Index 0)

    INFO    Start time: 11:07:18

    INFO    Device descriptor length : 12
    INFO    Device descriptor type : 1
    INFO    Major version : 2
    INFO    Minor version : 0
    INFO    Each interface specifies its own device class type
    INFO    Device sub class : 0
    INFO    Device protocol : 0
    INFO    Device MaxPacketSize0 : 8
    ABORT   Create file on 'usb.if' failed
    WARNING Failed to get vendor information for VendorID : 4d8
    INFO    Device ProductID : feec
    INFO    Device BCD : 1
    INFO    ENGLISH_US           language string descriptor is : Lukas Olivik, UREL FEKT VUT Brno
    INFO    ENGLISH_US           language string descriptor is : Rotacni ovladac k PC
    INFO    Device Serial Number String : 0
    INFO    Number of configurations device supports : 1
    INFO    Stop time: 11:07:19
    INFO    Stopping Test [ Device Descriptor Test (Configuration Index 0):
         Number of: Fails (0); Aborts (1); Warnings (1) ]
ConfigDescriptorTest_DeviceConfigured | Passed
    INFO

    ===============

    Now Starting Test: Configuration Descriptor Test (Configuration Index 0)

    INFO    Start time: 11:07:19

    INFO    Number of interface descriptors found 1
    INFO    Number of alternate interface descriptors found : 0
    INFO    Number of endpoint descriptors found : 2
    INFO    Configuration descriptor length : 9
    INFO    Configuration descriptor type : 2
    INFO    Configuration descriptor TotalLength : 29
    INFO    Configuration descriptor NumInterfaces : 1
    INFO    Configuration descriptor ConfigurationValue: 1
    INFO    Configuration descriptor string descriptor index : 0
    INFO    Configuration descriptor bmAttributes : 80
    INFO    Device does not support remote wake up
    INFO    Maximum power device requires : 100mA
    INFO    Device is BUS POWERED
    INFO    Device is currently BUS POWERED
    INFO    Currently remote wakeup is DISABLED
    INFO    Stop time: 11:07:20
    INFO    Stopping Test [ Configuration Descriptor Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
ConfigDescriptorTest_DeviceAddressed | Passed
    INFO

    ===============

    Now Starting Test: Configuration Descriptor Test (Configuration Index 0)

    INFO    Start time: 11:07:20

    INFO    Number of interface descriptors found 1
    INFO    Number of alternate interface descriptors found : 0
    INFO    Number of endpoint descriptors found : 2
    INFO    Configuration descriptor length : 9
    INFO    Configuration descriptor type : 2
    INFO    Configuration descriptor TotalLength : 29
    INFO    Configuration descriptor NumInterfaces : 1
    INFO    Configuration descriptor ConfigurationValue: 1
    INFO    Configuration descriptor string descriptor index : 0
    INFO    Configuration descriptor bmAttributes : 80
    INFO    Device does not support remote wake up
    INFO    Maximum power device requires : 100mA
    INFO    Device is BUS POWERED
    INFO    Device is currently BUS POWERED
    INFO    Currently remote wakeup is DISABLED
    INFO    Stop time: 11:07:21
    INFO    Stopping Test [ Configuration Descriptor Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
InterfaceDescriptorTest | Passed
    INFO

    ===============

    Now Starting Test: Interface Descriptor Test (Configuration Index 0)

    INFO    Start time: 11:07:21

    INFO    Bandwidth check passed
    INFO    Testing Interface number : 0 Alternate setting : 0
    INFO    Interface descriptor length : 9
    INFO    Interface descriptor bDescriptorType : 4
    INFO    Interface descriptor bAlternateSetting : 0
    INFO    Interface descriptor bNumEndPoints: 2
    INFO    Interface descriptor bInterfaceClass reserved for assignment by the USB-IF : 3
    INFO    Interface class code indicates [HID] Interface
    INFO    Interface descriptor bInterfaceSubClass : 0
    INFO    Device does not use a class-specific protocol on this interface
    INFO    Interface descriptor iInterface : 0x0
    INFO    Stop time: 11:07:22
    INFO    Stopping Test [ Interface Descriptor Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
EndpointDescriptorTest_DeviceConfigured | Passed
    INFO

    ===============

    Now Starting Test: Endpoint Descriptor Test (Configuration Index 0)

    INFO    Start time: 11:07:22

    INFO    Testing Interface number : 0 Alternate setting : 0
    INFO    Endpoint descriptor length : 7
    INFO    Endpoint descriptor type : 5
    INFO    Endpoint Type : Interrupt, Number : 1, Direction : IN
    INFO    Endpoint descriptor bmAttributes : 3
    INFO    Endpoint descriptor raw MaxPacketSize : 5
    INFO    Endpoint descriptor interval : a
    INFO    Endpoint descriptor length : 7
    INFO    Endpoint descriptor type : 5
    INFO    Endpoint Type : Interrupt, Number : 1, Direction : OUT
    INFO    Endpoint descriptor bmAttributes : 3
    INFO    Endpoint descriptor raw MaxPacketSize : 2
    INFO    Endpoint descriptor interval : a
    INFO    Stop time: 11:07:23
    INFO    Stopping Test [ Endpoint Descriptor Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
EndpointDescriptorTest_DeviceAddressed | Passed
    INFO

    ===============

    Now Starting Test: Endpoint Descriptor Test (Configuration Index 0)

    INFO    Start time: 11:07:23

    INFO    Testing Interface number : 0 Alternate setting : 0
    INFO    Endpoint descriptor length : 7
    INFO    Endpoint descriptor type : 5
    INFO    Endpoint Type : Interrupt, Number : 1, Direction : IN
    INFO    Endpoint descriptor bmAttributes : 3
    INFO    Endpoint descriptor raw MaxPacketSize : 5
    INFO    Endpoint descriptor interval : a
    INFO    Endpoint descriptor length : 7
    INFO    Endpoint descriptor type : 5
    INFO    Endpoint Type : Interrupt, Number : 1, Direction : OUT
    INFO    Endpoint descriptor bmAttributes : 3
    INFO    Endpoint descriptor raw MaxPacketSize : 2
    INFO    Endpoint descriptor interval : a
    INFO    Stop time: 11:07:24
    INFO    Stopping Test [ Endpoint Descriptor Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
HaltEndpointTest | Passed
    INFO

    ===============

    Now Starting Test: Halt Endpoint Test (Configuration Index 0)

    INFO    Start time: 11:07:24

    INFO    Testing Interface number : 0 Alternate setting : 0
    INFO    Testing EndPoint type : Interrupt, Address : 81
    INFO    Endpoint is currently not halted
    INFO    Endpoint is halted
    INFO    Cleared endpoint halt
    INFO    Testing EndPoint type : Interrupt, Address : 1
    INFO    Endpoint is currently not halted
    INFO    Endpoint is halted
    INFO    Cleared endpoint halt
    INFO    Stop time: 11:07:25
    INFO    Stopping Test [ Halt Endpoint Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
SetConfigurationTest | Passed
    INFO

    ===============

    Now Starting Test: SetConfiguration Test (Configuration Index 0)

    INFO    Start time: 11:07:25

    INFO    SetConfiguration with configuration value : 1
    INFO    Unconfigured the device
    INFO    SetConfiguration with configuration value : 1
    INFO    Stop time: 11:07:26
    INFO    Stopping Test [ SetConfiguration Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
SuspendResumeTest | Passed
    INFO

    ===============

    Now Starting Test: Suspend/Resume Test (Configuration Index 0)

    INFO    Start time: 11:07:26

    INFO    Suspended the parent port of the device
    INFO    Stop time: 11:07:28
    INFO    Stopping Test [ Suspend/Resume Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
RemoteWakeupTestEnabled | Passed
    INFO

    ===============

    Now Starting Test: Remote Wakeup Test (Configuration Index 0)

    INFO    Start time: 11:07:28

    INFO    The device does not support remote wakeup
    INFO    Stop time: 11:07:29
    INFO    Stopping Test [ Remote Wakeup Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
RemoteWakeupTestDisabled | Passed
    INFO

    ===============

    Now Starting Test: Remote Wakeup Test (Configuration Index 0)

    INFO    Start time: 11:07:29

    INFO    The device does not support remote wakeup
    INFO    Stop time: 11:07:30
    INFO    Stopping Test [ Remote Wakeup Test (Configuration Index 0):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
EnumerationTest | Passed
    INFO

    ===============

    Now Starting Test: Enumeration Test (repeat 150 times)

    INFO    Start time: 11:07:30

    INFO    Device speed is Full
    INFO    Stop time: 11:08:00
    INFO    Stopping Test [ Enumeration Test (repeat 150 times):
         Number of: Fails (0); Aborts (0); Warnings (0) ]
Summary
    INFO    Summary Log Counts [ Fails (0); Aborts (2); Warnings (2) ]