; Valve: SV2-DI
; Option jumpers: J1-J3 in
;
;   $History: DSTATE1.SCR $
;
;*****************  Version 4  *****************
;User: Dlindstr     Date: 5/06/97    Time: 8:38a
;Updated in $/SV2-DI/test/scripts
;added valve type and option settings to header
;
;*****************  Version 3  *****************
;User: Dlindstr     Date: 5/05/97    Time: 9:42a
;Updated in $/SV2-DI/test/scripts
;add test case for transition to wait PS close
;
;*****************  Version 2  *****************
;User: Dlindstr     Date: 5/02/97    Time: 12:57p
;Updated in $/SV2-DI/test/scripts
;added history keyword
;
;   Tests:  
;
   G Y F P W L P   WAIT    H L C H M P H I  TIMEOUT COMMENTS  ACTUAL
       L R   I O           U O O E A L S N
       A S   M W           M W O A E T I D
       M W   I E               L T N     C
       E     T R                         R
;                                          
; Wait PS Open (STATE1)   Direct Ignition
;                                                            Check
 0 0 0 0 1 0 1 0 :      0: x x x x x x x 0 :    200;    Lim closed
 0 0 0 0 1 0 1 1 :      0: 0 / 0 0 0 x 0 0 :    300;    Power unit
 0 0 0 0 1 0 1 1 :    200: 0 1 0 0 0 x 0 0 :    300;    Delay
 0 0 0 0 1 1 1 1 :      0: 0 1 0 0 0 x 0 0 :    200;    W request
;
; Limit Open
;
 0 0 0 0 1 1 1 1 :      0: 0 1 0 0 0 x 0 0 :    200;    Apply W , Idle
 0 0 0 0 1 1 1 1 :    800: 0 1 0 0 0 x 0 0 :    900;    Wait PS Open
 0 0 0 0 1 1 0 1 :      0: 0 1 0 0 0 0 0 / :    200;    Limit Open, ind on
 0 0 0 0 1 1 0 1 :      0: / \ 0 / 0 0 0 1 :    300;    Hum and Heat on
 0 0 0 0 1 0 1 1 :    400: 1 0 0 1 0 0 0 \ :    700;    PostPurge
 0 0 0 0 1 0 1 1 :    900: 1 0 0 1 0 0 0 0 :   1000;    Idle
;end
