MCP3424
=======

library for the Arduino.

  The MCP3424 is a low-cost 18Bit Sigma-Delta ADC with I2C Interface.

  This library implements the following features:

   - channel setting by address or pin selection
   - continuous and one_shot modes
   - selectable sample rates 12,14,16 and 18 bit
   - selectable PGA gains: x1, x2, x4, x8
   - conversion errors: overflow, underflow, i2c, progress, timeout
   - selectable blocking/non-blocking modes
   - highest valid gain selection
   - general call requests             


  Author:          Bernhard Schneider <bernhard@neaptide.org><br>
  Available from:  https://github.com/bersch/MCP3424<br>
  License:         GNU LGPL<br>

  
  This library may also be used for MCP3421, MCP3422, MCP3423, MCP3425, MCP3426, MCP3427, MCP3428

  #### See also: 
  
  ADC | Link
  ------------ | -------------
  **MCP3421** | http://ww1.microchip.com/downloads/en/DeviceDoc/22003e.pdf<br>
  **MCP3422/3/4** | http://ww1.microchip.com/downloads/en/DeviceDoc/22088b.pdf<br>
  **MCP3425** | http://ww1.microchip.com/downloads/en/DeviceDoc/22072b.pdf<br>
  **MCP3426/7/8** | http://ww1.microchip.com/downloads/en/DeviceDoc/22226a.pdf<br>
  
