Output: Gerber X2 Files
Type  : GerberX2
From  : Project [LED_driver.PrjPCB]
   Generated File[PCB_with_shield_top_Copper_Signal_Top.gbr]
   Generated File[PCB_with_shield_top_Copper_Plane_1.gbr]
   Generated File[PCB_with_shield_top_Copper_Signal_1.gbr]
   Generated File[PCB_with_shield_top_Copper_Signal_Bot.gbr]
   Generated File[PCB_with_shield_top_Pads_Bot.gbr]
   Generated File[PCB_with_shield_top_Pads_Top.gbr]
   Generated File[PCB_with_shield_top_Paste_Bot.gbr]
   Generated File[PCB_with_shield_top_Legend_Bot.gbr]
   Generated File[PCB_with_shield_top_Soldermask_Bot.gbr]
   Generated File[PCB_with_shield_top_Legend_Top.gbr]
   Generated File[PCB_with_shield_top_Paste_Top.gbr]
   Generated File[PCB_with_shield_top_Soldermask_Top.gbr]
   Generated File[PCB_with_shield_top_Keep-out.gbr]
   Generated File[PCB_with_shield_top_Mechanical_40.gbr]
   Generated File[PCB_with_shield_top_Mechanical_14.gbr]
   Generated File[PCB_with_shield_top_Mechanical_16.gbr]
   Generated File[PCB_with_shield_top_Mechanical_1.gbr]
   Generated File[PCB_with_shield_top_Placement.gbr]
   Generated File[PCB_with_shield_top_Assembly.gbr]
   Generated File[PCB_with_shield_top_Mechanical_11.gbr]
   Generated File[PCB_with_shield_top_Board_outline.gbr]
   Generated File[PCB_with_shield_top_Mechanical_42.gbr]
   Generated File[PCB_with_shield_top_Mechanical_26.gbr]
   Generated File[PCB_with_shield_top_Mechanical_25.gbr]
   Generated File[PCB_with_shield_top_Profile.gbr]
   Generated File[PCB_with_shield_top.RUL]
   Generated File[PCB_with_shield_top.EXTREP]
   Generated File[PCB_with_shield_top.REP]


Files Generated   : 28
Documents Printed : 0

Finished Output Generation At 12:35:01 On 12.04.2022
