# Static Call Graph for image .\Objects\timer.axf

#<CALLGRAPH># ARM Linker, 5060061: Last Updated: Sun May 22 11:45:08 2016

### Maximum Stack Usage = 8 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_sh ⇒ __user_setup_stackheap

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC0_Int_Handler ⇒ ADC0_Int_Handler

  ### Function Pointers

  - ADC0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - ADC1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - BusFault_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_ADC0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_ADC1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_DAC_Out_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_Err_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_I2C0_MRX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_I2C0_MTX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_I2C0_SRX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_I2C0_STX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_SINC2_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_SPI1_RX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_SPI1_TX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_UART_RX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_UART_TX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DebugMon_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int0_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int1_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int2_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int3_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int4_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int5_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int6_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int7_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Flsh_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - GP_Tmr0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - GP_Tmr1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - HardFault_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - I2C0_Master_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - I2C0_Slave_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - MemManage_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - NMI_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PWM0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PWM1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PWM2_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PWMTRIP_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PendSV_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Reset_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SINC2_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SPI0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SPI1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SVC_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SysTick_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SystemInit from system_aducm360.o(i.SystemInit) referenced from startup_aducm360.o(.text)
  - UART_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - UsageFault_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - WDog_Tmr_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - WakeUp_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_aducm360.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ exit
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_aducm360.o(.text))

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  ADC0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> ADC0_Int_Handler
  [Called By]
  - >> ADC0_Int_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  ADC1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_ADC0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_ADC1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_DAC_Out_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_Err_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_I2C0_MRX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_I2C0_MTX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_I2C0_SRX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_I2C0_STX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_SINC2_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_SPI1_RX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_SPI1_TX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_UART_RX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_UART_TX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int0_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int1_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int2_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int3_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int4_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int5_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int6_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int7_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Flsh_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  GP_Tmr0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  GP_Tmr1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  I2C0_Master_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  I2C0_Slave_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  PWM0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  PWM1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  PWM2_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  PWMTRIP_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  SINC2_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  SPI0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  SPI1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  UART_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  WDog_Tmr_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  WakeUp_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_aducm360.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  SystemInit (Thumb, 22 bytes, Stack size 0 bytes, system_aducm360.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_aducm360.o(.text)

  delay(long) (Thumb, 10 bytes, Stack size 0 bytes, timer.o(i._Z5delayl))
  [Called By]

  - >> main

  main (Thumb, 106 bytes, Stack size 0 bytes, timer.o(i.main))
  [Calls]

  - >> delay(long)
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  ### Undefined Global Symbols