# Static Call Graph for image .\Objects\pwrmng1.axf

#<CALLGRAPH># ARM Linker, 5060061: Last Updated: Mon May 23 14:57:10 2016

### Maximum Stack Usage = 80 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

svcKernelInitialize ⇒ svcThreadCreate ⇒ rt_tsk_create ⇒ rt_init_context ⇒ rt_init_stack

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- rt_alloc_box ⇒ rt_alloc_box
- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- ADC0_Int_Handler ⇒ ADC0_Int_Handler

  ### Function Pointers

  - ADC0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - ADC1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - BusFault_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_ADC0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_ADC1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_DAC_Out_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_Err_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_I2C0_MRX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_I2C0_MTX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_I2C0_SRX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_I2C0_STX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_SINC2_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_SPI1_RX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_SPI1_TX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_UART_RX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DMA_UART_TX_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - DebugMon_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int0_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int1_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int2_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int3_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int4_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int5_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int6_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Ext_Int7_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - Flsh_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - GP_Tmr0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - GP_Tmr1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - HardFault_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - I2C0_Master_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - I2C0_Slave_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - MemManage_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - NMI_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PWM0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PWM1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PWM2_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PWMTRIP_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - PendSV_Handler from hal_cm3.o(.emb_text) referenced from startup_aducm360.o(RESET)
  - Reset_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SINC2_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SPI0_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SPI1_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - SVC_Handler from hal_cm3.o(.emb_text) referenced from startup_aducm360.o(RESET)
  - SysTick_Handler from hal_cm3.o(.emb_text) referenced from startup_aducm360.o(RESET)
  - SystemInit from system_aducm360.o(i.SystemInit) referenced from startup_aducm360.o(.text)
  - UART_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - UsageFault_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - WDog_Tmr_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - WakeUp_Int_Handler from startup_aducm360.o(.text) referenced from startup_aducm360.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_aducm360.o(.text)
  - main from pwrmng2.o(i.main) referenced from rtx_conf_cm.o(.data)
  - osThreadExit from rt_cmsis.o(i.osThreadExit) referenced from rt_cmsis.o(i.svcThreadCreate)
  - osTimerThread from rt_cmsis.o(i.osTimerThread) referenced from rtx_conf_cm.o(.constdata)
  - os_idle_demon from rtx_conf_cm.o(i.os_idle_demon) referenced from rt_task.o(i.rt_sys_init)
  - rt_alloc_box from rt_membox.o(i.rt_alloc_box) referenced from hal_cm3.o(.emb_text)
  - rt_free_box from rt_membox.o(i.rt_free_box) referenced from hal_cm3.o(.emb_text)
  - rt_mut_release from rt_mutex.o(i.rt_mut_release) referenced from rtx_conf_cm.o(i._mutex_release)
  - rt_mut_wait from rt_mutex.o(i.rt_mut_wait) referenced from rtx_conf_cm.o(i._mutex_acquire)
  - svcKernelInitialize from rt_cmsis.o(i.svcKernelInitialize) referenced from rt_cmsis.o(i.osKernelInitialize)
  - svcKernelStart from rt_cmsis.o(i.svcKernelStart) referenced from rt_cmsis.o(i.osKernelStart)
  - svcMessageGet from rt_cmsis.o(i.svcMessageGet) referenced from rt_cmsis.o(i.osMessageGet)
  - svcThreadCreate from rt_cmsis.o(i.svcThreadCreate) referenced from rt_cmsis.o(i.osThreadCreate)
  - svcThreadGetId from rt_cmsis.o(i.svcThreadGetId) referenced from rt_cmsis.o(i.osThreadExit)
  - svcThreadTerminate from rt_cmsis.o(i.svcThreadTerminate) referenced from rt_cmsis.o(i.osThreadExit)
  - svcTimerCall from rt_cmsis.o(i.svcTimerCall) referenced from rt_cmsis.o(i.osTimerCall)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000007))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000010))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000A))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000B))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = __rt_entry_postli_1 ⇒ _platform_post_lib_init ⇒ osKernelInitialize ⇒ svcKernelInitialize ⇒ svcThreadCreate ⇒ rt_tsk_create ⇒ rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> _platform_post_lib_init

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ exit
  [Calls]
  - >> main
  - >> exit

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  _platform_post_lib_init (Thumb, 24 bytes, Stack size 0 bytes, rtx_conf_cm.o(.emb_text))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = _platform_post_lib_init ⇒ osKernelInitialize ⇒ svcKernelInitialize ⇒ svcThreadCreate ⇒ rt_tsk_create ⇒ rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> osThreadCreate
  - >> osKernelStart
  - >> osKernelInitialize
  - >> exit
  [Called By]
  - >> __rt_entry_postli_1

  rt_set_PSP (Thumb, 6 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)

  rt_get_PSP (Thumb, 6 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Called By]

  - >> rt_tsk_delete

  os_set_env (Thumb, 24 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)

  _alloc_box (Thumb, 28 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)

  _free_box (Thumb, 28 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)

  SVC_Handler (Thumb, 108 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Calls]

  - >> rt_stk_check
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  PendSV_Handler (Thumb, 56 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Stack]

  - Max Depth = 52
  - Call Chain = PendSV_Handler ⇒ rt_pop_req ⇒ rt_mbx_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_pop_req
  - >> rt_stk_check
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text))
  [Stack]

  - Max Depth = 72
  - Call Chain = SysTick_Handler ⇒ rt_systick ⇒ sysTimerTick ⇒ isrMessagePut ⇒ isr_mbx_send ⇒ rt_psq_enq
  [Calls]
  - >> rt_systick
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  OS_Tick_Handler (Thumb, 12 bytes, Stack size 0 bytes, hal_cm3.o(.emb_text), UNUSED)
  [Calls]

  - >> os_tick_irqack
  - >> rt_systick

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_aducm360.o(.text))

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  ADC0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Calls]

  - >> ADC0_Int_Handler
  [Called By]
  - >> ADC0_Int_Handler
  [Address Reference Count : 1]
  - startup_aducm360.o(RESET)

  ADC1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_ADC0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_ADC1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_DAC_Out_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_Err_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_I2C0_MRX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_I2C0_MTX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_I2C0_SRX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_I2C0_STX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_SINC2_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_SPI1_RX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_SPI1_TX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_UART_RX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  DMA_UART_TX_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int0_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int1_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int2_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int3_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int4_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int5_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int6_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Ext_Int7_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  Flsh_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  GP_Tmr0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  GP_Tmr1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  I2C0_Master_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  I2C0_Slave_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  PWM0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  PWM1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  PWM2_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  PWMTRIP_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  SINC2_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  SPI0_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  SPI1_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  UART_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  WDog_Tmr_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  WakeUp_Int_Handler (Thumb, 0 bytes, Stack size 0 bytes, startup_aducm360.o(.text))
  [Address Reference Count : 1]

  - startup_aducm360.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_aducm360.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> _platform_post_lib_init
  - >> __rt_entry_main

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  SystemInit (Thumb, 22 bytes, Stack size 0 bytes, system_aducm360.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_aducm360.o(.text)

  delay(long) (Thumb, 10 bytes, Stack size 0 bytes, pwrmng2.o(i._Z5delayl))
  [Called By]

  - >> main

  _init_box (Thumb, 70 bytes, Stack size 8 bytes, rt_membox.o(i._init_box))
  [Stack]

  - Max Depth = 8
  - Call Chain = _init_box
  [Called By]
  - >> rt_sys_init

  _mutex_acquire (Thumb, 22 bytes, Stack size 0 bytes, rtx_conf_cm.o(i._mutex_acquire), UNUSED, KEPT)

  _mutex_release (Thumb, 18 bytes, Stack size 0 bytes, rtx_conf_cm.o(i._mutex_release), UNUSED, KEPT)

  dbg_init (Thumb, 34 bytes, Stack size 0 bytes, hal_cm.o(i.dbg_init))
  [Called By]

  - >> rt_sys_init

  dbg_task_notify (Thumb, 32 bytes, Stack size 0 bytes, hal_cm.o(i.dbg_task_notify))
  [Called By]

  - >> rt_tsk_delete
  - >> rt_tsk_create

  dbg_task_switch (Thumb, 16 bytes, Stack size 0 bytes, hal_cm.o(i.dbg_task_switch))
  [Called By]

  - >> rt_switch_req

  isrMessageGet (Thumb, 42 bytes, Stack size 16 bytes, rt_cmsis.o(i.isrMessageGet))
  [Stack]

  - Max Depth = 40
  - Call Chain = isrMessageGet ⇒ isr_mbx_receive ⇒ rt_psq_enq
  [Calls]
  - >> isr_mbx_receive
  [Called By]
  - >> osMessageGet

  isrMessagePut (Thumb, 44 bytes, Stack size 16 bytes, rt_cmsis.o(i.isrMessagePut))
  [Stack]

  - Max Depth = 40
  - Call Chain = isrMessagePut ⇒ isr_mbx_send ⇒ rt_psq_enq
  [Calls]
  - >> rt_mbx_check
  - >> isr_mbx_send
  [Called By]
  - >> sysTimerTick

  isr_mbx_receive (Thumb, 82 bytes, Stack size 8 bytes, rt_mailbox.o(i.isr_mbx_receive))
  [Stack]

  - Max Depth = 24
  - Call Chain = isr_mbx_receive ⇒ rt_psq_enq
  [Calls]
  - >> rt_psq_enq
  - >> rt_psh_req
  [Called By]
  - >> isrMessageGet

  isr_mbx_send (Thumb, 14 bytes, Stack size 8 bytes, rt_mailbox.o(i.isr_mbx_send))
  [Stack]

  - Max Depth = 24
  - Call Chain = isr_mbx_send ⇒ rt_psq_enq
  [Calls]
  - >> rt_psq_enq
  - >> rt_psh_req
  [Called By]
  - >> isrMessagePut

  main (Thumb, 74 bytes, Stack size 0 bytes, pwrmng2.o(i.main))
  [Calls]

  - >> delay(long)
  [Called By]
  - >> __rt_entry_main
  [Address Reference Count : 1]
  - rtx_conf_cm.o(.data)

  osKernelInitialize (Thumb, 30 bytes, Stack size 0 bytes, rt_cmsis.o(i.osKernelInitialize))
  [Stack]

  - Max Depth = 80
  - Call Chain = osKernelInitialize ⇒ svcKernelInitialize ⇒ svcThreadCreate ⇒ rt_tsk_create ⇒ rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> svcKernelInitialize
  [Called By]
  - >> _platform_post_lib_init

  osKernelStart (Thumb, 98 bytes, Stack size 32 bytes, rt_cmsis.o(i.osKernelStart))
  [Stack]

  - Max Depth = 32
  - Call Chain = osKernelStart
  [Called By]
  - >> _platform_post_lib_init

  osMessageGet (Thumb, 18 bytes, Stack size 0 bytes, rt_cmsis.o(i.osMessageGet))
  [Stack]

  - Max Depth = 40
  - Call Chain = osMessageGet ⇒ isrMessageGet ⇒ isr_mbx_receive ⇒ rt_psq_enq
  [Calls]
  - >> isrMessageGet
  [Called By]
  - >> osTimerThread

  osThreadCreate (Thumb, 38 bytes, Stack size 0 bytes, rt_cmsis.o(i.osThreadCreate))
  [Stack]

  - Max Depth = 72
  - Call Chain = osThreadCreate ⇒ svcThreadCreate ⇒ rt_tsk_create ⇒ rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> svcThreadCreate
  [Called By]
  - >> _platform_post_lib_init

  osThreadExit (Thumb, 14 bytes, Stack size 0 bytes, rt_cmsis.o(i.osThreadExit))
  [Address Reference Count : 1]

  - rt_cmsis.o(i.svcThreadCreate)

  osTimerCall (Thumb, 8 bytes, Stack size 0 bytes, rt_cmsis.o(i.osTimerCall))
  [Called By]

  - >> osTimerThread

  osTimerThread (Thumb, 38 bytes, Stack size 0 bytes, rt_cmsis.o(i.osTimerThread))
  [Stack]

  - Max Depth = 40
  - Call Chain = osTimerThread ⇒ osMessageGet ⇒ isrMessageGet ⇒ isr_mbx_receive ⇒ rt_psq_enq
  [Calls]
  - >> osTimerCall
  - >> osMessageGet
  [Address Reference Count : 1]
  - rtx_conf_cm.o(.constdata)

  os_error (Thumb, 34 bytes, Stack size 0 bytes, rtx_conf_cm.o(i.os_error))
  [Called By]

  - >> rt_mbx_psh
  - >> rt_stk_check
  - >> rt_psq_enq
  - >> sysTimerTick

  os_idle_demon (Thumb, 4 bytes, Stack size 0 bytes, rtx_conf_cm.o(i.os_idle_demon))
  [Address Reference Count : 1]

  - rt_task.o(i.rt_sys_init)

  os_tick_init (Thumb, 32 bytes, Stack size 0 bytes, rt_system.o(i.os_tick_init))
  [Called By]

  - >> rt_sys_start

  os_tick_irqack (Thumb, 2 bytes, Stack size 0 bytes, rt_system.o(i.os_tick_irqack), UNUSED)
  [Called By]

  - >> OS_Tick_Handler

  rt_alloc_box (Thumb, 26 bytes, Stack size 0 bytes, rt_membox.o(i.rt_alloc_box))
  [Calls]

  - >> rt_alloc_box
  [Called By]
  - >> rt_mbx_psh
  - >> rt_init_context
  - >> rt_tsk_create
  - >> rt_alloc_box
  [Address Reference Count : 1]
  - hal_cm3.o(.emb_text)

  rt_alloc_mem (Thumb, 62 bytes, Stack size 8 bytes, rt_memory.o(i.rt_alloc_mem))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_alloc_mem
  [Called By]
  - >> svcThreadCreate

  rt_block (Thumb, 48 bytes, Stack size 16 bytes, rt_task.o(i.rt_block))
  [Stack]

  - Max Depth = 24
  - Call Chain = rt_block ⇒ rt_put_dly
  [Calls]
  - >> rt_put_dly
  - >> rt_switch_req
  - >> rt_get_first
  [Called By]
  - >> rt_mut_wait
  - >> rt_mbx_wait

  rt_chk_robin (Thumb, 60 bytes, Stack size 8 bytes, rt_robin.o(i.rt_chk_robin))
  [Stack]

  - Max Depth = 20
  - Call Chain = rt_chk_robin ⇒ rt_put_prio
  [Calls]
  - >> rt_put_prio
  - >> rt_get_first
  [Called By]
  - >> rt_systick

  rt_dec_dly (Thumb, 102 bytes, Stack size 16 bytes, rt_list.o(i.rt_dec_dly))
  [Stack]

  - Max Depth = 28
  - Call Chain = rt_dec_dly ⇒ rt_put_prio
  [Calls]
  - >> rt_put_prio
  [Called By]
  - >> rt_systick

  rt_dispatch (Thumb, 60 bytes, Stack size 16 bytes, rt_task.o(i.rt_dispatch))
  [Stack]

  - Max Depth = 28
  - Call Chain = rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_put_rdy_first
  - >> rt_switch_req
  - >> rt_put_prio
  - >> rt_get_first
  [Called By]
  - >> rt_mut_release
  - >> rt_tsk_prio
  - >> rt_tsk_delete
  - >> rt_tsk_create
  - >> rt_mbx_wait

  rt_evt_psh (Thumb, 76 bytes, Stack size 8 bytes, rt_event.o(i.rt_evt_psh))
  [Stack]

  - Max Depth = 20
  - Call Chain = rt_evt_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_ret_val2
  - >> rt_rmv_dly
  - >> rt_put_prio
  [Called By]
  - >> rt_pop_req

  rt_free_box (Thumb, 44 bytes, Stack size 0 bytes, rt_membox.o(i.rt_free_box))
  [Called By]

  - >> rt_tsk_delete
  [Address Reference Count : 1]
  - hal_cm3.o(.emb_text)

  rt_free_mem (Thumb, 40 bytes, Stack size 0 bytes, rt_memory.o(i.rt_free_mem))
  [Called By]

  - >> svcThreadTerminate
  - >> svcThreadCreate

  rt_get_first (Thumb, 40 bytes, Stack size 0 bytes, rt_list.o(i.rt_get_first))
  [Called By]

  - >> rt_mut_release
  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_chk_robin
  - >> rt_systick
  - >> rt_pop_req
  - >> rt_tsk_prio
  - >> rt_tsk_delete
  - >> rt_mbx_wait
  - >> rt_dispatch
  - >> rt_block

  rt_init_mem (Thumb, 26 bytes, Stack size 0 bytes, rt_memory.o(i.rt_init_mem))
  [Called By]

  - >> svcKernelInitialize

  rt_init_robin (Thumb, 14 bytes, Stack size 0 bytes, rt_robin.o(i.rt_init_robin))
  [Called By]

  - >> rt_sys_init

  rt_init_stack (Thumb, 118 bytes, Stack size 16 bytes, hal_cm.o(i.rt_init_stack))
  [Stack]

  - Max Depth = 16
  - Call Chain = rt_init_stack
  [Called By]
  - >> rt_init_context

  rt_mbx_check (Thumb, 8 bytes, Stack size 0 bytes, rt_mailbox.o(i.rt_mbx_check))
  [Called By]

  - >> isrMessagePut

  rt_mbx_init (Thumb, 26 bytes, Stack size 0 bytes, rt_mailbox.o(i.rt_mbx_init))
  [Called By]

  - >> svcMessageCreate

  rt_mbx_psh (Thumb, 236 bytes, Stack size 24 bytes, rt_mailbox.o(i.rt_mbx_psh))
  [Stack]

  - Max Depth = 36
  - Call Chain = rt_mbx_psh ⇒ rt_put_prio
  [Calls]
  - >> os_error
  - >> rt_ret_val2
  - >> rt_rmv_dly
  - >> rt_ret_val
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_alloc_box
  [Called By]
  - >> rt_pop_req

  rt_mbx_wait (Thumb, 174 bytes, Stack size 16 bytes, rt_mailbox.o(i.rt_mbx_wait))
  [Stack]

  - Max Depth = 44
  - Call Chain = rt_mbx_wait ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_ret_val
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_dispatch
  - >> rt_block
  [Called By]
  - >> svcMessageGet

  rt_mut_release (Thumb, 208 bytes, Stack size 24 bytes, rt_mutex.o(i.rt_mut_release))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_mut_release ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_ret_val
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_dispatch
  [Address Reference Count : 1]
  - rtx_conf_cm.o(i._mutex_release)

  rt_mut_wait (Thumb, 100 bytes, Stack size 16 bytes, rt_mutex.o(i.rt_mut_wait))
  [Stack]

  - Max Depth = 40
  - Call Chain = rt_mut_wait ⇒ rt_block ⇒ rt_put_dly
  [Calls]
  - >> rt_resort_prio
  - >> rt_put_prio
  - >> rt_block
  [Address Reference Count : 1]
  - rtx_conf_cm.o(i._mutex_acquire)

  rt_pop_req (Thumb, 112 bytes, Stack size 16 bytes, rt_system.o(i.rt_pop_req))
  [Stack]

  - Max Depth = 52
  - Call Chain = rt_pop_req ⇒ rt_mbx_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_put_rdy_first
  - >> rt_switch_req
  - >> rt_get_first
  [Called By]
  - >> PendSV_Handler

  rt_psh_req (Thumb, 22 bytes, Stack size 0 bytes, rt_system.o(i.rt_psh_req))
  [Called By]

  - >> isr_mbx_send
  - >> isr_mbx_receive

  rt_psq_enq (Thumb, 88 bytes, Stack size 16 bytes, rt_list.o(i.rt_psq_enq))
  [Stack]

  - Max Depth = 16
  - Call Chain = rt_psq_enq
  [Calls]
  - >> os_error
  [Called By]
  - >> isr_mbx_send
  - >> isr_mbx_receive

  rt_put_dly (Thumb, 68 bytes, Stack size 8 bytes, rt_list.o(i.rt_put_dly))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_put_dly
  [Called By]
  - >> rt_block

  rt_put_prio (Thumb, 54 bytes, Stack size 12 bytes, rt_list.o(i.rt_put_prio))
  [Stack]

  - Max Depth = 12
  - Call Chain = rt_put_prio
  [Called By]
  - >> rt_mut_wait
  - >> rt_mut_release
  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_dec_dly
  - >> rt_chk_robin
  - >> rt_resort_prio
  - >> rt_tsk_prio
  - >> rt_tsk_delete
  - >> rt_mbx_wait
  - >> rt_dispatch

  rt_put_rdy_first (Thumb, 14 bytes, Stack size 0 bytes, rt_list.o(i.rt_put_rdy_first))
  [Called By]

  - >> rt_systick
  - >> rt_pop_req
  - >> rt_dispatch

  rt_resort_prio (Thumb, 46 bytes, Stack size 8 bytes, rt_list.o(i.rt_resort_prio))
  [Stack]

  - Max Depth = 20
  - Call Chain = rt_resort_prio ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_list
  - >> rt_put_prio
  [Called By]
  - >> rt_mut_wait
  - >> rt_tsk_prio

  rt_ret_val (Thumb, 6 bytes, Stack size 0 bytes, hal_cm.o(i.rt_ret_val))
  [Called By]

  - >> rt_mut_release
  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_tsk_delete
  - >> rt_mbx_wait

  rt_ret_val2 (Thumb, 8 bytes, Stack size 0 bytes, hal_cm.o(i.rt_ret_val2))
  [Called By]

  - >> rt_mbx_psh
  - >> rt_evt_psh

  rt_rmv_dly (Thumb, 40 bytes, Stack size 8 bytes, rt_list.o(i.rt_rmv_dly))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_rmv_dly
  [Called By]
  - >> rt_mut_release
  - >> rt_sem_psh
  - >> rt_mbx_psh
  - >> rt_evt_psh
  - >> rt_tsk_delete
  - >> rt_mbx_wait

  rt_rmv_list (Thumb, 44 bytes, Stack size 0 bytes, rt_list.o(i.rt_rmv_list))
  [Called By]

  - >> rt_resort_prio
  - >> rt_tsk_delete

  rt_sem_psh (Thumb, 48 bytes, Stack size 8 bytes, rt_semaphore.o(i.rt_sem_psh))
  [Stack]

  - Max Depth = 20
  - Call Chain = rt_sem_psh ⇒ rt_put_prio
  [Calls]
  - >> rt_rmv_dly
  - >> rt_ret_val
  - >> rt_put_prio
  - >> rt_get_first
  [Called By]
  - >> rt_pop_req

  rt_stk_check (Thumb, 28 bytes, Stack size 0 bytes, rt_system.o(i.rt_stk_check))
  [Calls]

  - >> os_error
  [Called By]
  - >> PendSV_Handler
  - >> SVC_Handler
  - >> rt_tsk_delete

  rt_switch_req (Thumb, 30 bytes, Stack size 0 bytes, rt_task.o(i.rt_switch_req))
  [Calls]

  - >> dbg_task_switch
  [Called By]
  - >> rt_systick
  - >> rt_pop_req
  - >> rt_dispatch
  - >> rt_block

  rt_sys_init (Thumb, 138 bytes, Stack size 16 bytes, rt_task.o(i.rt_sys_init))
  [Stack]

  - Max Depth = 48
  - Call Chain = rt_sys_init ⇒ rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> rt_init_robin
  - >> dbg_init
  - >> rt_init_context
  - >> _init_box
  [Called By]
  - >> svcKernelInitialize

  rt_sys_start (Thumb, 110 bytes, Stack size 8 bytes, rt_task.o(i.rt_sys_start))
  [Stack]

  - Max Depth = 8
  - Call Chain = rt_sys_start
  [Calls]
  - >> os_tick_init
  [Called By]
  - >> svcKernelStart

  rt_systick (Thumb, 50 bytes, Stack size 8 bytes, rt_system.o(i.rt_systick))
  [Stack]

  - Max Depth = 72
  - Call Chain = rt_systick ⇒ sysTimerTick ⇒ isrMessagePut ⇒ isr_mbx_send ⇒ rt_psq_enq
  [Calls]
  - >> rt_dec_dly
  - >> rt_chk_robin
  - >> rt_put_rdy_first
  - >> rt_switch_req
  - >> rt_get_first
  - >> sysTimerTick
  [Called By]
  - >> OS_Tick_Handler
  - >> SysTick_Handler

  rt_tsk_create (Thumb, 118 bytes, Stack size 24 bytes, rt_task.o(i.rt_tsk_create))
  [Stack]

  - Max Depth = 56
  - Call Chain = rt_tsk_create ⇒ rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> dbg_task_notify
  - >> rt_init_context
  - >> rt_dispatch
  - >> rt_alloc_box
  [Called By]
  - >> svcThreadCreate

  rt_tsk_delete (Thumb, 352 bytes, Stack size 40 bytes, rt_task.o(i.rt_tsk_delete))
  [Stack]

  - Max Depth = 68
  - Call Chain = rt_tsk_delete ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_stk_check
  - >> rt_rmv_list
  - >> rt_get_PSP
  - >> dbg_task_notify
  - >> rt_rmv_dly
  - >> rt_ret_val
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_free_box
  - >> rt_dispatch
  [Called By]
  - >> svcThreadTerminate

  rt_tsk_prio (Thumb, 108 bytes, Stack size 16 bytes, rt_task.o(i.rt_tsk_prio))
  [Stack]

  - Max Depth = 44
  - Call Chain = rt_tsk_prio ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_resort_prio
  - >> rt_put_prio
  - >> rt_get_first
  - >> rt_dispatch
  [Called By]
  - >> svcKernelStart

  rt_tsk_self (Thumb, 12 bytes, Stack size 0 bytes, rt_task.o(i.rt_tsk_self))
  [Called By]

  - >> svcThreadGetId

  svcKernelInitialize (Thumb, 80 bytes, Stack size 8 bytes, rt_cmsis.o(i.svcKernelInitialize))
  [Stack]

  - Max Depth = 80
  - Call Chain = svcKernelInitialize ⇒ svcThreadCreate ⇒ rt_tsk_create ⇒ rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> rt_sys_init
  - >> rt_init_mem
  - >> svcThreadCreate
  - >> svcMessageCreate
  [Called By]
  - >> osKernelInitialize
  [Address Reference Count : 1]
  - rt_cmsis.o(i.osKernelInitialize)

  svcKernelStart (Thumb, 62 bytes, Stack size 16 bytes, rt_cmsis.o(i.svcKernelStart))
  [Stack]

  - Max Depth = 60
  - Call Chain = svcKernelStart ⇒ rt_tsk_prio ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_tsk_prio
  - >> rt_sys_start
  [Address Reference Count : 1]
  - rt_cmsis.o(i.osKernelStart)

  svcMessageCreate (Thumb, 36 bytes, Stack size 8 bytes, rt_cmsis.o(i.svcMessageCreate))
  [Stack]

  - Max Depth = 8
  - Call Chain = svcMessageCreate
  [Calls]
  - >> rt_mbx_init
  [Called By]
  - >> svcKernelInitialize

  svcMessageGet (Thumb, 58 bytes, Stack size 24 bytes, rt_cmsis.o(i.svcMessageGet))
  [Stack]

  - Max Depth = 68
  - Call Chain = svcMessageGet ⇒ rt_mbx_wait ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_ms2tick
  - >> rt_mbx_wait
  [Address Reference Count : 1]
  - rt_cmsis.o(i.osMessageGet)

  svcThreadCreate (Thumb, 100 bytes, Stack size 16 bytes, rt_cmsis.o(i.svcThreadCreate))
  [Stack]

  - Max Depth = 72
  - Call Chain = svcThreadCreate ⇒ rt_tsk_create ⇒ rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> rt_tsk_create
  - >> rt_free_mem
  - >> rt_alloc_mem
  [Called By]
  - >> osThreadCreate
  - >> svcKernelInitialize
  [Address Reference Count : 1]
  - rt_cmsis.o(i.osThreadCreate)

  svcThreadGetId (Thumb, 22 bytes, Stack size 8 bytes, rt_cmsis.o(i.svcThreadGetId))
  [Stack]

  - Max Depth = 8
  - Call Chain = svcThreadGetId
  [Calls]
  - >> rt_tsk_self
  [Address Reference Count : 1]
  - rt_cmsis.o(i.osThreadExit)

  svcThreadTerminate (Thumb, 50 bytes, Stack size 8 bytes, rt_cmsis.o(i.svcThreadTerminate))
  [Stack]

  - Max Depth = 76
  - Call Chain = svcThreadTerminate ⇒ rt_tsk_delete ⇒ rt_dispatch ⇒ rt_put_prio
  [Calls]
  - >> rt_tid2ptcb
  - >> rt_tsk_delete
  - >> rt_free_mem
  [Address Reference Count : 1]
  - rt_cmsis.o(i.osThreadExit)

  svcTimerCall (Thumb, 24 bytes, Stack size 8 bytes, rt_cmsis.o(i.svcTimerCall))
  [Stack]

  - Max Depth = 8
  - Call Chain = svcTimerCall
  [Calls]
  - >> rt_id2obj
  [Address Reference Count : 1]
  - rt_cmsis.o(i.osTimerCall)

  sysTimerTick (Thumb, 84 bytes, Stack size 24 bytes, rt_cmsis.o(i.sysTimerTick))
  [Stack]

  - Max Depth = 64
  - Call Chain = sysTimerTick ⇒ isrMessagePut ⇒ isr_mbx_send ⇒ rt_psq_enq
  [Calls]
  - >> rt_timer_insert
  - >> os_error
  - >> isrMessagePut
  [Called By]
  - >> rt_systick

  ### Local Symbols

  rt_id2obj (Thumb, 8 bytes, Stack size 0 bytes, rt_cmsis.o(i.rt_id2obj))
  [Called By]

  - >> svcTimerCall

  rt_ms2tick (Thumb, 58 bytes, Stack size 0 bytes, rt_cmsis.o(i.rt_ms2tick))
  [Called By]

  - >> svcMessageGet

  rt_tid2ptcb (Thumb, 18 bytes, Stack size 0 bytes, rt_cmsis.o(i.rt_tid2ptcb))
  [Called By]

  - >> svcThreadTerminate

  rt_timer_insert (Thumb, 48 bytes, Stack size 12 bytes, rt_cmsis.o(i.rt_timer_insert))
  [Stack]

  - Max Depth = 12
  - Call Chain = rt_timer_insert
  [Called By]
  - >> sysTimerTick

  rt_init_context (Thumb, 66 bytes, Stack size 16 bytes, rt_task.o(i.rt_init_context))
  [Stack]

  - Max Depth = 32
  - Call Chain = rt_init_context ⇒ rt_init_stack
  [Calls]
  - >> rt_init_stack
  - >> rt_alloc_box
  [Called By]
  - >> rt_tsk_create
  - >> rt_sys_init

  ### Undefined Global Symbols