------------------------------------------------------------
Server listening on UDP port 5001 with pid 2421
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57830 (sock=3) (peer 2.1.6) on 2022-05-13 13:36:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.15 MBytes  0.966 Mbits/sec   0.053 ms 31/854 (3.6%) 2.160/2.035/4.780/0.225 ms 82 pps 56
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 43340 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.048 ms 0/853 (0%) 1.890/1.781/4.721/0.190 ms 85 pps 66
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42260 (sock=5) (peer 2.1.6) on 2022-05-13 13:37:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.73 MBytes  1.45 Mbits/sec   0.034 ms 42/1279 (3.3%) 2.135/2.007/4.634/0.213 ms 124 pps 85
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 35155 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.034 ms 0/1278 (0%) 1.896/1.789/5.072/0.203 ms 127 pps 99
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36555 (sock=3) (peer 2.1.6) on 2022-05-13 13:37:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.29 MBytes  1.92 Mbits/sec   0.028 ms 70/1704 (4.1%) 1.968/1.821/4.328/0.156 ms 163 pps 122
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 54426 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.052 ms 0/1703 (0%) 1.950/1.820/3.850/0.130 ms 170 pps 128
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51936 (sock=4) (peer 2.1.6) on 2022-05-13 13:37:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.89 MBytes  2.42 Mbits/sec   0.023 ms 70/2129 (3.3%) 1.942/1.766/4.534/0.181 ms 206 pps 156
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 57630 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36891 (sock=3) (peer 2.1.6) on 2022-05-13 13:38:18 (CEST)
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.041 ms 0/2128 (0%) 2.044/1.868/4.504/0.150 ms 212 pps 153
[  9] 0.00-10.00 sec  3.46 MBytes  2.90 Mbits/sec   0.045 ms 86/2554 (3.4%) 2.058/1.908/4.427/0.168 ms 247 pps 176
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[SUM] 0.00-20.28 sec  6.44 MBytes  2.66 Mbits/sec  0/0      227 pps
[SUM-2] Sent 4683 datagrams
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 53284 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.029 ms 0/2553 (0%) 1.936/1.811/5.099/0.166 ms 255 pps 194
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53834 (sock=5) (peer 2.1.6) on 2022-05-13 13:38:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.04 MBytes  3.38 Mbits/sec   0.021 ms 101/2980 (3.4%) 2.085/1.925/4.627/0.179 ms 288 pps 203
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 43961 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.037 ms 0/2979 (0%) 1.986/1.832/6.692/0.185 ms 297 pps 220
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47085 (sock=3) (peer 2.1.6) on 2022-05-13 13:38:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.05 sec  4.61 MBytes  3.84 Mbits/sec   2.748 ms 121/3406 (3.6%) 2.093/1.916/45.859/0.794 ms 327 pps 230
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 45311 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.109 ms 0/3404 (0%) 1.815/1.639/4.740/0.170 ms 340 pps 276
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44108 (sock=4) (peer 2.1.6) on 2022-05-13 13:39:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.28 MBytes  4.43 Mbits/sec   0.020 ms 61/3830 (1.6%) 2.131/1.632/7.500/0.336 ms 377 pps 260
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 55962 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.039 ms 0/3829 (0%) 2.201/1.902/5.566/0.240 ms 382 pps 256
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57677 (sock=3) (peer 2.1.6) on 2022-05-13 13:39:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.77 MBytes  4.84 Mbits/sec   0.053 ms 141/4255 (3.3%) 1.862/1.659/4.680/0.266 ms 411 pps 325
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 59460 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.026 ms 0/4254 (0%) 2.072/1.811/5.416/0.213 ms 425 pps 302
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54089 (sock=4) (peer 2.1.6) on 2022-05-13 13:40:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.38 MBytes  5.35 Mbits/sec   0.056 ms 127/4680 (2.7%) 1.967/1.706/11.908/0.395 ms 455 pps 340
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 54436 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.106 ms 0/4679 (0%) 2.158/1.932/5.086/0.207 ms 467 pps 319
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56224 (sock=3) (peer 2.1.6) on 2022-05-13 13:40:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  6.87 MBytes  5.77 Mbits/sec   0.014 ms 202/5105 (4%) 1.924/1.612/9.211/0.539 ms 490 pps 375
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 32818 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.031 ms 0/5104 (0%) 2.017/1.704/4.752/0.255 ms 510 pps 372
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 32847 (sock=4) (peer 2.1.6) on 2022-05-13 13:40:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  7.40 MBytes  6.21 Mbits/sec   0.021 ms 254/5531 (4.6%) 2.349/1.796/9.012/0.810 ms 528 pps 330
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 35666 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.99 sec  7.75 MBytes  6.51 Mbits/sec   0.017 ms 0/5530 (0%) 1.956/1.676/16.570/0.764 ms 553 pps 416
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55541 (sock=3) (peer 2.1.6) on 2022-05-13 13:41:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.03 sec  7.99 MBytes  6.68 Mbits/sec   0.034 ms 260/5956 (4.4%) 26.520/2.290/39.157/9.327 ms 568 pps 31
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 58796 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.99 sec  8.35 MBytes  7.01 Mbits/sec   0.008 ms 0/5955 (0%) 11.125/5.372/23.632/0.630 ms 596 pps 79
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35160 (sock=4) (peer 2.1.6) on 2022-05-13 13:41:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  8.13 MBytes  6.78 Mbits/sec   0.199 ms 582/6381 (9.1%) 50.326/-1.253/55.709/7.813 ms 577 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 34304 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec   0.041 ms 0/6380 (0%) 1.039/0.564/6.048/0.413 ms 637 pps 903
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46028 (sock=3) (peer 2.1.6) on 2022-05-13 13:41:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.350 ms 1200/6806 (18%) 52.415/2.950/56.199/5.830 ms 558 pps 16
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 57320 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   0.062 ms 0/6805 (0%) 1.765/1.358/6.176/0.611 ms 680 pps 567
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41940 (sock=4) (peer 2.1.6) on 2022-05-13 13:42:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.05 sec  6.82 MBytes  5.69 Mbits/sec   0.495 ms 2368/7231 (33%) 52.863/2.629/67.187/5.324 ms 484 pps 13
[ 31] 0.00-10.05 sec  29 datagrams received out-of-order
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 44273 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.04 sec  9.88 MBytes  8.25 Mbits/sec   0.061 ms 183/7230 (2.5%) 41.479/2.221/46.623/0.375 ms 719 pps 25
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33108 (sock=3) (peer 2.1.6) on 2022-05-13 13:42:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.06 sec  6.57 MBytes  5.48 Mbits/sec   0.549 ms 2972/7656 (39%) 58.275/4.321/63.172/5.448 ms 466 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 54721 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.03 sec  9.87 MBytes  8.26 Mbits/sec   0.212 ms 611/7655 (8%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47466 (sock=4) (peer 2.1.6) on 2022-05-13 13:42:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  6.80 MBytes  5.67 Mbits/sec   0.762 ms 3234/8084 (40%) 72.957/19.506/151.140/7.406 ms 482 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 36915 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  9.90 MBytes  8.26 Mbits/sec   0.295 ms 1022/8081 (13%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44603 (sock=3) (peer 2.1.6) on 2022-05-13 13:43:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.05 sec  7.26 MBytes  6.06 Mbits/sec   0.532 ms 3328/8508 (39%) 75.340/24.438/80.036/3.300 ms 515 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2421 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 59497 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  9.89 MBytes  8.26 Mbits/sec   0.403 ms 1454/8506 (17%) -/-/-/- ms 846 pps
