------------------------------------------------------------
Server listening on UDP port 5001 with pid 1861
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39669 (sock=3) (peer 2.1.6) on 2022-05-13 12:00:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.020 ms 0/854 (0%) -1.536/-1.999/0.579/0.247 ms 85 pps -82
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 35096 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.042 ms 0/853 (0%) 5.078/4.702/7.731/0.321 ms 85 pps 25
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55655 (sock=5) (peer 2.1.6) on 2022-05-13 12:00:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.020 ms 0/1279 (0%) -0.581/-0.794/1.524/0.156 ms 128 pps -323
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 50264 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.026 ms 0/1278 (0%) 4.370/4.061/6.686/0.224 ms 127 pps 43
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57728 (sock=3) (peer 2.1.6) on 2022-05-13 12:00:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.016 ms 0/1704 (0%) -0.081/-0.243/2.414/0.158 ms 170 pps -3089
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 38584 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.025 ms 0/1703 (0%) 3.879/3.640/9.189/0.229 ms 170 pps 64
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36434 (sock=4) (peer 2.1.6) on 2022-05-13 12:01:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.008 ms 0/2129 (0%) 0.356/0.236/2.901/0.136 ms 213 pps 878
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 54846 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.056 ms 0/2128 (0%) 3.510/3.243/6.484/0.192 ms 212 pps 89
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54308 (sock=3) (peer 2.1.6) on 2022-05-13 12:01:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.070 ms 0/2554 (0%) 0.712/0.538/3.230/0.177 ms 255 pps 527
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 33377 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.096 ms 0/2553 (0%) 3.185/2.940/5.853/0.177 ms 255 pps 118
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53029 (sock=4) (peer 2.1.6) on 2022-05-13 12:01:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.084 ms 0/2980 (0%) 1.053/0.959/3.554/0.169 ms 298 pps 416
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 59855 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.033 ms 0/2979 (0%) 2.781/2.591/7.629/0.224 ms 297 pps 157
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44776 (sock=3) (peer 2.1.6) on 2022-05-13 12:02:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.011 ms 0/3405 (0%) 1.323/1.190/4.121/0.218 ms 340 pps 378
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 36904 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.030 ms 0/3404 (0%) 2.594/2.392/5.296/0.161 ms 340 pps 193
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36953 (sock=4) (peer 2.1.6) on 2022-05-13 12:02:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.017 ms 0/3830 (0%) 1.427/1.203/4.298/0.225 ms 383 pps 394
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 45685 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.113 ms 0/3829 (0%) 2.551/2.238/5.077/0.202 ms 382 pps 221
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59522 (sock=3) (peer 2.1.6) on 2022-05-13 12:02:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.020 ms 0/4255 (0%) 1.578/1.381/4.136/0.256 ms 425 pps 396
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 34765 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.020 ms 0/4254 (0%) 2.410/2.153/9.408/0.288 ms 425 pps 259
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40806 (sock=4) (peer 2.1.6) on 2022-05-13 12:03:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.074 ms 0/4680 (0%) 1.689/1.471/5.028/0.322 ms 468 pps 407
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 45052 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.100 ms 0/4679 (0%) 2.324/2.087/5.114/0.209 ms 467 pps 296
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48249 (sock=3) (peer 2.1.6) on 2022-05-13 12:03:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.055 ms 0/5105 (0%) 1.728/1.420/4.693/0.423 ms 510 pps 434
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 48857 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.041 ms 0/5104 (0%) 2.348/2.058/5.917/0.253 ms 510 pps 319
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52697 (sock=4) (peer 2.1.6) on 2022-05-13 12:03:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.028 ms 0/5531 (0%) 1.724/1.296/7.387/0.756 ms 553 pps 472
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 48893 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.030 ms 0/5530 (0%) 2.334/1.976/5.469/0.324 ms 552 pps 348
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36056 (sock=3) (peer 2.1.6) on 2022-05-13 12:04:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.03 sec  8.35 MBytes  6.98 Mbits/sec   0.026 ms 2/5956 (0.034%) 26.939/1.996/40.041/9.629 ms 593 pps 32
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 49983 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.99 sec  8.35 MBytes  7.01 Mbits/sec   0.094 ms 0/5955 (0%) 13.043/7.001/24.135/0.714 ms 596 pps 67
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42478 (sock=4) (peer 2.1.6) on 2022-05-13 12:04:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.04 sec  8.40 MBytes  7.02 Mbits/sec   0.162 ms 388/6381 (6.1%) 41.621/-2.744/48.535/6.701 ms 597 pps 21
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 53945 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-9.99 sec  8.94 MBytes  7.51 Mbits/sec   0.040 ms 0/6380 (0%) 11.404/6.817/20.019/0.252 ms 638 pps 82
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36531 (sock=3) (peer 2.1.6) on 2022-05-13 12:04:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.04 sec  8.44 MBytes  7.05 Mbits/sec   0.311 ms 788/6807 (12%) 42.607/-2.707/48.991/5.101 ms 599 pps 21
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 48243 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-9.99 sec  7.97 MBytes  6.69 Mbits/sec   0.026 ms 1120/6805 (16%) 29.938/7.720/1704.677/0.335 ms 680 pps 28
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52652 (sock=4) (peer 2.1.6) on 2022-05-13 12:05:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.06 sec  8.40 MBytes  7.01 Mbits/sec   0.468 ms 1238/7231 (17%) 50.669/-3.280/55.873/5.818 ms 596 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 40281 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.04 sec  9.89 MBytes  8.26 Mbits/sec   0.099 ms 176/7230 (2.4%) 40.273/0.630/44.594/0.161 ms 720 pps 26
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56578 (sock=3) (peer 2.1.6) on 2022-05-13 12:05:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.06 sec  8.40 MBytes  7.01 Mbits/sec   0.551 ms 1664/7656 (22%) 59.754/6.942/64.252/4.931 ms 596 pps 15
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 49462 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.04 sec  9.87 MBytes  8.25 Mbits/sec   0.242 ms 615/7655 (8%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35150 (sock=4) (peer 2.1.6) on 2022-05-13 12:05:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  8.40 MBytes  7.00 Mbits/sec   0.548 ms 2092/8083 (26%) 72.954/18.445/78.377/4.877 ms 595 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 37908 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  9.89 MBytes  8.26 Mbits/sec   0.329 ms 1028/8081 (13%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58069 (sock=3) (peer 2.1.6) on 2022-05-13 12:06:16 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.05 sec  8.40 MBytes  7.02 Mbits/sec   0.562 ms 2514/8507 (30%) 79.204/32.088/83.327/3.871 ms 597 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1861 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 39246 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  9.90 MBytes  8.27 Mbits/sec   0.396 ms 1441/8506 (17%) -/-/-/- ms 846 pps
