------------------------------------------------------------
Server listening on UDP port 5001 with pid 2352
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58394 (sock=3) (peer 2.1.6) on 2022-05-13 13:23:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.18 MBytes  0.988 Mbits/sec   0.029 ms 12/854 (1.4%) 2.478/2.313/4.840/0.193 ms 84 pps 50
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 56520 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.032 ms 0/853 (0%) 1.909/1.756/4.868/0.228 ms 85 pps 66
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59006 (sock=5) (peer 2.1.6) on 2022-05-13 13:23:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.73 MBytes  1.45 Mbits/sec   0.011 ms 46/1279 (3.6%) 2.712/2.624/5.409/0.192 ms 123 pps 67
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 55682 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.038 ms 0/1278 (0%) 1.827/1.690/5.049/0.173 ms 127 pps 103
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44437 (sock=3) (peer 2.1.6) on 2022-05-13 13:24:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.37 MBytes  1.99 Mbits/sec   0.023 ms 13/1704 (0.76%) 2.540/2.269/5.711/0.235 ms 169 pps 98
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 53118 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.022 ms 0/1703 (0%) 2.115/1.871/5.059/0.179 ms 170 pps 118
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35895 (sock=4) (peer 2.1.6) on 2022-05-13 13:24:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.94 MBytes  2.46 Mbits/sec   0.011 ms 32/2129 (1.5%) 2.402/2.016/5.088/0.254 ms 210 pps 128
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 57817 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.104 ms 0/2128 (0%) 2.287/2.019/6.705/0.263 ms 212 pps 137
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43657 (sock=3) (peer 2.1.6) on 2022-05-13 13:24:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.48 MBytes  2.92 Mbits/sec   0.034 ms 69/2554 (2.7%) 1.689/1.010/6.556/0.469 ms 248 pps 216
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 50421 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.099 ms 0/2553 (0%) 3.159/2.848/6.541/0.257 ms 255 pps 119
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42579 (sock=4) (peer 2.1.6) on 2022-05-13 13:25:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  4.09 MBytes  3.43 Mbits/sec   0.011 ms 60/2980 (2%) 0.933/-0.021/6.657/0.612 ms 292 pps 460
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 43801 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.041 ms 0/2979 (0%) 4.287/3.926/6.603/0.232 ms 297 pps 102
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41357 (sock=3) (peer 2.1.6) on 2022-05-13 13:25:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.69 MBytes  3.93 Mbits/sec   0.078 ms 58/3405 (1.7%) 0.066/-0.463/6.151/0.589 ms 335 pps 7476
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 46624 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.047 ms 0/3404 (0%) 4.063/3.579/8.759/0.361 ms 340 pps 123
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37108 (sock=4) (peer 2.1.6) on 2022-05-13 13:26:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.34 MBytes  4.48 Mbits/sec   0.020 ms 18/3830 (0.47%) 0.786/0.415/7.021/0.681 ms 381 pps 713
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 53553 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.032 ms 0/3829 (0%) 3.259/2.740/6.187/0.298 ms 382 pps 173
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37453 (sock=3) (peer 2.1.6) on 2022-05-13 13:26:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.88 MBytes  4.93 Mbits/sec   0.015 ms 59/4255 (1.4%) 1.294/0.650/7.654/0.884 ms 420 pps 477
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 58968 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.028 ms 0/4254 (0%) 3.256/2.865/6.442/0.284 ms 425 pps 192
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37812 (sock=4) (peer 2.1.6) on 2022-05-13 13:26:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.021 ms 0/4680 (0%) 1.205/0.608/7.871/1.231 ms 468 pps 571
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 58408 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.268 ms 0/4679 (0%) 3.054/2.080/6.805/0.553 ms 467 pps 225
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59513 (sock=3) (peer 2.1.6) on 2022-05-13 13:27:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.15 MBytes  6.00 Mbits/sec   0.054 ms 4/5105 (0.078%) 5.671/1.090/11.506/2.252 ms 510 pps 132
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 55708 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.248 ms 0/5104 (0%) 3.005/2.584/6.268/0.367 ms 510 pps 250
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44603 (sock=4) (peer 2.1.6) on 2022-05-13 13:27:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.06 sec  7.14 MBytes  5.96 Mbits/sec   0.280 ms 435/5531 (7.9%) 59.336/1.862/63.328/9.302 ms 506 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 40659 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.025 ms 0/5530 (0%) 1.612/1.003/6.591/0.543 ms 553 pps 504
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42418 (sock=3) (peer 2.1.6) on 2022-05-13 13:27:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.06 sec  7.19 MBytes  5.99 Mbits/sec   0.414 ms 828/5956 (14%) 61.349/3.047/66.627/6.835 ms 510 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 36972 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  6.90 MBytes  5.79 Mbits/sec   0.128 ms 1034/5955 (17%) -/-/-/- ms 595 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59236 (sock=4) (peer 2.1.6) on 2022-05-13 13:28:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  7.16 MBytes  5.97 Mbits/sec   0.539 ms 1275/6381 (20%) 61.889/4.121/67.680/5.470 ms 508 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 43815 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  8.75 MBytes  7.30 Mbits/sec   0.136 ms 142/6380 (2.2%) 46.418/4.929/51.882/0.443 ms 635 pps 20
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42552 (sock=3) (peer 2.1.6) on 2022-05-13 13:28:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.04 sec  7.28 MBytes  6.08 Mbits/sec   0.609 ms 1615/6807 (24%) 56.646/6.695/66.456/6.205 ms 517 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 33624 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.03 sec  8.74 MBytes  7.31 Mbits/sec   0.245 ms 574/6805 (8.4%) 61.729/21.799/72.651/0.411 ms 678 pps 15
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60978 (sock=4) (peer 2.1.6) on 2022-05-13 13:28:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.08 sec  7.19 MBytes  5.98 Mbits/sec   0.704 ms 2101/7231 (29%) 75.448/7.657/89.101/9.261 ms 509 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 54238 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  8.76 MBytes  7.32 Mbits/sec   0.364 ms 980/7230 (14%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45674 (sock=3) (peer 2.1.6) on 2022-05-13 13:29:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.06 sec  6.90 MBytes  5.76 Mbits/sec   0.649 ms 2731/7656 (36%) 88.468/30.260/94.274/4.096 ms 490 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 36935 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.04 sec  8.75 MBytes  7.31 Mbits/sec   0.471 ms 1411/7655 (18%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50200 (sock=4) (peer 2.1.6) on 2022-05-13 13:29:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  7.14 MBytes  5.95 Mbits/sec   0.613 ms 2992/8082 (37%) 87.934/29.139/89.781/4.219 ms 506 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 55866 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  8.75 MBytes  7.31 Mbits/sec   0.519 ms 1836/8081 (23%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39261 (sock=3) (peer 2.1.6) on 2022-05-13 13:29:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.06 sec  7.11 MBytes  5.93 Mbits/sec   0.549 ms 3433/8508 (40%) 87.889/29.059/95.340/4.116 ms 504 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2352 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 44518 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  8.78 MBytes  7.33 Mbits/sec   0.545 ms 2245/8506 (26%) -/-/-/- ms 846 pps
