------------------------------------------------------------
Server listening on UDP port 5001 with pid 2124
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49949 (sock=3) (peer 2.1.6) on 2022-05-13 12:52:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.19 MBytes  0.994 Mbits/sec   0.236 ms 7/854 (0.82%) -0.243/-0.481/3.278/0.204 ms 85 pps -512
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 51648 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.034 ms 0/853 (0%) 4.083/3.872/6.784/0.240 ms 85 pps 31
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37775 (sock=5) (peer 2.1.6) on 2022-05-13 12:53:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.77 MBytes  1.48 Mbits/sec   0.049 ms 17/1279 (1.3%) 0.194/0.059/2.692/0.161 ms 126 pps 954
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 38649 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.039 ms 0/1278 (0%) 3.671/3.438/5.925/0.196 ms 127 pps 51
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37027 (sock=3) (peer 2.1.6) on 2022-05-13 12:53:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.38 MBytes  2.00 Mbits/sec   0.014 ms 5/1704 (0.29%) 0.565/0.396/3.165/0.182 ms 170 pps 441
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 35845 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.020 ms 0/1703 (0%) 3.371/3.135/5.848/0.182 ms 170 pps 74
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53511 (sock=4) (peer 2.1.6) on 2022-05-13 12:53:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.030 ms 3/2129 (0.14%) 0.849/0.737/6.031/0.192 ms 212 pps 368
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 41668 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.257 ms 0/2128 (0%) 3.080/2.849/5.545/0.168 ms 212 pps 101
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54471 (sock=3) (peer 2.1.6) on 2022-05-13 12:54:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.57 MBytes  2.99 Mbits/sec   0.009 ms 11/2554 (0.43%) 1.120/0.982/5.899/0.210 ms 254 pps 334
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 59634 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.139 ms 0/2553 (0%) 2.919/2.691/5.946/0.181 ms 255 pps 129
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54079 (sock=4) (peer 2.1.6) on 2022-05-13 12:54:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.15 MBytes  3.48 Mbits/sec   0.022 ms 18/2980 (0.6%) 1.319/1.220/4.024/0.171 ms 296 pps 330
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 59928 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval       Transfer     Bandwidth        Jitter   Lost/Total Datagrams
[*12] 0.00-943272827.22 sec  3311740859203 MBytes  29452 Mbits/sec  943272827216.501 ms 909588537/875902519 (1e+02%)
[*12] 0.00-943272827.22 sec  808530483 datagrams received out-of-order
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35417 (sock=3) (peer 2.1.6) on 2022-05-13 12:54:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.70 MBytes  3.94 Mbits/sec   0.014 ms 55/3405 (1.6%) 1.451/1.287/5.769/0.246 ms 335 pps 339
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 46377 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.037 ms 0/3404 (0%) 2.561/2.347/5.885/0.193 ms 340 pps 195
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36093 (sock=4) (peer 2.1.6) on 2022-05-13 12:55:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.31 MBytes  4.45 Mbits/sec   0.198 ms 43/3830 (1.1%) 1.381/1.148/5.464/0.315 ms 379 pps 403
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 60875 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.025 ms 0/3829 (0%) 2.544/2.304/5.356/0.191 ms 382 pps 221
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59425 (sock=3) (peer 2.1.6) on 2022-05-13 12:55:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.87 MBytes  4.92 Mbits/sec   0.119 ms 70/4255 (1.6%) 1.574/1.326/4.857/0.286 ms 418 pps 391
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 54199 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.032 ms 0/4254 (0%) 2.428/2.137/5.337/0.212 ms 425 pps 257
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60135 (sock=4) (peer 2.1.6) on 2022-05-13 12:55:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.34 MBytes  5.32 Mbits/sec   0.175 ms 158/4680 (3.4%) 1.459/1.104/7.973/0.511 ms 452 pps 456
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 39641 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.045 ms 0/4679 (0%) 2.545/2.196/6.292/0.264 ms 467 pps 270
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50280 (sock=3) (peer 2.1.6) on 2022-05-13 12:56:08 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  6.98 MBytes  5.85 Mbits/sec   0.284 ms 127/5105 (2.5%) 1.526/1.303/4.524/0.422 ms 498 pps 479
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 46453 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.024 ms 0/5104 (0%) 2.363/2.006/5.301/0.267 ms 510 pps 317
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38379 (sock=4) (peer 2.1.6) on 2022-05-13 12:56:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  7.67 MBytes  6.43 Mbits/sec   0.051 ms 58/5531 (1%) 2.031/1.624/5.482/0.634 ms 547 pps 396
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 49279 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.028 ms 0/5530 (0%) 2.127/1.896/5.221/0.265 ms 552 pps 382
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51811 (sock=3) (peer 2.1.6) on 2022-05-13 12:56:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.03 sec  8.31 MBytes  6.95 Mbits/sec   0.042 ms 28/5956 (0.47%) 29.477/2.070/41.503/9.417 ms 591 pps 29
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 51544 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.98 sec  8.35 MBytes  7.02 Mbits/sec   0.028 ms 0/5955 (0%) 16.585/9.221/29.612/0.657 ms 596 pps 53
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52800 (sock=4) (peer 2.1.6) on 2022-05-13 12:57:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  8.39 MBytes  6.99 Mbits/sec   0.227 ms 397/6381 (6.2%) 48.051/-4.961/54.389/8.672 ms 595 pps 18
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 55477 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec   0.039 ms 0/6380 (0%) -/-/-/- ms 637 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51266 (sock=3) (peer 2.1.6) on 2022-05-13 12:57:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.05 sec  8.41 MBytes  7.02 Mbits/sec   0.385 ms 809/6806 (12%) 52.772/3.299/55.063/5.287 ms 597 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 35497 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   0.077 ms 0/6805 (0%) 2.027/1.375/13.040/0.691 ms 680 pps 493
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53401 (sock=4) (peer 2.1.6) on 2022-05-13 12:57:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.05 sec  8.39 MBytes  7.00 Mbits/sec   0.455 ms 1243/7231 (17%) 53.008/2.496/57.191/4.435 ms 596 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 37467 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.04 sec  9.87 MBytes  8.24 Mbits/sec   0.077 ms 193/7230 (2.7%) 41.761/2.042/53.555/0.325 ms 719 pps 25
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51556 (sock=3) (peer 2.1.6) on 2022-05-13 12:58:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.05 sec  8.09 MBytes  6.75 Mbits/sec   0.506 ms 1885/7657 (25%) 52.932/2.541/54.825/4.369 ms 574 pps 16
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 42096 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.04 sec  9.88 MBytes  8.25 Mbits/sec   0.217 ms 610/7655 (8%) 43.357/2.535/48.850/0.558 ms 762 pps 24
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41786 (sock=4) (peer 2.1.6) on 2022-05-13 12:58:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  8.38 MBytes  6.99 Mbits/sec   0.547 ms 2107/8083 (26%) 57.189/4.743/60.431/4.366 ms 594 pps 15
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 59220 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.03 sec  9.86 MBytes  8.24 Mbits/sec   0.343 ms 1047/8081 (13%) -/-/-/- ms 805 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39355 (sock=3) (peer 2.1.6) on 2022-05-13 12:58:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.04 sec  8.38 MBytes  7.00 Mbits/sec   0.560 ms 2527/8507 (30%) 62.609/18.356/71.041/4.508 ms 596 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2124 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 45282 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  9.88 MBytes  8.25 Mbits/sec   0.357 ms 1458/8506 (17%) -/-/-/- ms 846 pps
