------------------------------------------------------------
Server listening on UDP port 5001 with pid 3891
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39052 (sock=3) (peer 2.1.6) on 2022-05-13 15:43:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.049 ms 0/854 (0%) -3.031/-3.426/-0.888/0.286 ms 85 pps -41
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 39369 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.031 ms 0/853 (0%) 7.405/7.031/11.230/0.410 ms 85 pps 17
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58469 (sock=5) (peer 2.1.6) on 2022-05-13 15:44:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.040 ms 0/1279 (0%) -1.839/-2.133/1.774/0.271 ms 128 pps -102
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 38544 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.049 ms 0/1278 (0%) 6.371/5.987/9.877/0.301 ms 127 pps 29
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46958 (sock=3) (peer 2.1.6) on 2022-05-13 15:44:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.024 ms 0/1704 (0%) -1.181/-1.422/1.835/0.241 ms 170 pps -212
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 59832 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.029 ms 0/1703 (0%) 5.618/5.264/8.987/0.270 ms 170 pps 45
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47064 (sock=4) (peer 2.1.6) on 2022-05-13 15:44:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.024 ms 0/2129 (0%) -0.380/-0.551/4.955/0.250 ms 213 pps -822
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 42305 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.055 ms 0/2128 (0%) 5.051/4.684/8.267/0.274 ms 212 pps 62
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60346 (sock=3) (peer 2.1.6) on 2022-05-13 15:45:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.027 ms 0/2554 (0%) 0.201/-0.045/3.266/0.251 ms 255 pps 1863
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 52119 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.022 ms 0/2553 (0%) 4.415/4.072/7.839/0.289 ms 255 pps 85
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47019 (sock=4) (peer 2.1.6) on 2022-05-13 15:45:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.136 ms 0/2980 (0%) 0.824/0.646/3.759/0.288 ms 298 pps 531
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 55751 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.046 ms 0/2979 (0%) 3.869/3.531/7.600/0.299 ms 297 pps 113
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44971 (sock=3) (peer 2.1.6) on 2022-05-13 15:45:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.362 ms 0/3405 (0%) 1.201/0.959/4.598/0.385 ms 340 pps 416
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 38750 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.020 ms 0/3404 (0%) 3.600/3.218/7.051/0.283 ms 340 pps 139
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41475 (sock=4) (peer 2.1.6) on 2022-05-13 15:46:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.019 ms 0/3830 (0%) 1.595/1.259/5.796/0.555 ms 383 pps 353
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 55099 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.031 ms 0/3829 (0%) 3.331/3.033/6.986/0.293 ms 382 pps 169
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56650 (sock=3) (peer 2.1.6) on 2022-05-13 15:46:28 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.164 ms 0/4255 (0%) 2.034/1.328/8.083/0.968 ms 425 pps 307
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 42882 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.029 ms 0/4254 (0%) 3.297/2.825/7.599/0.484 ms 425 pps 190
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52258 (sock=4) (peer 2.1.6) on 2022-05-13 15:46:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.05 sec  6.37 MBytes  5.32 Mbits/sec   0.207 ms 136/4680 (2.9%) 54.720/2.130/68.864/11.122 ms 452 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 41265 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.056 ms 0/4679 (0%) 26.518/18.756/37.799/0.540 ms 468 pps 26
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60775 (sock=3) (peer 2.1.6) on 2022-05-13 15:47:09 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.08 sec  6.37 MBytes  5.30 Mbits/sec   0.380 ms 561/5105 (11%) -/-/-/- ms 451 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 60381 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-9.99 sec  7.16 MBytes  6.01 Mbits/sec   0.094 ms 0/5104 (0%) 9.086/5.410/20.120/0.650 ms 511 pps 83
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49457 (sock=4) (peer 2.1.6) on 2022-05-13 15:47:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.08 sec  6.38 MBytes  5.32 Mbits/sec   0.607 ms 977/5531 (18%) 67.997/-0.382/72.414/7.658 ms 452 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 59495 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.28 sec  6.58 MBytes  5.37 Mbits/sec  73.113 ms 837/5531 (15%) 16.696/0.399/1789.213/0.436 ms 538 pps 40
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57089 (sock=3) (peer 2.1.6) on 2022-05-13 15:47:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.692 ms 1403/5957 (24%) 70.708/4.314/77.441/6.318 ms 452 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 52467 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.06 sec  7.86 MBytes  6.56 Mbits/sec   0.171 ms 350/5955 (5.9%) 53.356/2.928/63.226/0.719 ms 592 pps 15
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34761 (sock=4) (peer 2.1.6) on 2022-05-13 15:48:09 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.748 ms 1823/6381 (29%) 70.919/4.115/73.606/5.633 ms 453 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 57824 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  7.85 MBytes  6.56 Mbits/sec   0.361 ms 781/6380 (12%) 52.179/4.260/63.583/0.368 ms 635 pps 16
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34551 (sock=3) (peer 2.1.6) on 2022-05-13 15:48:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.09 sec  6.42 MBytes  5.33 Mbits/sec   0.724 ms 2230/6806 (33%) 90.477/14.026/101.455/8.496 ms 454 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 35028 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.467 ms 1199/6806 (18%) -/-/-/- ms 676 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60107 (sock=4) (peer 2.1.6) on 2022-05-13 15:48:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.05 sec  6.38 MBytes  5.33 Mbits/sec   0.679 ms 2679/7231 (37%) 89.036/32.869/101.889/7.111 ms 453 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 39055 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.04 sec  7.86 MBytes  6.56 Mbits/sec   0.546 ms 1625/7231 (22%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53116 (sock=3) (peer 2.1.6) on 2022-05-13 15:49:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.08 sec  6.39 MBytes  5.31 Mbits/sec   0.579 ms 3102/7657 (41%) 95.047/23.322/101.199/6.011 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 32773 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.601 ms 2045/7655 (27%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58159 (sock=4) (peer 2.1.6) on 2022-05-13 15:49:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.701 ms 3526/8083 (44%) 100.202/33.803/136.147/5.118 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 45693 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  7.88 MBytes  6.57 Mbits/sec   0.646 ms 2464/8082 (30%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45357 (sock=3) (peer 2.1.6) on 2022-05-13 15:49:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.251 ms 3949/8507 (46%) 99.207/31.669/101.358/4.426 ms 453 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3891 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 39522 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  7.88 MBytes  6.58 Mbits/sec   0.583 ms 2884/8507 (34%) -/-/-/- ms 846 pps
