------------------------------------------------------------
Server listening on UDP port 5001 with pid 2290
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35876 (sock=3) (peer 2.1.6) on 2022-05-13 13:16:09 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.05 MBytes  0.877 Mbits/sec   0.267 ms 107/854 (13%) 10.898/10.154/13.384/0.651 ms 75 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 42333 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.103 ms 0/853 (0%) -/-/-/- ms 85 pps
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44682 (sock=5) (peer 2.1.6) on 2022-05-13 13:16:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.77 MBytes  1.48 Mbits/sec   0.016 ms 19/1279 (1.5%) 8.699/8.167/11.923/0.419 ms 126 pps 21
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 56616 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.026 ms 0/1278 (0%) -/-/-/- ms 127 pps
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59034 (sock=3) (peer 2.1.6) on 2022-05-13 13:16:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.31 MBytes  1.93 Mbits/sec   0.011 ms 58/1704 (3.4%) 7.415/6.894/11.625/0.358 ms 164 pps 33
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 43767 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.054 ms 0/1703 (0%) -/-/-/- ms 170 pps
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58200 (sock=4) (peer 2.1.6) on 2022-05-13 13:17:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  2.87 MBytes  2.40 Mbits/sec   0.030 ms 84/2129 (3.9%) 6.376/5.992/9.744/0.286 ms 204 pps 47
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 45230 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55820 (sock=3) (peer 2.1.6) on 2022-05-13 13:17:31 (CEST)
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.105 ms 0/2128 (0%) -/-/-/- ms 212 pps
[  9] 0.00-10.00 sec  3.53 MBytes  2.96 Mbits/sec   0.141 ms 37/2554 (1.4%) 5.573/5.069/9.094/0.346 ms 252 pps 66
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[SUM] 0.00-20.27 sec  6.51 MBytes  2.69 Mbits/sec  0/0      229 pps
[SUM-2] Sent 4683 datagrams
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 44443 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.034 ms 0/2553 (0%) -/-/-/- ms 255 pps
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44706 (sock=5) (peer 2.1.6) on 2022-05-13 13:17:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.07 MBytes  3.41 Mbits/sec   0.106 ms 77/2980 (2.6%) 4.913/4.563/8.164/0.387 ms 290 pps 87
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 41643 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.105 ms 0/2979 (0%) 0.259/0.050/5.542/0.326 ms 297 pps 1691
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58860 (sock=3) (peer 2.1.6) on 2022-05-13 13:18:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.05 sec  4.52 MBytes  3.78 Mbits/sec   2.722 ms 179/3406 (5.3%) 4.519/4.134/47.563/0.868 ms 321 pps 104
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 48776 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.025 ms 0/3404 (0%) 0.671/0.438/4.236/0.249 ms 340 pps 745
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33274 (sock=4) (peer 2.1.6) on 2022-05-13 13:18:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  4.87 MBytes  4.08 Mbits/sec   0.352 ms 356/3830 (9.3%) 4.249/3.789/7.990/0.571 ms 347 pps 120
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 44313 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53129 (sock=3) (peer 2.1.6) on 2022-05-13 13:18:53 (CEST)
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.026 ms 0/3829 (0%) 0.919/0.656/5.826/0.292 ms 382 pps 612
[ 17] 0.00-10.01 sec  5.83 MBytes  4.89 Mbits/sec   0.239 ms 94/4255 (2.2%) 4.189/3.486/10.861/1.081 ms 416 pps 146
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[SUM] 0.00-20.28 sec  11.2 MBytes  4.63 Mbits/sec  0/0      394 pps
[SUM-2] Sent 8085 datagrams
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 38375 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.032 ms 0/4254 (0%) 1.281/0.918/5.762/0.451 ms 425 pps 488
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44858 (sock=5) (peer 2.1.6) on 2022-05-13 13:19:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.02 sec  6.24 MBytes  5.23 Mbits/sec   0.227 ms 229/4681 (4.9%) 41.367/4.006/69.448/16.129 ms 444 pps 16
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 54139 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.97 sec  6.56 MBytes  5.52 Mbits/sec   0.055 ms 0/4679 (0%) 45.585/25.873/70.442/0.740 ms 469 pps 15
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59801 (sock=3) (peer 2.1.6) on 2022-05-13 13:19:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.07 sec  6.20 MBytes  5.16 Mbits/sec   0.413 ms 685/5105 (13%) -/-/-/- ms 439 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 58315 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-9.99 sec  5.99 MBytes  5.03 Mbits/sec   0.104 ms 831/5104 (16%) 31.828/6.322/1701.449/0.683 ms 511 pps 20
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41113 (sock=4) (peer 2.1.6) on 2022-05-13 13:19:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.08 sec  6.18 MBytes  5.14 Mbits/sec   0.587 ms 1125/5531 (20%) 70.567/-0.867/78.061/8.553 ms 437 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 36172 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.01 sec  6.49 MBytes  5.44 Mbits/sec   0.039 ms 902/5530 (16%) -/-/-/- ms 552 pps
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42537 (sock=3) (peer 2.1.6) on 2022-05-13 13:20:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.08 sec  6.31 MBytes  5.25 Mbits/sec   0.711 ms 1454/5956 (24%) 80.278/10.691/85.139/6.867 ms 447 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 58866 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.249 ms 350/5955 (5.9%) -/-/-/- ms 592 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59102 (sock=4) (peer 2.1.6) on 2022-05-13 13:20:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.07 sec  6.30 MBytes  5.25 Mbits/sec   0.757 ms 1884/6381 (30%) 91.712/22.962/95.385/5.689 ms 446 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 51033 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.349 ms 772/6380 (12%) -/-/-/- ms 634 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38510 (sock=3) (peer 2.1.6) on 2022-05-13 13:20:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.07 sec  6.30 MBytes  5.25 Mbits/sec   0.714 ms 2313/6806 (34%) 99.863/31.799/102.866/5.731 ms 446 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 55470 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.05 sec  7.87 MBytes  6.56 Mbits/sec   0.513 ms 1194/6805 (18%) -/-/-/- ms 676 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43241 (sock=4) (peer 2.1.6) on 2022-05-13 13:21:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.07 sec  6.29 MBytes  5.24 Mbits/sec   0.669 ms 2748/7232 (38%) 102.246/39.370/104.481/4.705 ms 445 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 41264 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.06 sec  7.87 MBytes  6.57 Mbits/sec   0.549 ms 1616/7230 (22%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48030 (sock=3) (peer 2.1.6) on 2022-05-13 13:21:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  6.20 MBytes  5.17 Mbits/sec   0.550 ms 3233/7656 (42%) 101.619/34.561/134.460/4.969 ms 439 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 51833 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  7.88 MBytes  6.57 Mbits/sec   0.592 ms 2037/7656 (27%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42390 (sock=4) (peer 2.1.6) on 2022-05-13 13:21:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.07 sec  6.29 MBytes  5.24 Mbits/sec   0.418 ms 3594/8082 (44%) 101.183/34.108/103.118/4.749 ms 446 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 41850 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  7.89 MBytes  6.58 Mbits/sec   0.627 ms 2455/8081 (30%) -/-/-/- ms 803 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50100 (sock=3) (peer 2.1.6) on 2022-05-13 13:22:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.07 sec  6.22 MBytes  5.18 Mbits/sec   0.232 ms 4068/8507 (48%) 100.960/34.375/103.638/4.711 ms 441 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2290 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 59891 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  7.89 MBytes  6.58 Mbits/sec   0.585 ms 2878/8506 (34%) -/-/-/- ms 845 pps
