------------------------------------------------------------
Server listening on UDP port 5001 with pid 2236
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36385 (sock=3) (peer 2.1.6) on 2022-05-13 13:08:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.028 ms 0/854 (0%) 4.881/4.626/7.569/0.313 ms 85 pps 26
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 59291 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.041 ms 0/853 (0%) 0.467/0.243/1.971/0.133 ms 85 pps 268
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41081 (sock=5) (peer 2.1.6) on 2022-05-13 13:08:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.010 ms 0/1279 (0%) 4.081/3.938/9.493/0.277 ms 128 pps 46
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 47874 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.028 ms 0/1278 (0%) 1.096/0.954/3.926/0.174 ms 127 pps 171
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60523 (sock=3) (peer 2.1.6) on 2022-05-13 13:09:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.046 ms 0/1704 (0%) 3.827/3.529/7.319/0.231 ms 170 pps 65
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 43116 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.036 ms 0/1703 (0%) 1.484/1.301/5.081/0.185 ms 170 pps 169
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38928 (sock=4) (peer 2.1.6) on 2022-05-13 13:09:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.189 ms 0/2129 (0%) 3.406/3.156/7.086/0.264 ms 213 pps 92
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 58596 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-9.99 sec  2.98 MBytes  2.51 Mbits/sec   0.025 ms 0/2128 (0%) 1.846/1.563/21.087/0.851 ms 213 pps 170
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40441 (sock=3) (peer 2.1.6) on 2022-05-13 13:10:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.010 ms 0/2554 (0%) 3.193/2.934/6.596/0.299 ms 255 pps 118
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 41704 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.036 ms 0/2553 (0%) 1.776/1.581/5.246/0.237 ms 255 pps 211
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57094 (sock=4) (peer 2.1.6) on 2022-05-13 13:10:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.029 ms 0/2980 (0%) 3.117/2.760/6.629/0.338 ms 298 pps 140
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 35697 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.020 ms 0/2979 (0%) 1.948/1.682/5.567/0.229 ms 297 pps 225
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48687 (sock=3) (peer 2.1.6) on 2022-05-13 13:10:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.111 ms 0/3405 (0%) 2.907/2.630/7.608/0.407 ms 340 pps 172
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 51900 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.021 ms 0/3404 (0%) 2.016/1.736/5.850/0.278 ms 340 pps 248
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55401 (sock=4) (peer 2.1.6) on 2022-05-13 13:11:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.332 ms 0/3830 (0%) 2.960/2.619/6.698/0.549 ms 383 pps 190
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 41307 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.059 ms 0/3829 (0%) 2.038/1.702/5.866/0.307 ms 382 pps 276
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 32953 (sock=3) (peer 2.1.6) on 2022-05-13 13:11:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.213 ms 0/4255 (0%) 3.193/2.468/7.623/0.913 ms 425 pps 196
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 33890 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.028 ms 0/4254 (0%) 2.142/1.798/5.815/0.365 ms 425 pps 292
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46153 (sock=4) (peer 2.1.6) on 2022-05-13 13:11:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.04 sec  6.37 MBytes  5.32 Mbits/sec   0.072 ms 139/4680 (3%) 48.835/3.112/68.710/12.700 ms 453 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 43040 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.97 sec  6.56 MBytes  5.52 Mbits/sec   0.010 ms 0/4679 (0%) 27.486/15.599/45.721/0.409 ms 469 pps 25
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39947 (sock=3) (peer 2.1.6) on 2022-05-13 13:12:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.09 sec  6.38 MBytes  5.30 Mbits/sec   0.458 ms 556/5105 (11%) -/-/-/- ms 451 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 60892 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-9.99 sec  7.16 MBytes  6.01 Mbits/sec   0.195 ms 0/5104 (0%) -/-/-/- ms 510 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49378 (sock=4) (peer 2.1.6) on 2022-05-13 13:12:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.02 sec  6.38 MBytes  5.34 Mbits/sec   0.576 ms 980/5531 (18%) 50.221/10.071/77.193/15.332 ms 454 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 54652 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.97 sec  7.75 MBytes  6.52 Mbits/sec   0.119 ms 0/5530 (0%) 32.223/16.160/54.012/0.873 ms 554 pps 25
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37106 (sock=3) (peer 2.1.6) on 2022-05-13 13:12:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.06 sec  6.38 MBytes  5.32 Mbits/sec   0.735 ms 1408/5956 (24%) -/-/-/- ms 452 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 52507 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.02 sec  7.82 MBytes  6.55 Mbits/sec   0.181 ms 376/5955 (6.3%) 71.942/36.377/87.593/0.391 ms 594 pps 11
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34054 (sock=4) (peer 2.1.6) on 2022-05-13 13:13:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.10 sec  6.38 MBytes  5.30 Mbits/sec   0.765 ms 1830/6381 (29%) 86.586/2.550/105.172/12.412 ms 450 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 42869 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.05 sec  7.88 MBytes  6.57 Mbits/sec   0.371 ms 761/6380 (12%) -/-/-/- ms 634 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50006 (sock=3) (peer 2.1.6) on 2022-05-13 13:13:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.07 sec  6.41 MBytes  5.34 Mbits/sec   0.761 ms 2235/6807 (33%) 103.229/37.835/105.840/5.190 ms 454 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 51732 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.05 sec  7.85 MBytes  6.55 Mbits/sec   0.503 ms 1206/6805 (18%) -/-/-/- ms 676 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38573 (sock=4) (peer 2.1.6) on 2022-05-13 13:13:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.660 ms 2678/7231 (37%) 102.554/35.654/107.703/5.016 ms 452 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 34354 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.575 ms 1622/7230 (22%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48709 (sock=3) (peer 2.1.6) on 2022-05-13 13:14:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.557 ms 3104/7656 (41%) 102.183/37.180/106.044/4.750 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 45889 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  7.87 MBytes  6.57 Mbits/sec   0.585 ms 2041/7656 (27%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56586 (sock=4) (peer 2.1.6) on 2022-05-13 13:14:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.483 ms 3529/8083 (44%) 101.989/36.828/136.783/4.961 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 54299 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.06 sec  7.89 MBytes  6.58 Mbits/sec   0.586 ms 2452/8081 (30%) -/-/-/- ms 803 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35127 (sock=3) (peer 2.1.6) on 2022-05-13 13:14:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.01 sec  6.38 MBytes  5.35 Mbits/sec   0.247 ms 3955/8507 (46%) 73.297/36.672/102.352/16.634 ms 455 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2236 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 50131 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.11 sec  7.92 MBytes  6.57 Mbits/sec   0.588 ms 2861/8507 (34%) 111.496/36.280/140.808/0.841 ms 841 pps 7
