------------------------------------------------------------
Server listening on UDP port 5001 with pid 3947
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59805 (sock=3) (peer 2.1.6) on 2022-05-13 15:51:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.092 ms 0/854 (0%) 0.479/0.310/2.974/0.192 ms 85 pps 261
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3947 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 56257 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.036 ms 0/853 (0%) 3.934/3.720/6.844/0.274 ms 85 pps 32
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51042 (sock=5) (peer 2.1.6) on 2022-05-13 15:51:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.097 ms 0/1279 (0%) 0.707/0.515/3.931/0.209 ms 128 pps 265
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3947 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 35658 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.026 ms 0/1278 (0%) 3.631/3.362/6.247/0.209 ms 127 pps 52
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45265 (sock=3) (peer 2.1.6) on 2022-05-13 15:52:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.036 ms 0/1704 (0%) 0.970/0.757/3.742/0.209 ms 170 pps 258
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3947 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 55901 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.148 ms 0/1703 (0%) 3.332/3.095/6.265/0.201 ms 170 pps 75
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44530 (sock=4) (peer 2.1.6) on 2022-05-13 15:52:28 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.100 ms 0/2129 (0%) 1.338/1.151/4.337/0.196 ms 213 pps 234
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3947 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 34156 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.064 ms 0/2128 (0%) 3.124/2.868/6.245/0.191 ms 212 pps 100
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34320 (sock=3) (peer 2.1.6) on 2022-05-13 15:52:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.054 ms 0/2554 (0%) 1.571/1.385/4.768/0.215 ms 255 pps 239
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3947 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34320 (sock=4) (peer 2.1.6) on 2022-05-13 15:52:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-0.01 sec  0.001 MBytes  2.07 Mbits/sec   0.000 ms 2564/2566 (1e+02%) 164.601/161.757/167.444/161.807 ms 176 pps 2
[ 11] 0.00-0.01 sec  1 datagrams received out-of-order
[*10] local 10.0.23.60%eth0 port 43475 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3947 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 41498 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-9.99 sec  3.58 MBytes  3.01 Mbits/sec   0.286 ms 0/2553 (0%) 2.836/2.418/19.556/0.814 ms 255 pps 132
[*12] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 12] Sent 2554 datagrams
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42198 (sock=5) (peer 2.1.6) on 2022-05-13 15:53:09 (CEST)
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-0.02 sec  0.003 MBytes  1.17 Mbits/sec   1.259 ms 2552/2554 (1e+02%) 12.640/2.566/22.714/14.476 ms 126761 pps 12
[ 13] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.046 ms 0/2980 (0%) 2.022/1.864/5.981/0.255 ms 298 pps 217
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[SUM] 0.00-20.28 sec  11.3 MBytes  4.69 Mbits/sec  2564/0        0 pps
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34076 (sock=3) (peer 2.1.6) on 2022-05-13 15:53:19 (CEST)
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3947 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 50268 connected with 10.0.23.61 port 5001 (reverse) (sock=5) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.034 ms 0/3405 (0%) 1.845/1.661/4.792/0.258 ms 340 pps 271
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 14] Sent 2980 datagrams
------------------------------------------------------------
Server listening on UDP port 5001 with pid 3969
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37388 (sock=3) (peer 2.1.6) on 2022-05-13 15:54:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.337 ms 0/2980 (0%) 1.960/1.753/5.136/0.261 ms 298 pps 223
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 56468 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[  2] Sent 2980 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.016 ms 0/2979 (0%) 2.522/2.236/6.425/0.230 ms 297 pps 174
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55936 (sock=5) (peer 2.1.6) on 2022-05-13 15:55:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.045 ms 0/3405 (0%) 1.999/1.772/6.418/0.281 ms 340 pps 250
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 36080 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  4] Sent 3405 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.030 ms 0/3404 (0%) 2.379/2.073/5.437/0.223 ms 340 pps 210
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47890 (sock=3) (peer 2.1.6) on 2022-05-13 15:55:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.030 ms 0/3830 (0%) 2.211/1.958/5.253/0.335 ms 383 pps 255
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 49019 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[  6] Sent 3830 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.036 ms 0/3829 (0%) 2.212/1.896/5.334/0.249 ms 382 pps 254
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40661 (sock=4) (peer 2.1.6) on 2022-05-13 15:55:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.016 ms 0/4255 (0%) 2.335/1.990/7.609/0.499 ms 425 pps 268
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 56312 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[  8] Sent 4255 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-9.99 sec  5.96 MBytes  5.01 Mbits/sec   0.068 ms 0/4254 (0%) 2.295/2.022/19.170/0.813 ms 425 pps 273
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44273 (sock=3) (peer 2.1.6) on 2022-05-13 15:56:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.017 ms 0/4680 (0%) 2.517/2.057/9.095/0.678 ms 468 pps 273
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 42553 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 10] Sent 4680 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.048 ms 0/4679 (0%) 2.130/1.795/5.223/0.302 ms 467 pps 323
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39617 (sock=4) (peer 2.1.6) on 2022-05-13 15:56:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.043 ms 1/5105 (0.02%) 4.712/0.137/10.984/2.382 ms 510 pps 159
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 57155 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.038 ms 0/5104 (0%) 3.367/2.505/7.331/0.633 ms 510 pps 223
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47917 (sock=3) (peer 2.1.6) on 2022-05-13 15:56:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.203 ms 356/5532 (6.4%) 59.009/1.922/66.032/9.121 ms 514 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 52629 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 14] Sent 5531 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.040 ms 0/5530 (0%) 1.859/1.550/7.543/0.509 ms 553 pps 437
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48740 (sock=4) (peer 2.1.6) on 2022-05-13 15:57:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.407 ms 779/5956 (13%) 60.620/2.918/69.724/6.810 ms 514 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 59066 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 16] Sent 5956 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-9.99 sec  8.35 MBytes  7.01 Mbits/sec   0.044 ms 0/5955 (0%) 2.145/1.723/10.241/0.847 ms 595 pps 408
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56023 (sock=3) (peer 2.1.6) on 2022-05-13 15:57:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.06 sec  7.27 MBytes  6.06 Mbits/sec   0.558 ms 1198/6381 (19%) 61.043/3.755/62.989/5.559 ms 515 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 55979 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 18] Sent 6381 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.05 sec  8.75 MBytes  7.31 Mbits/sec   0.067 ms 136/6380 (2.1%) 46.956/4.965/52.434/0.664 ms 634 pps 19
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59491 (sock=4) (peer 2.1.6) on 2022-05-13 15:57:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.02 sec  7.27 MBytes  6.09 Mbits/sec   0.624 ms 1618/6806 (24%) 41.195/3.334/62.826/12.202 ms 518 pps 18
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 52549 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 20] Sent 6806 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.03 sec  8.75 MBytes  7.32 Mbits/sec   0.263 ms 565/6805 (8.3%) 92.258/45.423/109.822/0.745 ms 678 pps 10
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54857 (sock=3) (peer 2.1.6) on 2022-05-13 15:58:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.10 sec  7.26 MBytes  6.03 Mbits/sec   0.650 ms 2052/7231 (28%) -/-/-/- ms 513 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 46761 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 22] Sent 7231 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.03 sec  8.75 MBytes  7.31 Mbits/sec   0.346 ms 992/7230 (14%) -/-/-/- ms 720 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41086 (sock=4) (peer 2.1.6) on 2022-05-13 15:58:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.05 sec  7.27 MBytes  6.06 Mbits/sec   0.644 ms 2473/7657 (32%) 92.535/38.171/97.610/4.659 ms 516 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 47784 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 24] Sent 7656 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.05 sec  8.76 MBytes  7.31 Mbits/sec   0.490 ms 1407/7655 (18%) -/-/-/- ms 761 pps
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34222 (sock=3) (peer 2.1.6) on 2022-05-13 15:58:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.06 sec  7.27 MBytes  6.06 Mbits/sec   0.600 ms 2898/8083 (36%) 88.357/29.523/93.590/4.318 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 59260 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 26] Sent 8082 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.05 sec  8.75 MBytes  7.31 Mbits/sec   0.497 ms 1837/8082 (23%) -/-/-/- ms 804 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35061 (sock=4) (peer 2.1.6) on 2022-05-13 15:59:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  7.26 MBytes  6.06 Mbits/sec   0.586 ms 3327/8508 (39%) 88.421/29.555/92.886/4.176 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3969 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 50578 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 28] Sent 8507 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.05 sec  8.77 MBytes  7.32 Mbits/sec   0.535 ms 2249/8506 (26%) -/-/-/- ms 846 pps
