------------------------------------------------------------
Server listening on UDP port 5001 with pid 3719
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37691 (sock=3) (peer 2.1.6) on 2022-05-13 15:19:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.015 ms 0/854 (0%) 2.168/2.023/4.002/0.166 ms 85 pps 58
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 43949 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.067 ms 0/853 (0%) 1.824/1.667/4.653/0.199 ms 85 pps 69
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44006 (sock=5) (peer 2.1.6) on 2022-05-13 15:19:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.117 ms 1/1279 (0.078%) 2.250/2.116/4.099/0.178 ms 128 pps 83
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 60610 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.103 ms 0/1278 (0%) 1.836/1.684/4.394/0.148 ms 127 pps 102
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33348 (sock=3) (peer 2.1.6) on 2022-05-13 15:19:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.013 ms 0/1704 (0%) 2.172/2.000/6.181/0.232 ms 170 pps 115
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 42149 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.020 ms 0/1703 (0%) 1.873/1.735/5.159/0.161 ms 170 pps 134
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41055 (sock=4) (peer 2.1.6) on 2022-05-13 15:20:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.021 ms 1/2129 (0.047%) 2.128/1.959/4.910/0.169 ms 213 pps 147
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 43852 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.015 ms 0/2128 (0%) 1.950/1.754/4.751/0.166 ms 212 pps 160
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46745 (sock=3) (peer 2.1.6) on 2022-05-13 15:20:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.015 ms 1/2554 (0.039%) 2.165/2.013/4.701/0.171 ms 255 pps 173
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 58877 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.021 ms 0/2553 (0%) 1.912/1.703/5.505/0.179 ms 255 pps 196
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57682 (sock=4) (peer 2.1.6) on 2022-05-13 15:20:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.021 ms 0/2980 (0%) 2.123/1.905/5.718/0.203 ms 298 pps 206
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 46817 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.036 ms 0/2979 (0%) 2.049/1.846/4.487/0.154 ms 297 pps 214
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37414 (sock=3) (peer 2.1.6) on 2022-05-13 15:21:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.085 ms 0/3405 (0%) 2.028/1.878/4.814/0.206 ms 340 pps 247
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 54517 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.022 ms 0/3404 (0%) 2.034/1.798/5.329/0.181 ms 340 pps 246
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45189 (sock=4) (peer 2.1.6) on 2022-05-13 15:21:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.193 ms 0/3830 (0%) 2.023/1.752/4.787/0.253 ms 383 pps 278
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 41028 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.218 ms 0/3829 (0%) 2.027/1.771/4.592/0.194 ms 382 pps 278
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45699 (sock=3) (peer 2.1.6) on 2022-05-13 15:22:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.044 ms 0/4255 (0%) 2.158/1.961/6.247/0.279 ms 425 pps 290
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 44740 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.042 ms 0/4254 (0%) 1.813/1.598/4.372/0.192 ms 425 pps 345
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57833 (sock=4) (peer 2.1.6) on 2022-05-13 15:22:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.010 ms 2/4680 (0.043%) 2.222/1.879/5.039/0.355 ms 468 pps 309
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 49794 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.087 ms 0/4679 (0%) 1.962/1.715/4.796/0.204 ms 467 pps 350
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46311 (sock=3) (peer 2.1.6) on 2022-05-13 15:22:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.15 MBytes  6.00 Mbits/sec   0.241 ms 4/5105 (0.078%) 2.060/1.750/5.714/0.467 ms 510 pps 364
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 51308 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.031 ms 0/5104 (0%) 2.033/1.747/7.778/0.313 ms 510 pps 369
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46941 (sock=4) (peer 2.1.6) on 2022-05-13 15:23:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.067 ms 2/5531 (0.036%) 2.256/1.775/7.217/0.636 ms 553 pps 360
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 42409 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.032 ms 0/5530 (0%) 1.961/1.699/4.774/0.259 ms 552 pps 414
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57449 (sock=3) (peer 2.1.6) on 2022-05-13 15:23:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.03 sec  8.34 MBytes  6.98 Mbits/sec   0.032 ms 5/5956 (0.084%) 25.881/2.303/39.301/9.874 ms 593 pps 34
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 51813 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.98 sec  8.35 MBytes  7.02 Mbits/sec   0.129 ms 0/5955 (0%) 10.146/4.207/24.689/0.386 ms 596 pps 86
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38095 (sock=4) (peer 2.1.6) on 2022-05-13 15:23:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  8.39 MBytes  7.00 Mbits/sec   0.212 ms 397/6381 (6.2%) 50.506/-0.070/55.615/8.087 ms 595 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 50775 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec   0.038 ms 0/6380 (0%) 1.149/0.875/3.908/0.342 ms 637 pps 816
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46499 (sock=3) (peer 2.1.6) on 2022-05-13 15:24:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.05 sec  8.44 MBytes  7.04 Mbits/sec   0.314 ms 785/6806 (12%) 52.469/2.961/58.060/5.645 ms 599 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 35268 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.01 sec  7.98 MBytes  6.68 Mbits/sec   0.057 ms 1116/6805 (16%) 18.286/1.396/1687.399/0.321 ms 679 pps 46
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34576 (sock=4) (peer 2.1.6) on 2022-05-13 15:24:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.05 sec  8.40 MBytes  7.01 Mbits/sec   0.468 ms 1237/7231 (17%) 53.145/2.786/55.303/4.884 ms 596 pps 16
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 34705 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.04 sec  9.87 MBytes  8.25 Mbits/sec   0.096 ms 190/7230 (2.6%) 39.666/1.864/48.303/0.778 ms 720 pps 26
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46355 (sock=3) (peer 2.1.6) on 2022-05-13 15:24:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  8.38 MBytes  6.98 Mbits/sec   0.541 ms 1676/7656 (22%) 68.496/10.016/81.162/7.041 ms 594 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 33633 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.04 sec  9.88 MBytes  8.25 Mbits/sec   0.186 ms 609/7655 (8%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45082 (sock=4) (peer 2.1.6) on 2022-05-13 15:25:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.05 sec  8.38 MBytes  6.99 Mbits/sec   0.589 ms 2104/8082 (26%) 75.717/25.491/80.594/3.904 ms 595 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 36976 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  9.90 MBytes  8.27 Mbits/sec   0.308 ms 1018/8082 (13%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41880 (sock=3) (peer 2.1.6) on 2022-05-13 15:25:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.05 sec  8.39 MBytes  7.00 Mbits/sec   0.572 ms 2520/8507 (30%) 75.170/24.665/77.180/3.811 ms 596 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3719 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 51745 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  9.89 MBytes  8.26 Mbits/sec   0.374 ms 1454/8506 (17%) -/-/-/- ms 846 pps
------------------------------------------------------------
Server listening on UDP port 5001 with pid 3774
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
