------------------------------------------------------------
Server listening on UDP port 5001 with pid 6660
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 44853 (sock=3) (peer 2.1.6) on 2022-05-10 16:52:57 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.00 sec  1.20 MBytes  1.00 Mbits/sec   1.697 ms 0/854 (0%) -/-/-/- ms 85 pps
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 46700 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   6.807 ms 0/853 (0%) 25.151/15.799/90.537/1.542 ms 85 pps 5
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 42948 (sock=5) (peer 2.1.6) on 2022-05-10 16:53:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.02 sec  2.39 MBytes  2.00 Mbits/sec   4.506 ms 0/1704 (0%) -/-/-/- ms 170 pps
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 51728 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.02 sec  2.39 MBytes  2.00 Mbits/sec   8.240 ms 0/1703 (0%) 15.375/1.412/68.819/1.570 ms 169 pps 16
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 54388 (sock=3) (peer 2.1.6) on 2022-05-10 16:53:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  3.58 MBytes  3.00 Mbits/sec   2.296 ms 0/2554 (0%) 6.321/0.861/50.223/6.244 ms 255 pps 59
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 35045 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-9.98 sec  3.58 MBytes  3.01 Mbits/sec   3.643 ms 0/2553 (0%) -/-/-/- ms 255 pps
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58592 (sock=4) (peer 2.1.6) on 2022-05-10 16:53:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   1.027 ms 0/3405 (0%) 6.782/2.918/46.475/4.760 ms 340 pps 74
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 54542 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-9.99 sec  4.77 MBytes  4.01 Mbits/sec   3.471 ms 0/3404 (0%) -/-/-/- ms 340 pps
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51256 (sock=3) (peer 2.1.6) on 2022-05-10 16:54:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   1.644 ms 0/4255 (0%) 8.487/4.430/43.024/3.686 ms 425 pps 74
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 60682 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-9.98 sec  5.96 MBytes  5.01 Mbits/sec   2.710 ms 0/4254 (0%) -/-/-/- ms 426 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 48227 (sock=4) (peer 2.1.6) on 2022-05-10 16:54:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  7.16 MBytes  6.00 Mbits/sec   1.842 ms 0/5105 (0%) 7.947/3.732/42.742/3.989 ms 510 pps 94
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 55422 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   2.081 ms 0/5104 (0%) -/-/-/- ms 510 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35800 (sock=3) (peer 2.1.6) on 2022-05-10 16:55:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.01 sec  8.35 MBytes  7.00 Mbits/sec   2.152 ms 0/5956 (0%) 12.048/5.107/58.790/6.358 ms 595 pps 73
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 58916 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  8.05 MBytes  6.75 Mbits/sec   2.065 ms 215/5955 (3.6%) -/-/-/- ms 595 pps
[ 15] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46369 (sock=4) (peer 2.1.6) on 2022-05-10 16:55:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.01 sec  9.54 MBytes  7.99 Mbits/sec   2.364 ms 4/6806 (0.059%) 12.867/5.252/146.064/15.390 ms 679 pps 78
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.217%eth0 port 54332 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 16] Sent 6806 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-9.98 sec  9.54 MBytes  8.02 Mbits/sec   1.642 ms 0/6805 (0%) -/-/-/- ms 681 pps
[ 17] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36617 (sock=3) (peer 2.1.6) on 2022-05-10 16:55:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.01 sec  10.7 MBytes  9.00 Mbits/sec   1.634 ms 0/7656 (0%) 14.664/9.689/55.520/4.850 ms 765 pps 77
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.217%eth0 port 56646 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 18] Sent 7656 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.01 sec  10.7 MBytes  9.00 Mbits/sec   2.030 ms 0/7655 (0%) -/-/-/- ms 764 pps
[ 19] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40076 (sock=4) (peer 2.1.6) on 2022-05-10 16:56:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.01 sec  11.9 MBytes  10.0 Mbits/sec   1.296 ms 0/8507 (0%) 11.377/6.210/57.826/6.207 ms 850 pps 110
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.217%eth0 port 33488 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 20] Sent 8507 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.02 sec  11.9 MBytes  9.98 Mbits/sec   1.723 ms 0/8506 (0%) -/-/-/- ms 848 pps
[ 21] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 37317 (sock=3) (peer 2.1.6) on 2022-05-10 16:56:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec   1.010 ms 0/9357 (0%) 9.804/6.398/28.086/3.089 ms 935 pps 140
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1069.09 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.217%eth0 port 47321 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec  0/0      936 pps
[ 22] Sent 9357 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec   0.987 ms 0/9356 (0%) -/-/-/- ms 935 pps
[ 23] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36264 (sock=4) (peer 2.1.6) on 2022-05-10 16:56:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec   0.983 ms 0/10207 (0%) 10.508/7.352/34.247/3.126 ms 1021 pps 143
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 980.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.217%eth0 port 55157 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec  0/0     1021 pps
[ 24] Sent 10207 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.03 sec  14.3 MBytes  12.0 Mbits/sec   1.704 ms 0/10206 (0%) -/-/-/- ms 1017 pps
[ 25] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58350 (sock=3) (peer 2.1.6) on 2022-05-10 16:57:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec   1.020 ms 0/11058 (0%) 9.166/5.095/39.178/3.960 ms 1106 pps 177
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 904.62 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.217%eth0 port 56630 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec  0/0     1106 pps
[ 26] Sent 11058 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec   0.857 ms 0/11057 (0%) -/-/-/- ms 1105 pps
[ 27] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 39702 (sock=4) (peer 2.1.6) on 2022-05-10 16:57:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec   0.986 ms 7/11908 (0.059%) 15.229/7.124/143.341/13.658 ms 1190 pps 115
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.217%eth0 port 38595 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec  0/0     1191 pps
[ 28] Sent 11908 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec   1.164 ms 0/11907 (0%) -/-/-/- ms 1190 pps
[ 29] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38570 (sock=3) (peer 2.1.6) on 2022-05-10 16:57:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec   0.858 ms 0/12758 (0%) 8.071/5.369/30.804/2.646 ms 1276 pps 232
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.217%eth0 port 45322 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[ 30] Sent 12758 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.01 sec  17.7 MBytes  14.8 Mbits/sec   1.199 ms 133/12757 (1%) -/-/-/- ms 1273 pps
[ 31] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58057 (sock=4) (peer 2.1.6) on 2022-05-10 16:58:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-9.95 sec  19.1 MBytes  16.1 Mbits/sec   1.059 ms 0/13609 (0%) 11.040/5.591/83.200/7.227 ms 1367 pps 182
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 735.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.217%eth0 port 51111 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec  0/0     1361 pps
[ 32] Sent 13609 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec   0.834 ms 0/13608 (0%) -/-/-/- ms 1361 pps
[ 33] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38917 (sock=3) (peer 2.1.6) on 2022-05-10 16:58:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-9.99 sec  20.3 MBytes  17.0 Mbits/sec   0.759 ms 0/14459 (0%) 8.554/4.234/32.262/3.128 ms 1447 pps 249
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 691.76 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.217%eth0 port 54529 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec  0/0     1446 pps
[ 34] Sent 14459 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.01 sec  20.3 MBytes  17.0 Mbits/sec   0.915 ms 0/14458 (0%) -/-/-/- ms 1444 pps
[ 35] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 33867 (sock=4) (peer 2.1.6) on 2022-05-10 16:58:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.00 sec  21.4 MBytes  18.0 Mbits/sec   0.730 ms 28/15309 (0.18%) 8.813/3.449/96.327/8.160 ms 1528 pps 255
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 653.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.217%eth0 port 34951 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec  0/0     1531 pps
[ 36] Sent 15309 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  21.5 MBytes  17.9 Mbits/sec   1.145 ms 0/15308 (0%) -/-/-/- ms 1524 pps
[ 37] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45444 (sock=3) (peer 2.1.6) on 2022-05-10 16:59:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.05 sec  22.3 MBytes  18.6 Mbits/sec   1.847 ms 247/16160 (1.5%) 16.146/6.999/164.369/18.734 ms 1584 pps 144
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 618.95 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.217%eth0 port 36224 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec  0/0     1616 pps
[ 38] Sent 16160 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.03 sec  22.7 MBytes  19.0 Mbits/sec   1.811 ms 0/16159 (0%) -/-/-/- ms 1611 pps
[ 39] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45424 (sock=4) (peer 2.1.6) on 2022-05-10 16:59:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 39] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec   0.819 ms 0/17010 (0%) 12.908/5.497/63.226/7.493 ms 1701 pps 194
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 588.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*40] local 10.0.23.217%eth0 port 54575 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*40] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec  0/0     1701 pps
[ 40] Sent 17010 datagrams
[ 40] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*40] 0.00-10.05 sec  23.8 MBytes  19.9 Mbits/sec   0.844 ms 6/17009 (0.035%) -/-/-/- ms 1693 pps
[ 41] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 54065 (sock=3) (peer 2.1.6) on 2022-05-10 16:59:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 41] 0.00-10.01 sec  25.0 MBytes  21.0 Mbits/sec   0.887 ms 0/17860 (0%) 10.491/5.203/43.270/4.805 ms 1785 pps 250
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 560.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*42] local 10.0.23.217%eth0 port 33816 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec  0/0     1786 pps
[ 42] Sent 17860 datagrams
[ 42] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*42] 0.00-10.00 sec  24.6 MBytes  20.7 Mbits/sec   0.573 ms 291/17859 (1.6%) -/-/-/- ms 1785 pps
[ 43] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 49386 (sock=4) (peer 2.1.6) on 2022-05-10 17:00:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 43] 0.00-10.01 sec  26.2 MBytes  22.0 Mbits/sec   0.908 ms 0/18711 (0%) 14.218/7.052/40.003/4.811 ms 1869 pps 193
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 534.55 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*44] local 10.0.23.217%eth0 port 48656 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*44] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec  0/0     1871 pps
[ 44] Sent 18711 datagrams
[ 44] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*44] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec   0.434 ms 0/18710 (0%) -/-/-/- ms 1870 pps
[ 45] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 57008 (sock=3) (peer 2.1.6) on 2022-05-10 17:00:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 45] 0.00-10.01 sec  27.4 MBytes  23.0 Mbits/sec   0.840 ms 0/19561 (0%) 12.600/7.030/40.720/4.560 ms 1955 pps 228
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 511.30 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*46] local 10.0.23.217%eth0 port 33207 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*46] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec  0/0     1956 pps
[ 46] Sent 19561 datagrams
[ 46] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*46] 0.00-10.04 sec  27.1 MBytes  22.7 Mbits/sec   2.440 ms 216/19560 (1.1%) -/-/-/- ms 1948 pps
[ 47] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 41993 (sock=4) (peer 2.1.6) on 2022-05-10 17:00:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 47] 0.00-10.01 sec  28.6 MBytes  24.0 Mbits/sec   0.700 ms 0/20411 (0%) 11.367/3.008/43.625/5.216 ms 2039 pps 264
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*48] local 10.0.23.217%eth0 port 40538 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*48] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec  0/0     2041 pps
[ 48] Sent 20411 datagrams
[ 48] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*48] 0.00-10.01 sec  28.6 MBytes  24.0 Mbits/sec   0.367 ms 0/20410 (0%) -/-/-/- ms 2039 pps
[ 49] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58453 (sock=3) (peer 2.1.6) on 2022-05-10 17:01:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 49] 0.00-10.00 sec  29.4 MBytes  24.7 Mbits/sec   0.587 ms 257/21262 (1.2%) 17.022/6.901/142.684/14.811 ms 2100 pps 181
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 470.40 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*50] local 10.0.23.217%eth0 port 44740 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*50] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec  0/0     2126 pps
[ 50] Sent 21262 datagrams
[ 50] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*50] 0.00-10.03 sec  29.7 MBytes  24.8 Mbits/sec   2.122 ms 101/21261 (0.48%) -/-/-/- ms 2120 pps
[ 51] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53509 (sock=4) (peer 2.1.6) on 2022-05-10 17:01:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 51] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec   0.667 ms 0/22112 (0%) 12.086/7.100/36.356/3.233 ms 2211 pps 269
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 452.31 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*52] local 10.0.23.217%eth0 port 46173 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*52] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec  0/0     2211 pps
[ 52] Sent 22112 datagrams
[ 52] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*52] 0.00-10.02 sec  31.0 MBytes  26.0 Mbits/sec   0.339 ms 0/22111 (0%) -/-/-/- ms 2206 pps
[ 53] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 47128 (sock=3) (peer 2.1.6) on 2022-05-10 17:01:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 53] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec   0.471 ms 0/22963 (0%) 9.248/4.342/26.540/3.097 ms 2297 pps 365
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6660 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 435.56 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*54] local 10.0.23.217%eth0 port 45437 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*54] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec  0/0     2296 pps
[ 54] Sent 22962 datagrams
------------------------------------------------------------
Server listening on UDP port 5001 with pid 6770
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40871 (sock=3) (peer 2.1.6) on 2022-05-10 17:03:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  32.2 MBytes  27.0 Mbits/sec   0.676 ms 0/22962 (0%) 7.806/3.069/40.181/3.739 ms 2293 pps 432
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6770 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 435.56 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 55416 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec  0/0     2296 pps
[  2] Sent 22962 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.07 sec  31.7 MBytes  26.4 Mbits/sec   0.323 ms 365/22961 (1.6%) -/-/-/- ms 2279 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 48179 (sock=5) (peer 2.1.6) on 2022-05-10 17:04:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec   0.337 ms 0/23813 (0%) 13.436/5.790/59.222/5.592 ms 2382 pps 261
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6770 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 420.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 34041 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec  0/0     2381 pps
[  4] Sent 23813 datagrams
------------------------------------------------------------
Server listening on UDP port 5001 with pid 6799
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 44018 (sock=3) (peer 2.1.6) on 2022-05-10 17:05:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.00 sec  32.7 MBytes  27.4 Mbits/sec   0.430 ms 469/23813 (2%) 7.501/2.072/136.555/11.813 ms 2334 pps 457
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6799 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 420.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 50474 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec  0/0     2381 pps
[  2] Sent 23813 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  33.3 MBytes  27.9 Mbits/sec   0.428 ms 67/23812 (0.28%) 34.285/0.570/176.995/0.366 ms 2377 pps 102
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45638 (sock=5) (peer 2.1.6) on 2022-05-10 17:06:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  34.6 MBytes  29.0 Mbits/sec   0.396 ms 0/24663 (0%) 16.505/5.661/46.749/6.246 ms 2465 pps 220
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6799 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 405.52 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 51113 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec  0/0     2466 pps
[  4] Sent 24663 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.00 sec  34.2 MBytes  28.7 Mbits/sec   0.413 ms 240/24662 (0.97%) -/-/-/- ms 2465 pps
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35575 (sock=3) (peer 2.1.6) on 2022-05-10 17:06:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  35.5 MBytes  29.8 Mbits/sec   0.493 ms 208/25513 (0.82%) 18.142/8.040/124.232/12.941 ms 2531 pps 205
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 6799 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 392.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 34623 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec  0/0     2551 pps
[  6] Sent 25513 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.04 sec  34.8 MBytes  29.1 Mbits/sec   0.350 ms 687/25512 (2.7%) -/-/-/- ms 2541 pps
