------------------------------------------------------------
Server listening on UDP port 5001 with pid 4012
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36197 (sock=3) (peer 2.1.6) on 2022-05-13 16:00:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  4.17 MBytes  3.50 Mbits/sec   0.037 ms 2/2980 (0.067%) 1.930/1.745/4.554/0.196 ms 298 pps 227
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 50969 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[  2] Sent 2980 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.036 ms 0/2979 (0%) 2.207/2.098/7.601/0.201 ms 297 pps 198
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35373 (sock=5) (peer 2.1.6) on 2022-05-13 16:00:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.00 sec  4.76 MBytes  3.99 Mbits/sec   0.014 ms 9/3405 (0.26%) 1.449/1.281/5.583/0.256 ms 339 pps 344
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 41698 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  4] Sent 3405 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.048 ms 0/3404 (0%) 2.392/2.114/5.923/0.206 ms 340 pps 209
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55230 (sock=3) (peer 2.1.6) on 2022-05-13 16:01:16 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.025 ms 3/3830 (0.078%) 1.738/1.498/4.503/0.241 ms 383 pps 324
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 41507 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[  6] Sent 3830 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.032 ms 0/3829 (0%) 2.322/2.040/5.027/0.198 ms 382 pps 242
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41164 (sock=4) (peer 2.1.6) on 2022-05-13 16:01:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.014 ms 0/4255 (0%) 1.791/1.608/4.624/0.268 ms 425 pps 349
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 45228 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[  8] Sent 4255 datagrams
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60054 (sock=3) (peer 2.1.6) on 2022-05-13 16:01:57 (CEST)
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.085 ms 0/4254 (0%) 2.213/1.990/6.341/0.196 ms 425 pps 283
[  9] 0.00-10.00 sec  6.55 MBytes  5.49 Mbits/sec   0.147 ms 8/4680 (0.17%) 1.864/1.565/6.071/0.376 ms 467 pps 368
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[SUM] 0.00-20.27 sec  12.5 MBytes  5.18 Mbits/sec  0/0      440 pps
[SUM-2] Sent 8935 datagrams
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 59609 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 10] Sent 4680 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.055 ms 0/4679 (0%) 2.147/1.873/4.935/0.219 ms 467 pps 320
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40875 (sock=5) (peer 2.1.6) on 2022-05-13 16:02:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  7.14 MBytes  5.99 Mbits/sec   0.101 ms 12/5105 (0.24%) 1.860/1.510/6.223/0.476 ms 509 pps 402
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 39672 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.042 ms 0/5104 (0%) 2.108/1.782/5.132/0.261 ms 510 pps 356
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34117 (sock=3) (peer 2.1.6) on 2022-05-13 16:02:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  7.74 MBytes  6.49 Mbits/sec   0.035 ms 13/5531 (0.24%) 2.142/1.665/8.150/0.700 ms 552 pps 379
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 54980 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 14] Sent 5531 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.075 ms 0/5530 (0%) 2.205/1.869/6.696/0.284 ms 552 pps 369
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58754 (sock=4) (peer 2.1.6) on 2022-05-13 16:02:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.04 sec  8.25 MBytes  6.89 Mbits/sec   0.124 ms 74/5957 (1.2%) 25.755/2.098/42.356/9.812 ms 586 pps 33
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 39304 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 16] Sent 5956 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-9.99 sec  8.35 MBytes  7.01 Mbits/sec   0.023 ms 0/5955 (0%) 12.332/6.183/24.448/0.674 ms 596 pps 71
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44122 (sock=3) (peer 2.1.6) on 2022-05-13 16:03:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.04 sec  8.36 MBytes  6.98 Mbits/sec   0.171 ms 421/6381 (6.6%) 39.235/-2.040/49.704/7.140 ms 594 pps 22
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 33010 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 18] Sent 6381 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-9.99 sec  8.94 MBytes  7.51 Mbits/sec   0.028 ms 0/6380 (0%) 17.603/10.320/28.357/0.542 ms 638 pps 53
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53210 (sock=4) (peer 2.1.6) on 2022-05-13 16:03:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.06 sec  8.42 MBytes  7.02 Mbits/sec   0.313 ms 802/6806 (12%) 48.576/-5.960/55.231/7.195 ms 597 pps 18
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 39562 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 20] Sent 6806 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.03 sec  6.41 MBytes  5.36 Mbits/sec   0.054 ms 2235/6805 (33%) -/-/-/- ms 678 pps
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53571 (sock=3) (peer 2.1.6) on 2022-05-13 16:03:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.05 sec  8.37 MBytes  6.99 Mbits/sec   0.427 ms 1258/7232 (17%) 53.985/4.051/59.458/4.824 ms 594 pps 16
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 45298 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 22] Sent 7231 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.04 sec  9.87 MBytes  8.25 Mbits/sec   0.056 ms 190/7230 (2.6%) 40.896/1.279/46.353/0.571 ms 720 pps 25
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60860 (sock=4) (peer 2.1.6) on 2022-05-13 16:04:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.21 sec  7.69 MBytes  6.32 Mbits/sec   4.605 ms 2172/7659 (28%) 67.815/7.834/268.324/17.598 ms 538 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 35030 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 24] Sent 7656 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.03 sec  9.88 MBytes  8.26 Mbits/sec   0.208 ms 606/7655 (7.9%) -/-/-/- ms 762 pps
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52237 (sock=3) (peer 2.1.6) on 2022-05-13 16:04:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.05 sec  8.34 MBytes  6.96 Mbits/sec   0.552 ms 2135/8082 (26%) 78.149/30.247/81.953/3.908 ms 592 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 58189 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 26] Sent 8082 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.04 sec  9.87 MBytes  8.25 Mbits/sec   0.340 ms 1041/8081 (13%) -/-/-/- ms 804 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53582 (sock=4) (peer 2.1.6) on 2022-05-13 16:05:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.05 sec  8.36 MBytes  6.98 Mbits/sec   0.583 ms 2543/8508 (30%) 75.595/24.891/82.972/3.807 ms 593 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4012 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 36964 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 28] Sent 8507 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  9.89 MBytes  8.26 Mbits/sec   0.371 ms 1451/8506 (17%) -/-/-/- ms 846 pps
