------------------------------------------------------------
Server listening on UDP port 5001 with pid 1916
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57685 (sock=3) (peer 2.1.6) on 2022-05-13 12:08:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.036 ms 0/854 (0%) -4.590/-5.100/-3.201/0.330 ms 85 pps -27
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 38728 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.028 ms 0/853 (0%) 8.207/7.823/10.964/0.403 ms 85 pps 15
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36507 (sock=5) (peer 2.1.6) on 2022-05-13 12:08:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.015 ms 0/1279 (0%) -3.158/-3.468/-0.443/0.242 ms 128 pps -59
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 46024 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.039 ms 0/1278 (0%) 7.094/6.666/10.147/0.348 ms 127 pps 26
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39375 (sock=3) (peer 2.1.6) on 2022-05-13 12:08:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.045 ms 0/1704 (0%) -2.213/-2.468/0.377/0.232 ms 170 pps -113
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 53825 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.035 ms 0/1703 (0%) 5.998/5.667/8.788/0.271 ms 170 pps 42
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52535 (sock=4) (peer 2.1.6) on 2022-05-13 12:09:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.043 ms 0/2129 (0%) -1.042/-1.358/3.626/0.273 ms 213 pps -300
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 53999 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.028 ms 0/2128 (0%) 4.884/4.537/7.900/0.259 ms 212 pps 64
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42741 (sock=3) (peer 2.1.6) on 2022-05-13 12:09:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.061 ms 0/2554 (0%) -0.318/-0.509/2.521/0.203 ms 255 pps -1180
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 36080 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.039 ms 0/2553 (0%) 4.326/3.904/7.851/0.292 ms 255 pps 87
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33957 (sock=4) (peer 2.1.6) on 2022-05-13 12:09:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.037 ms 0/2980 (0%) 0.377/0.121/3.300/0.223 ms 298 pps 1160
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 60086 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.209 ms 0/2979 (0%) 3.949/3.648/6.696/0.220 ms 297 pps 111
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35326 (sock=3) (peer 2.1.6) on 2022-05-13 12:10:16 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.013 ms 0/3405 (0%) 0.746/0.594/3.832/0.245 ms 340 pps 671
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 50374 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.125 ms 0/3404 (0%) 3.399/3.057/6.290/0.253 ms 340 pps 147
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38523 (sock=4) (peer 2.1.6) on 2022-05-13 12:10:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.019 ms 0/3830 (0%) 1.215/1.036/4.180/0.289 ms 383 pps 463
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 56635 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.030 ms 0/3829 (0%) 3.061/2.794/7.572/0.241 ms 382 pps 184
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35514 (sock=3) (peer 2.1.6) on 2022-05-13 12:10:57 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.012 ms 0/4255 (0%) 1.443/1.210/5.298/0.404 ms 425 pps 433
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 58278 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.037 ms 0/4254 (0%) 2.882/2.610/6.201/0.275 ms 425 pps 217
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42443 (sock=4) (peer 2.1.6) on 2022-05-13 12:11:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.073 ms 0/4680 (0%) 1.518/1.100/7.280/0.595 ms 468 pps 453
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 54060 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.029 ms 0/4679 (0%) 2.869/2.439/5.928/0.310 ms 467 pps 240
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47196 (sock=3) (peer 2.1.6) on 2022-05-13 12:11:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.020 ms 0/5105 (0%) 2.029/1.297/6.024/0.939 ms 510 pps 370
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 50685 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.033 ms 0/5104 (0%) 2.737/2.315/6.430/0.352 ms 510 pps 274
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48807 (sock=4) (peer 2.1.6) on 2022-05-13 12:11:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.03 sec  7.51 MBytes  6.28 Mbits/sec   0.091 ms 173/5531 (3.1%) 41.039/2.033/58.057/10.375 ms 534 pps 19
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 34957 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.98 sec  7.75 MBytes  6.52 Mbits/sec   0.029 ms 0/5530 (0%) 24.322/14.099/37.942/0.514 ms 553 pps 33
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46061 (sock=3) (peer 2.1.6) on 2022-05-13 12:12:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.02 sec  7.52 MBytes  6.29 Mbits/sec   0.289 ms 596/5957 (10%) 28.553/-9.265/48.919/11.561 ms 535 pps 28
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 51299 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.98 sec  8.35 MBytes  7.02 Mbits/sec   0.033 ms 0/5955 (0%) 45.226/26.463/63.676/0.544 ms 596 pps 19
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60670 (sock=4) (peer 2.1.6) on 2022-05-13 12:12:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.09 sec  7.52 MBytes  6.25 Mbits/sec   0.483 ms 1015/6381 (16%) -/-/-/- ms 532 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 57537 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.00 sec  8.94 MBytes  7.51 Mbits/sec   0.043 ms 0/6380 (0%) -/-/-/- ms 638 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47377 (sock=3) (peer 2.1.6) on 2022-05-13 12:12:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.06 sec  7.54 MBytes  6.29 Mbits/sec   0.661 ms 1429/6807 (21%) 65.142/11.494/69.992/4.527 ms 535 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 52868 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.04 sec  9.02 MBytes  7.53 Mbits/sec   0.145 ms 373/6805 (5.5%) -/-/-/- ms 677 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45493 (sock=4) (peer 2.1.6) on 2022-05-13 12:13:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.08 sec  7.52 MBytes  6.26 Mbits/sec   0.608 ms 1866/7232 (26%) 77.881/12.107/88.871/7.911 ms 532 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 43528 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  9.03 MBytes  7.54 Mbits/sec   0.317 ms 786/7230 (11%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57894 (sock=3) (peer 2.1.6) on 2022-05-13 12:13:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.06 sec  7.51 MBytes  6.27 Mbits/sec   0.630 ms 2296/7656 (30%) 86.947/30.860/88.809/4.411 ms 533 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 57600 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  9.05 MBytes  7.56 Mbits/sec   0.381 ms 1199/7655 (16%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54664 (sock=4) (peer 2.1.6) on 2022-05-13 12:14:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  7.51 MBytes  6.27 Mbits/sec   0.612 ms 2722/8082 (34%) 86.285/29.642/92.187/3.971 ms 533 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 60393 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  9.05 MBytes  7.56 Mbits/sec   0.457 ms 1625/8081 (20%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54337 (sock=3) (peer 2.1.6) on 2022-05-13 12:14:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.06 sec  6.80 MBytes  5.67 Mbits/sec   0.567 ms 3655/8507 (43%) 86.514/29.365/160.047/6.544 ms 482 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1916 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 42460 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  9.05 MBytes  7.56 Mbits/sec   0.508 ms 2054/8506 (24%) -/-/-/- ms 847 pps
