------------------------------------------------------------
Server listening on UDP port 5001 with pid 3593
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50816 (sock=3) (peer 2.1.6) on 2022-05-13 15:00:57 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.012 ms 0/854 (0%) 1.665/1.439/3.580/0.164 ms 85 pps 75
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 59922 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.136 ms 0/853 (0%) 2.589/2.423/4.698/0.177 ms 85 pps 48
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48260 (sock=5) (peer 2.1.6) on 2022-05-13 15:01:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.049 ms 0/1279 (0%) 1.929/1.813/4.727/0.184 ms 128 pps 97
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 37117 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.031 ms 0/1278 (0%) 2.454/2.325/5.964/0.215 ms 127 pps 76
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42526 (sock=3) (peer 2.1.6) on 2022-05-13 15:01:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.018 ms 0/1704 (0%) 2.002/1.733/4.991/0.201 ms 170 pps 125
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 43537 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.233 ms 0/1703 (0%) 2.559/2.347/5.203/0.184 ms 170 pps 98
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54332 (sock=4) (peer 2.1.6) on 2022-05-13 15:01:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.021 ms 0/2129 (0%) 1.917/1.788/4.716/0.184 ms 213 pps 163
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 34241 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.040 ms 0/2128 (0%) 2.426/2.220/5.407/0.166 ms 212 pps 129
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33873 (sock=3) (peer 2.1.6) on 2022-05-13 15:02:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.013 ms 0/2554 (0%) 1.891/1.739/4.865/0.196 ms 255 pps 199
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 36047 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.039 ms 0/2553 (0%) 2.514/2.242/5.423/0.211 ms 255 pps 149
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36200 (sock=4) (peer 2.1.6) on 2022-05-13 15:02:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.085 ms 0/2980 (0%) 2.010/1.836/4.783/0.206 ms 298 pps 218
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 53491 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.031 ms 0/2979 (0%) 2.343/2.112/5.358/0.195 ms 297 pps 187
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46901 (sock=3) (peer 2.1.6) on 2022-05-13 15:03:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.167 ms 0/3405 (0%) 2.109/1.924/7.538/0.270 ms 340 pps 237
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 49120 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.020 ms 0/3404 (0%) 2.306/2.051/5.311/0.203 ms 340 pps 217
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41173 (sock=4) (peer 2.1.6) on 2022-05-13 15:03:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.183 ms 0/3830 (0%) 2.138/1.916/5.288/0.294 ms 383 pps 263
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 37991 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.033 ms 0/3829 (0%) 2.226/2.019/5.200/0.226 ms 382 pps 253
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60901 (sock=3) (peer 2.1.6) on 2022-05-13 15:03:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.058 ms 0/4255 (0%) 2.068/1.768/7.262/0.446 ms 425 pps 302
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 45402 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.299 ms 0/4254 (0%) 2.221/1.867/7.574/0.315 ms 425 pps 282
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55647 (sock=4) (peer 2.1.6) on 2022-05-13 15:04:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.045 ms 0/4680 (0%) 2.405/2.058/10.613/0.582 ms 468 pps 286
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 44320 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.074 ms 0/4679 (0%) 1.982/1.706/5.028/0.260 ms 467 pps 347
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59749 (sock=3) (peer 2.1.6) on 2022-05-13 15:04:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.04 sec  5.99 MBytes  5.01 Mbits/sec   0.090 ms 829/5105 (16%) 20.515/2.074/1688.389/153.913 ms 426 pps 31
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 41585 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.049 ms 0/5104 (0%) 2.059/1.726/8.261/0.336 ms 510 pps 364
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41438 (sock=4) (peer 2.1.6) on 2022-05-13 15:04:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.03 sec  7.51 MBytes  6.28 Mbits/sec   0.116 ms 175/5531 (3.2%) 40.505/2.628/58.530/11.048 ms 534 pps 19
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 58882 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.99 sec  7.75 MBytes  6.51 Mbits/sec   0.027 ms 0/5530 (0%) 38.545/25.630/53.295/0.149 ms 553 pps 21
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41837 (sock=3) (peer 2.1.6) on 2022-05-13 15:05:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.09 sec  7.52 MBytes  6.26 Mbits/sec   0.339 ms 590/5956 (9.9%) -/-/-/- ms 532 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 53427 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   0.031 ms 0/5955 (0%) -/-/-/- ms 595 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56338 (sock=4) (peer 2.1.6) on 2022-05-13 15:05:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  7.52 MBytes  6.27 Mbits/sec   0.482 ms 1016/6381 (16%) 61.150/5.564/63.526/5.733 ms 533 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 51970 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec   0.071 ms 0/6380 (0%) -/-/-/- ms 638 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59761 (sock=3) (peer 2.1.6) on 2022-05-13 15:05:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.06 sec  7.54 MBytes  6.29 Mbits/sec   0.569 ms 1428/6807 (21%) 61.334/4.607/66.955/5.033 ms 535 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 37813 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.04 sec  9.03 MBytes  7.54 Mbits/sec   0.184 ms 366/6805 (5.4%) 44.250/2.039/48.821/0.711 ms 677 pps 21
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54026 (sock=4) (peer 2.1.6) on 2022-05-13 15:06:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.05 sec  7.51 MBytes  6.27 Mbits/sec   0.640 ms 1871/7231 (26%) 61.577/8.702/85.852/4.838 ms 533 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 49316 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.03 sec  9.01 MBytes  7.54 Mbits/sec   0.283 ms 802/7230 (11%) 39.767/8.204/50.729/0.799 ms 721 pps 24
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36672 (sock=3) (peer 2.1.6) on 2022-05-13 15:06:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  7.51 MBytes  6.26 Mbits/sec   0.639 ms 2296/7656 (30%) 81.244/19.184/107.522/5.974 ms 532 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 46496 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  9.03 MBytes  7.54 Mbits/sec   0.402 ms 1217/7655 (16%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55520 (sock=4) (peer 2.1.6) on 2022-05-13 15:06:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  7.52 MBytes  6.27 Mbits/sec   0.621 ms 2716/8082 (34%) 86.186/29.881/89.760/3.942 ms 533 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 39443 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  9.05 MBytes  7.56 Mbits/sec   0.444 ms 1627/8082 (20%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39278 (sock=3) (peer 2.1.6) on 2022-05-13 15:07:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.06 sec  7.53 MBytes  6.28 Mbits/sec   0.577 ms 3137/8507 (37%) 85.650/28.611/90.726/4.085 ms 534 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3593 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 60109 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  9.01 MBytes  7.53 Mbits/sec   0.540 ms 2078/8506 (24%) -/-/-/- ms 846 pps
------------------------------------------------------------
Server listening on UDP port 5001 with pid 3650
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
