------------------------------------------------------------
Server listening on UDP port 5001 with pid 1728
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38312 (sock=3) (peer 2.1.6) on 2022-05-13 11:40:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.112 ms 0/854 (0%) -0.682/-1.142/2.549/0.296 ms 85 pps -184
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 42299 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.242 ms 0/853 (0%) 5.144/4.869/6.647/0.236 ms 85 pps 24
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57476 (sock=5) (peer 2.1.6) on 2022-05-13 11:40:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.058 ms 0/1279 (0%) 0.117/-0.052/3.199/0.189 ms 128 pps 1607
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 44740 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.038 ms 0/1278 (0%) 4.645/4.334/10.031/0.294 ms 127 pps 40
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41093 (sock=3) (peer 2.1.6) on 2022-05-13 11:41:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.062 ms 0/1704 (0%) 0.492/0.271/3.803/0.220 ms 170 pps 509
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 53215 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.025 ms 0/1703 (0%) 4.117/3.745/7.341/0.285 ms 170 pps 61
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56679 (sock=4) (peer 2.1.6) on 2022-05-13 11:41:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.007 ms 0/2129 (0%) 1.070/0.875/4.247/0.234 ms 213 pps 292
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 50145 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.063 ms 0/2128 (0%) 3.820/3.539/7.204/0.214 ms 212 pps 82
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57166 (sock=3) (peer 2.1.6) on 2022-05-13 11:41:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.012 ms 0/2554 (0%) 1.135/0.861/4.824/0.267 ms 255 pps 331
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 47185 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.032 ms 0/2553 (0%) 3.721/3.340/7.076/0.280 ms 255 pps 101
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50796 (sock=4) (peer 2.1.6) on 2022-05-13 11:42:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.010 ms 0/2980 (0%) 1.383/1.139/4.192/0.292 ms 298 pps 316
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 57539 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.205 ms 0/2979 (0%) 3.365/3.027/6.622/0.278 ms 297 pps 130
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60307 (sock=3) (peer 2.1.6) on 2022-05-13 11:42:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.046 ms 0/3405 (0%) 1.640/1.329/5.020/0.389 ms 340 pps 305
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 47879 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.064 ms 0/3404 (0%) 3.198/2.785/8.738/0.318 ms 340 pps 156
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48193 (sock=4) (peer 2.1.6) on 2022-05-13 11:42:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.045 ms 0/3830 (0%) 2.047/1.716/5.704/0.542 ms 383 pps 275
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 52715 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.032 ms 0/3829 (0%) 2.881/2.528/7.768/0.341 ms 382 pps 195
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41829 (sock=3) (peer 2.1.6) on 2022-05-13 11:43:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.03 sec  5.00 MBytes  4.18 Mbits/sec   0.147 ms 686/4255 (16%) 23.298/2.056/1688.899/165.338 ms 356 pps 22
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 60338 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.049 ms 0/4254 (0%) 2.755/2.384/6.514/0.391 ms 425 pps 227
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35903 (sock=4) (peer 2.1.6) on 2022-05-13 11:43:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.04 sec  6.37 MBytes  5.32 Mbits/sec   0.083 ms 137/4681 (2.9%) 48.458/2.476/67.530/12.431 ms 453 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 60323 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.98 sec  6.56 MBytes  5.51 Mbits/sec   0.029 ms 0/4679 (0%) 27.351/15.758/43.170/0.592 ms 468 pps 25
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46110 (sock=3) (peer 2.1.6) on 2022-05-13 11:43:57 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.09 sec  6.38 MBytes  5.31 Mbits/sec   0.405 ms 553/5105 (11%) -/-/-/- ms 451 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 56615 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.031 ms 0/5104 (0%) -/-/-/- ms 510 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39446 (sock=4) (peer 2.1.6) on 2022-05-13 11:44:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.07 sec  6.38 MBytes  5.31 Mbits/sec   0.589 ms 981/5531 (18%) 71.352/5.704/74.665/6.439 ms 452 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 34936 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-11.34 sec  7.48 MBytes  5.54 Mbits/sec  30.605 ms 243/5580 (4.4%) 14.251/0.178/1686.688/0.563 ms 492 pps 49
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44764 (sock=3) (peer 2.1.6) on 2022-05-13 11:44:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.707 ms 1403/5956 (24%) 71.245/4.785/74.250/6.319 ms 452 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 42514 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.05 sec  7.85 MBytes  6.56 Mbits/sec   0.253 ms 353/5955 (5.9%) 51.590/2.958/60.551/0.665 ms 592 pps 16
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39993 (sock=4) (peer 2.1.6) on 2022-05-13 11:44:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.09 sec  6.38 MBytes  5.30 Mbits/sec   0.757 ms 1832/6381 (29%) 88.794/11.651/100.894/9.289 ms 451 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 40447 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.410 ms 774/6380 (12%) -/-/-/- ms 634 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47487 (sock=3) (peer 2.1.6) on 2022-05-13 11:45:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.07 sec  6.41 MBytes  5.34 Mbits/sec   0.810 ms 2233/6807 (33%) 98.991/32.815/102.293/5.197 ms 454 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 52151 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.522 ms 1200/6805 (18%) -/-/-/- ms 676 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36303 (sock=4) (peer 2.1.6) on 2022-05-13 11:45:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.07 sec  6.38 MBytes  5.31 Mbits/sec   0.657 ms 2681/7231 (37%) 98.674/31.943/100.620/5.156 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 51189 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.546 ms 1626/7231 (22%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36982 (sock=3) (peer 2.1.6) on 2022-05-13 11:46:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.564 ms 3101/7656 (41%) 98.526/31.670/105.291/4.934 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 34605 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  7.88 MBytes  6.57 Mbits/sec   0.580 ms 2036/7656 (27%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54341 (sock=4) (peer 2.1.6) on 2022-05-13 11:46:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  6.38 MBytes  5.32 Mbits/sec   0.664 ms 3529/8083 (44%) 92.370/31.474/99.464/5.300 ms 453 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 51403 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  7.87 MBytes  6.57 Mbits/sec   0.611 ms 2464/8081 (30%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46846 (sock=3) (peer 2.1.6) on 2022-05-13 11:46:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.08 sec  6.38 MBytes  5.31 Mbits/sec   0.248 ms 3956/8507 (47%) 95.761/25.136/100.279/5.210 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1728 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 55143 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  7.89 MBytes  6.58 Mbits/sec   0.585 ms 2879/8506 (34%) -/-/-/- ms 846 pps
