------------------------------------------------------------
Server listening on UDP port 5001 with pid 2194
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 39467 (sock=3) (peer 2.1.6) on 2022-05-04 12:46:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  1.19 MBytes  0.997 Mbits/sec   3.103 ms 5/854 (0.59%) 17.322/5.049/104.666/18.259 ms 85 pps 7
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2194 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 33660 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.05 sec  1.20 MBytes  0.998 Mbits/sec  12.640 ms 0/853 (0%) 30.942/2.288/80.743/2.212 ms 84 pps 4
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35131 (sock=5) (peer 2.1.6) on 2022-05-04 12:46:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.02 sec  2.39 MBytes  2.00 Mbits/sec   1.100 ms 0/1704 (0%) -/-/-/- ms 170 pps
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2194 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 41991 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   3.864 ms 0/1703 (0%) 20.575/7.761/64.225/1.582 ms 170 pps 12
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 50706 (sock=3) (peer 2.1.6) on 2022-05-04 12:47:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  3.58 MBytes  3.00 Mbits/sec   1.746 ms 1/2554 (0.039%) -/-/-/- ms 255 pps
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2194 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 41044 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  3.57 MBytes  2.99 Mbits/sec   1.434 ms 6/2553 (0.24%) 51.417/9.013/88.203/1.244 ms 255 pps 7
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35392 (sock=4) (peer 2.1.6) on 2022-05-04 12:47:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.05 sec  4.73 MBytes  3.95 Mbits/sec   1.635 ms 32/3405 (0.94%) -/-/-/- ms 336 pps
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2194 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 48742 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval       Transfer     Bandwidth        Jitter   Lost/Total Datagrams
[ *8] 0.00-943272827.22 sec  3311740859203 MBytes  29452 Mbits/sec  943272827216.501 ms 909588537/875902519 (1e+02%)
[ *8] 0.00-943272827.22 sec  808530483 datagrams received out-of-order
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 37840 (sock=3) (peer 2.1.6) on 2022-05-04 12:47:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.15 sec  5.03 MBytes  4.16 Mbits/sec   1.433 ms 669/4255 (16%) -/-/-/- ms 353 pps
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2194 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 56937 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.04 sec  4.72 MBytes  3.94 Mbits/sec   1.019 ms 887/4254 (21%) 118.349/73.760/163.947/0.400 ms 423 pps 4
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 48704 (sock=4) (peer 2.1.6) on 2022-05-04 12:48:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.98 MBytes  4.17 Mbits/sec   1.119 ms 1554/5105 (30%) 35.003/22.206/67.414/5.566 ms 355 pps 15
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2194 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 56067 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.20 sec  4.78 MBytes  3.93 Mbits/sec   1.362 ms 1691/5104 (33%) 149.150/1.038/247.884/1.097 ms 500 pps 3
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 47127 (sock=3) (peer 2.1.6) on 2022-05-04 12:49:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.14 sec  5.33 MBytes  4.41 Mbits/sec   1.352 ms 2153/5956 (36%) -/-/-/- ms 375 pps
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2194 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 51818 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.09 sec  4.95 MBytes  4.11 Mbits/sec   2.204 ms 2427/5955 (41%) 140.594/66.585/303.864/0.907 ms 590 pps 4
