------------------------------------------------------------
Server listening on UDP port 5001 with pid 1491
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 32990 (sock=3) (peer 2.1.6) on 2022-05-13 11:06:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.021 ms 0/854 (0%) 2.021/1.792/4.844/0.262 ms 85 pps 62
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 59716 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.067 ms 0/853 (0%) 2.363/2.198/3.546/0.140 ms 85 pps 53
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55006 (sock=5) (peer 2.1.6) on 2022-05-13 11:06:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.038 ms 0/1279 (0%) 2.074/1.916/4.683/0.180 ms 128 pps 91
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 50149 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.033 ms 0/1278 (0%) 2.301/2.117/7.635/0.226 ms 127 pps 82
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44844 (sock=3) (peer 2.1.6) on 2022-05-13 11:06:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.013 ms 0/1704 (0%) 2.143/1.947/5.163/0.219 ms 170 pps 117
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 53473 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.053 ms 0/1703 (0%) 2.275/2.108/5.225/0.190 ms 170 pps 110
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44256 (sock=4) (peer 2.1.6) on 2022-05-13 11:07:16 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.046 ms 0/2129 (0%) 2.176/2.028/5.121/0.178 ms 213 pps 144
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 36527 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.029 ms 0/2128 (0%) 2.242/2.026/5.378/0.166 ms 212 pps 139
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39635 (sock=3) (peer 2.1.6) on 2022-05-13 11:07:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.036 ms 0/2554 (0%) 2.094/1.942/5.114/0.189 ms 255 pps 179
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 56347 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.033 ms 0/2553 (0%) 2.274/1.997/5.347/0.212 ms 255 pps 165
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43520 (sock=4) (peer 2.1.6) on 2022-05-13 11:07:57 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.067 ms 0/2980 (0%) 2.217/1.982/7.992/0.264 ms 298 pps 198
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 42981 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.026 ms 0/2979 (0%) 2.138/1.944/5.286/0.207 ms 297 pps 205
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51287 (sock=3) (peer 2.1.6) on 2022-05-13 11:08:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.211 ms 0/3405 (0%) 2.240/2.026/5.850/0.283 ms 340 pps 223
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 52220 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.030 ms 0/3404 (0%) 2.155/1.905/5.102/0.216 ms 340 pps 232
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43747 (sock=4) (peer 2.1.6) on 2022-05-13 11:08:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.043 ms 0/3830 (0%) 2.280/2.071/5.002/0.300 ms 383 pps 247
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 38909 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.033 ms 0/3829 (0%) 2.124/1.915/5.956/0.222 ms 382 pps 265
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38323 (sock=3) (peer 2.1.6) on 2022-05-13 11:08:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.060 ms 0/4255 (0%) 2.146/1.871/6.892/0.395 ms 425 pps 291
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 34438 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.044 ms 0/4254 (0%) 2.159/1.837/5.412/0.268 ms 425 pps 290
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52450 (sock=4) (peer 2.1.6) on 2022-05-13 11:09:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.017 ms 0/4680 (0%) 2.237/1.819/6.232/0.558 ms 468 pps 308
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 34816 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.183 ms 0/4679 (0%) 2.286/1.908/5.293/0.310 ms 467 pps 301
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38789 (sock=3) (peer 2.1.6) on 2022-05-13 11:09:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.152 ms 0/5105 (0%) 2.505/1.813/6.417/0.889 ms 510 pps 300
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 48208 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.172 ms 0/5104 (0%) 2.257/1.826/6.296/0.344 ms 510 pps 332
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35799 (sock=4) (peer 2.1.6) on 2022-05-13 11:10:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.03 sec  7.51 MBytes  6.28 Mbits/sec   0.103 ms 173/5531 (3.1%) 42.155/2.517/60.597/10.266 ms 534 pps 19
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 37853 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.98 sec  7.75 MBytes  6.52 Mbits/sec   0.045 ms 0/5530 (0%) 22.299/12.622/35.602/0.256 ms 554 pps 37
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58725 (sock=3) (peer 2.1.6) on 2022-05-13 11:10:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.07 sec  7.51 MBytes  6.26 Mbits/sec   0.304 ms 598/5957 (10%) 54.232/-8.290/63.300/8.790 ms 532 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 53837 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   0.044 ms 0/5955 (0%) -/-/-/- ms 595 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53135 (sock=4) (peer 2.1.6) on 2022-05-13 11:10:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  7.52 MBytes  6.27 Mbits/sec   0.455 ms 1016/6382 (16%) 60.715/5.014/62.917/5.688 ms 533 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 59986 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  7.47 MBytes  6.25 Mbits/sec   0.036 ms 1048/6380 (16%) 50.960/0.223/1691.265/0.254 ms 635 pps 15
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42337 (sock=3) (peer 2.1.6) on 2022-05-13 11:11:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.07 sec  6.81 MBytes  5.67 Mbits/sec   0.580 ms 1949/6806 (29%) 72.058/7.451/164.564/10.565 ms 482 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 48274 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.05 sec  9.03 MBytes  7.54 Mbits/sec   0.150 ms 368/6806 (5.4%) -/-/-/- ms 677 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33981 (sock=4) (peer 2.1.6) on 2022-05-13 11:11:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.06 sec  7.52 MBytes  6.27 Mbits/sec   0.646 ms 1864/7231 (26%) 81.474/23.977/84.218/4.922 ms 533 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 53738 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.04 sec  9.04 MBytes  7.55 Mbits/sec   0.300 ms 783/7230 (11%) -/-/-/- ms 720 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47687 (sock=3) (peer 2.1.6) on 2022-05-13 11:11:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.04 sec  7.53 MBytes  6.29 Mbits/sec   0.642 ms 2289/7657 (30%) 72.667/27.548/85.129/7.277 ms 535 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 57807 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.04 sec  9.02 MBytes  7.54 Mbits/sec   0.424 ms 1220/7655 (16%) 49.191/3.194/58.089/0.410 ms 762 pps 19
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36232 (sock=4) (peer 2.1.6) on 2022-05-13 11:12:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.08 sec  7.53 MBytes  6.26 Mbits/sec   0.627 ms 2715/8083 (34%) 77.257/11.169/88.302/7.357 ms 533 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 35222 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.03 sec  9.04 MBytes  7.56 Mbits/sec   0.458 ms 1635/8081 (20%) -/-/-/- ms 805 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35394 (sock=3) (peer 2.1.6) on 2022-05-13 11:12:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.08 sec  7.53 MBytes  6.27 Mbits/sec   0.572 ms 3135/8508 (37%) 114.667/48.521/125.501/7.321 ms 533 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1491 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 43781 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.06 sec  9.04 MBytes  7.54 Mbits/sec   0.493 ms 2057/8506 (24%) -/-/-/- ms 845 pps
