------------------------------------------------------------
Server listening on UDP port 5001 with pid 1441
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56713 (sock=3) (peer 2.1.6) on 2022-05-13 10:57:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.022 ms 0/854 (0%) 1.456/1.277/3.788/0.157 ms 85 pps 86
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 49695 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.094 ms 0/853 (0%) 2.496/2.347/4.442/0.160 ms 85 pps 50
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60409 (sock=5) (peer 2.1.6) on 2022-05-13 10:57:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.055 ms 0/1704 (0%) 1.587/1.425/4.242/0.181 ms 170 pps 158
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 60379 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.040 ms 0/1703 (0%) 2.470/2.274/5.246/0.167 ms 170 pps 101
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51631 (sock=3) (peer 2.1.6) on 2022-05-13 10:57:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.012 ms 0/2554 (0%) 1.645/1.493/4.409/0.162 ms 255 pps 228
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 41773 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.019 ms 0/2553 (0%) 2.406/2.198/6.958/0.180 ms 255 pps 156
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33125 (sock=4) (peer 2.1.6) on 2022-05-13 10:58:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.131 ms 0/3405 (0%) 1.598/1.456/4.446/0.192 ms 340 pps 313
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 34597 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.019 ms 0/3404 (0%) 2.381/2.145/5.117/0.171 ms 340 pps 210
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52203 (sock=3) (peer 2.1.6) on 2022-05-13 10:58:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.025 ms 0/4255 (0%) 1.731/1.562/4.388/0.254 ms 425 pps 361
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 38587 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.082 ms 0/4254 (0%) 2.209/2.042/5.133/0.182 ms 425 pps 283
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33349 (sock=4) (peer 2.1.6) on 2022-05-13 10:58:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.071 ms 0/5105 (0%) 1.826/1.561/4.942/0.430 ms 510 pps 411
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 56322 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.034 ms 0/5104 (0%) 2.300/2.013/8.847/0.276 ms 510 pps 326
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59415 (sock=3) (peer 2.1.6) on 2022-05-13 10:59:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.03 sec  8.35 MBytes  6.98 Mbits/sec   0.033 ms 2/5956 (0.034%) 25.421/2.014/39.071/9.851 ms 593 pps 34
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 48727 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-9.99 sec  8.35 MBytes  7.01 Mbits/sec   0.020 ms 0/5955 (0%) 12.344/6.767/23.950/0.821 ms 596 pps 71
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38410 (sock=4) (peer 2.1.6) on 2022-05-13 10:59:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.05 sec  8.45 MBytes  7.05 Mbits/sec   0.303 ms 781/6806 (11%) 44.477/-2.447/48.645/5.106 ms 600 pps 20
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 57502 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 16] Sent 6806 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.16 sec  8.00 MBytes  6.60 Mbits/sec  70.381 ms 1111/6817 (16%) 22.403/5.846/1795.183/0.293 ms 670 pps 37
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49469 (sock=3) (peer 2.1.6) on 2022-05-13 10:59:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.06 sec  8.41 MBytes  7.01 Mbits/sec   0.671 ms 1661/7657 (22%) 52.312/-0.805/58.925/4.410 ms 596 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 38971 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 18] Sent 7656 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.04 sec  9.88 MBytes  8.25 Mbits/sec   0.181 ms 608/7655 (7.9%) 40.732/0.989/45.484/0.388 ms 762 pps 25
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36590 (sock=4) (peer 2.1.6) on 2022-05-13 11:00:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.06 sec  8.40 MBytes  7.00 Mbits/sec   0.584 ms 2518/8507 (30%) 60.448/5.537/65.726/4.899 ms 595 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 40332 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 20] Sent 8507 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.04 sec  9.89 MBytes  8.26 Mbits/sec   0.405 ms 1454/8506 (17%) -/-/-/- ms 847 pps
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59043 (sock=3) (peer 2.1.6) on 2022-05-13 11:00:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.06 sec  8.41 MBytes  7.01 Mbits/sec   0.518 ms 3361/9357 (36%) 73.912/21.011/77.188/3.767 ms 596 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1069.09 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 58658 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec  0/0      936 pps
[ 22] Sent 9357 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.04 sec  9.90 MBytes  8.27 Mbits/sec   0.464 ms 2292/9356 (24%) -/-/-/- ms 931 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59083 (sock=4) (peer 2.1.6) on 2022-05-13 11:00:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.05 sec  8.46 MBytes  7.06 Mbits/sec   0.410 ms 4173/10207 (41%) 75.577/25.369/77.515/3.234 ms 600 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 980.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 34944 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec  0/0     1021 pps
[ 24] Sent 10207 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.04 sec  9.90 MBytes  8.27 Mbits/sec   0.495 ms 3147/10206 (31%) -/-/-/- ms 1016 pps
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35094 (sock=3) (peer 2.1.6) on 2022-05-13 11:01:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.05 sec  8.41 MBytes  7.02 Mbits/sec   0.219 ms 5060/11058 (46%) 75.752/24.643/77.516/3.147 ms 597 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 904.62 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 47014 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec  0/0     1106 pps
[ 26] Sent 11058 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.04 sec  9.91 MBytes  8.28 Mbits/sec   0.487 ms 3988/11057 (36%) -/-/-/- ms 1100 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35363 (sock=4) (peer 2.1.6) on 2022-05-13 11:01:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.05 sec  8.41 MBytes  7.02 Mbits/sec   0.067 ms 5910/11909 (50%) 75.901/24.908/77.261/3.039 ms 597 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 55937 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec  0/0     1191 pps
[ 28] Sent 11908 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  9.90 MBytes  8.27 Mbits/sec   0.365 ms 4842/11907 (41%) -/-/-/- ms 1185 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49645 (sock=3) (peer 2.1.6) on 2022-05-13 11:01:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.05 sec  8.41 MBytes  7.02 Mbits/sec   0.211 ms 6758/12759 (53%) 75.865/24.874/77.616/2.930 ms 597 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1441 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 45015 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[ 30] Sent 12758 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.04 sec  9.90 MBytes  8.27 Mbits/sec   0.257 ms 5694/12758 (45%) -/-/-/- ms 1270 pps
------------------------------------------------------------
Server listening on UDP port 5001 with pid 1548
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41658 (sock=3) (peer 2.1.6) on 2022-05-13 11:15:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.116 ms 0/854 (0%) -0.503/-0.845/2.009/0.233 ms 85 pps -249
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 51763 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.025 ms 0/853 (0%) 4.213/3.947/6.907/0.263 ms 85 pps 30
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51472 (sock=5) (peer 2.1.6) on 2022-05-13 11:15:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.016 ms 0/1279 (0%) 0.083/-0.054/2.264/0.151 ms 128 pps 2274
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 36023 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.036 ms 0/1278 (0%) 3.837/3.576/6.430/0.200 ms 127 pps 49
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37772 (sock=3) (peer 2.1.6) on 2022-05-13 11:16:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.210 ms 0/1704 (0%) 0.452/0.269/3.179/0.176 ms 170 pps 553
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 39188 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.036 ms 0/1703 (0%) 3.358/3.153/5.865/0.174 ms 170 pps 75
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57488 (sock=4) (peer 2.1.6) on 2022-05-13 11:16:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.016 ms 0/2129 (0%) 0.774/0.667/3.422/0.152 ms 213 pps 404
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 33218 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.051 ms 0/2128 (0%) 3.119/2.906/5.695/0.169 ms 212 pps 100
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58996 (sock=3) (peer 2.1.6) on 2022-05-13 11:16:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.118 ms 0/2554 (0%) 1.025/0.839/4.145/0.202 ms 255 pps 366
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 32965 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.022 ms 0/2553 (0%) 2.777/2.539/5.591/0.185 ms 255 pps 135
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37462 (sock=4) (peer 2.1.6) on 2022-05-13 11:17:05 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.014 ms 0/2980 (0%) 1.242/1.048/6.651/0.228 ms 298 pps 352
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 40072 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.041 ms 0/2979 (0%) 2.791/2.536/5.278/0.182 ms 297 pps 157
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48505 (sock=3) (peer 2.1.6) on 2022-05-13 11:17:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.023 ms 0/3405 (0%) 1.302/1.113/4.089/0.207 ms 340 pps 384
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 44147 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.023 ms 0/3404 (0%) 2.723/2.429/5.451/0.194 ms 340 pps 184
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57832 (sock=4) (peer 2.1.6) on 2022-05-13 11:17:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.008 ms 0/3830 (0%) 1.438/1.267/7.997/0.287 ms 383 pps 391
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 43765 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.135 ms 0/3829 (0%) 2.421/2.185/7.045/0.251 ms 382 pps 232
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56899 (sock=3) (peer 2.1.6) on 2022-05-13 11:18:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.010 ms 0/4255 (0%) 1.670/1.458/4.486/0.275 ms 425 pps 375
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 60602 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.034 ms 0/4254 (0%) 2.343/2.147/5.464/0.196 ms 425 pps 267
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41896 (sock=4) (peer 2.1.6) on 2022-05-13 11:18:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.165 ms 0/4680 (0%) 1.719/1.454/4.665/0.326 ms 468 pps 400
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 40176 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.042 ms 0/4679 (0%) 2.315/2.087/5.236/0.207 ms 467 pps 297
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33680 (sock=3) (peer 2.1.6) on 2022-05-13 11:18:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.056 ms 0/5105 (0%) 1.810/1.542/6.988/0.475 ms 510 pps 415
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 53098 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36078 (sock=4) (peer 2.1.6) on 2022-05-13 11:19:08 (CEST)
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.131 ms 0/5104 (0%) 2.165/1.826/6.828/0.289 ms 510 pps 346
[ 23] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.032 ms 0/5531 (0%) 2.269/1.853/5.761/0.610 ms 553 pps 358
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[SUM] 0.00-20.27 sec  14.9 MBytes  6.17 Mbits/sec  0/0      525 pps
[SUM-2] Sent 10636 datagrams
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 58803 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.060 ms 0/5530 (0%) 1.978/1.708/4.802/0.255 ms 552 pps 411
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36179 (sock=5) (peer 2.1.6) on 2022-05-13 11:19:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.03 sec  8.35 MBytes  6.98 Mbits/sec   0.034 ms 2/5956 (0.034%) 25.576/2.283/39.528/9.956 ms 593 pps 34
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 53292 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.99 sec  8.35 MBytes  7.01 Mbits/sec   0.036 ms 0/5955 (0%) 12.891/6.761/24.704/0.261 ms 596 pps 68
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44859 (sock=3) (peer 2.1.6) on 2022-05-13 11:19:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.03 sec  8.39 MBytes  7.02 Mbits/sec   0.171 ms 395/6381 (6.2%) 34.718/-2.535/48.818/8.473 ms 597 pps 25
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 45691 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-9.99 sec  8.94 MBytes  7.51 Mbits/sec   0.119 ms 0/6380 (0%) 31.872/20.333/44.274/0.470 ms 638 pps 29
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42942 (sock=4) (peer 2.1.6) on 2022-05-13 11:20:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.07 sec  8.45 MBytes  7.04 Mbits/sec   0.332 ms 776/6806 (11%) -/-/-/- ms 599 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 34750 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   0.062 ms 0/6805 (0%) 12.185/5.261/20.629/0.459 ms 680 pps 82
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58128 (sock=3) (peer 2.1.6) on 2022-05-13 11:20:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.06 sec  8.41 MBytes  7.01 Mbits/sec   0.436 ms 1233/7231 (17%) 50.192/-5.445/56.812/6.264 ms 596 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 41023 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.03 sec  9.87 MBytes  8.25 Mbits/sec   0.067 ms 191/7230 (2.6%) 35.617/4.344/41.923/0.581 ms 720 pps 29
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39944 (sock=4) (peer 2.1.6) on 2022-05-13 11:20:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  8.40 MBytes  7.00 Mbits/sec   0.516 ms 1663/7656 (22%) 71.137/14.218/78.644/6.165 ms 595 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 59815 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.04 sec  9.87 MBytes  8.24 Mbits/sec   0.205 ms 615/7655 (8%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59118 (sock=3) (peer 2.1.6) on 2022-05-13 11:21:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.05 sec  8.40 MBytes  7.01 Mbits/sec   0.541 ms 2088/8083 (26%) 77.348/27.059/79.587/4.007 ms 596 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 57552 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  9.89 MBytes  8.26 Mbits/sec   0.331 ms 1026/8081 (13%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58458 (sock=4) (peer 2.1.6) on 2022-05-13 11:21:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.05 sec  8.40 MBytes  7.01 Mbits/sec   0.573 ms 2515/8508 (30%) 76.968/26.350/78.669/3.805 ms 596 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1548 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 46758 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  9.88 MBytes  8.25 Mbits/sec   0.406 ms 1457/8506 (17%) -/-/-/- ms 846 pps
