------------------------------------------------------------
Server listening on UDP port 5001 with pid 1970
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 43833 (sock=3) (peer 2.1.6) on 2022-05-04 12:26:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  1.20 MBytes  1.00 Mbits/sec   4.154 ms 0/854 (0%) 7.802/3.890/42.598/5.019 ms 85 pps 16
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 35368 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.03 sec  1.20 MBytes  1.00 Mbits/sec   6.031 ms 0/853 (0%) -/-/-/- ms 85 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40597 (sock=5) (peer 2.1.6) on 2022-05-04 12:26:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.00 sec  2.39 MBytes  2.00 Mbits/sec   1.828 ms 0/1704 (0%) 4.800/2.283/27.818/2.841 ms 170 pps 52
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 48439 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   6.209 ms 0/1703 (0%) 8.920/0.325/63.840/0.746 ms 170 pps 28
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46107 (sock=3) (peer 2.1.6) on 2022-05-04 12:27:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.548 ms 0/2554 (0%) 3.934/1.344/26.209/3.106 ms 255 pps 95
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 35213 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  3.58 MBytes  3.00 Mbits/sec   4.969 ms 0/2553 (0%) 10.653/0.552/67.822/0.816 ms 254 pps 35
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58193 (sock=4) (peer 2.1.6) on 2022-05-04 12:27:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   1.554 ms 0/3405 (0%) 3.479/1.078/21.562/2.712 ms 340 pps 144
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 46184 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-9.99 sec  4.77 MBytes  4.01 Mbits/sec   4.118 ms 0/3404 (0%) 13.022/0.661/70.714/0.697 ms 340 pps 38
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40540 (sock=3) (peer 2.1.6) on 2022-05-04 12:27:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.02 sec  5.97 MBytes  5.00 Mbits/sec   1.957 ms 0/4255 (0%) 5.220/1.967/27.347/2.802 ms 425 pps 120
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 38341 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.02 sec  5.96 MBytes  4.99 Mbits/sec   3.830 ms 0/4254 (0%) -/-/-/- ms 424 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53776 (sock=4) (peer 2.1.6) on 2022-05-04 12:28:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   1.037 ms 0/5105 (0%) 9.208/4.488/32.817/3.556 ms 510 pps 81
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 49895 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-9.98 sec  7.16 MBytes  6.01 Mbits/sec   2.446 ms 0/5104 (0%) -/-/-/- ms 511 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 49573 (sock=3) (peer 2.1.6) on 2022-05-04 12:28:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   0.646 ms 0/5956 (0%) 7.963/4.782/31.724/3.101 ms 595 pps 110
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 51885 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.01 sec  8.35 MBytes  6.99 Mbits/sec   2.380 ms 0/5955 (0%) -/-/-/- ms 594 pps
[ 15] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 59472 (sock=4) (peer 2.1.6) on 2022-05-04 12:28:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   1.152 ms 0/6806 (0%) 7.652/4.852/30.934/3.038 ms 680 pps 131
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.217%eth0 port 58479 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 16] Sent 6806 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.01 sec  9.54 MBytes  8.00 Mbits/sec   1.909 ms 0/6805 (0%) -/-/-/- ms 679 pps
[ 17] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60204 (sock=3) (peer 2.1.6) on 2022-05-04 12:29:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec   0.855 ms 0/7656 (0%) 5.021/2.461/22.998/2.766 ms 765 pps 224
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.217%eth0 port 50715 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 18] Sent 7656 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec   1.469 ms 0/7655 (0%) -/-/-/- ms 765 pps
[ 19] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35159 (sock=4) (peer 2.1.6) on 2022-05-04 12:29:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec   0.874 ms 0/8507 (0%) 5.589/2.787/24.298/3.023 ms 850 pps 224
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.217%eth0 port 55974 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 20] Sent 8507 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.02 sec  11.9 MBytes  9.98 Mbits/sec   1.912 ms 0/8506 (0%) -/-/-/- ms 848 pps
[ 21] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60150 (sock=3) (peer 2.1.6) on 2022-05-04 12:30:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.01 sec  13.1 MBytes  11.0 Mbits/sec   1.548 ms 0/9357 (0%) 6.596/3.336/26.350/3.114 ms 935 pps 208
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1069.09 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.217%eth0 port 54040 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec  0/0      936 pps
[ 22] Sent 9357 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.01 sec  13.1 MBytes  11.0 Mbits/sec   2.185 ms 0/9356 (0%) -/-/-/- ms 934 pps
[ 23] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 37987 (sock=4) (peer 2.1.6) on 2022-05-04 12:30:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec   1.002 ms 0/10207 (0%) 8.454/4.914/26.712/2.951 ms 1020 pps 177
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 980.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.217%eth0 port 48449 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec  0/0     1021 pps
[ 24] Sent 10207 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.99 sec  14.3 MBytes  12.0 Mbits/sec   1.122 ms 0/10206 (0%) -/-/-/- ms 1021 pps
[ 25] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 57438 (sock=3) (peer 2.1.6) on 2022-05-04 12:30:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.01 sec  15.5 MBytes  13.0 Mbits/sec   1.161 ms 0/11058 (0%) 7.958/4.715/35.642/3.179 ms 1105 pps 204
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 904.62 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.217%eth0 port 47403 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec  0/0     1106 pps
[ 26] Sent 11058 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.99 sec  15.5 MBytes  13.0 Mbits/sec   1.182 ms 0/11057 (0%) -/-/-/- ms 1106 pps
[ 27] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51602 (sock=4) (peer 2.1.6) on 2022-05-04 12:31:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec   0.867 ms 0/11908 (0%) 5.924/2.698/24.202/2.928 ms 1191 pps 296
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.217%eth0 port 46454 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec  0/0     1191 pps
[ 28] Sent 11908 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-9.99 sec  16.7 MBytes  14.0 Mbits/sec   1.257 ms 0/11907 (0%) 15.841/0.460/80.090/0.567 ms 1191 pps 111
[ 29] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53016 (sock=3) (peer 2.1.6) on 2022-05-04 12:31:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec   0.802 ms 0/12758 (0%) 5.991/2.339/29.519/3.146 ms 1275 pps 313
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.217%eth0 port 48759 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[ 30] Sent 12758 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.01 sec  17.9 MBytes  15.0 Mbits/sec   0.853 ms 0/12757 (0%) -/-/-/- ms 1274 pps
[ 31] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51931 (sock=4) (peer 2.1.6) on 2022-05-04 12:31:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec   1.001 ms 0/13609 (0%) 8.835/5.228/37.831/3.054 ms 1360 pps 226
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 735.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.217%eth0 port 44333 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec  0/0     1361 pps
[ 32] Sent 13609 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.01 sec  19.1 MBytes  16.0 Mbits/sec   0.898 ms 0/13608 (0%) -/-/-/- ms 1359 pps
[ 33] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53232 (sock=3) (peer 2.1.6) on 2022-05-04 12:32:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.01 sec  20.3 MBytes  17.0 Mbits/sec   1.007 ms 0/14459 (0%) 8.038/4.758/25.631/3.069 ms 1445 pps 264
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 691.76 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.217%eth0 port 49802 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec  0/0     1446 pps
[ 34] Sent 14459 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec   0.742 ms 10/14458 (0.069%) -/-/-/- ms 1445 pps
[ 35] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45322 (sock=4) (peer 2.1.6) on 2022-05-04 12:32:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec   0.784 ms 0/15309 (0%) 7.637/3.435/37.682/3.630 ms 1530 pps 295
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 653.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.217%eth0 port 57565 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec  0/0     1531 pps
[ 36] Sent 15309 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.01 sec  21.5 MBytes  18.0 Mbits/sec   0.692 ms 0/15308 (0%) -/-/-/- ms 1529 pps
[ 37] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 50227 (sock=3) (peer 2.1.6) on 2022-05-04 12:32:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec   0.672 ms 0/16160 (0%) 6.136/0.918/30.055/3.668 ms 1615 pps 387
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 618.95 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.217%eth0 port 39729 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec  0/0     1616 pps
[ 38] Sent 16160 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.03 sec  22.7 MBytes  18.9 Mbits/sec   1.320 ms 0/16159 (0%) -/-/-/- ms 1610 pps
[ 39] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 47055 (sock=4) (peer 2.1.6) on 2022-05-04 12:33:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 39] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec   0.633 ms 0/17010 (0%) 12.015/5.972/39.892/3.813 ms 1700 pps 208
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 588.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*40] local 10.0.23.217%eth0 port 37627 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*40] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec  0/0     1701 pps
[ 40] Sent 17010 datagrams
[ 40] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*40] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec   0.559 ms 5/17009 (0.029%) -/-/-/- ms 1700 pps
[ 41] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36407 (sock=3) (peer 2.1.6) on 2022-05-04 12:33:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 41] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec   0.538 ms 0/17860 (0%) 11.891/5.685/40.603/4.377 ms 1785 pps 221
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 560.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*42] local 10.0.23.217%eth0 port 44817 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec  0/0     1786 pps
[ 42] Sent 17860 datagrams
[ 42] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*42] 0.00-10.01 sec  24.7 MBytes  20.7 Mbits/sec   0.568 ms 273/17859 (1.5%) -/-/-/- ms 1784 pps
[ 43] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46648 (sock=4) (peer 2.1.6) on 2022-05-04 12:33:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 43] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec   0.575 ms 0/18711 (0%) 6.843/0.434/31.007/3.732 ms 1870 pps 402
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 534.55 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*44] local 10.0.23.217%eth0 port 37594 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*44] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec  0/0     1871 pps
[ 44] Sent 18711 datagrams
[ 44] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*44] 0.00-10.01 sec  26.2 MBytes  21.9 Mbits/sec   0.877 ms 35/18710 (0.19%) 23.480/0.128/94.784/0.184 ms 1869 pps 117
[ 45] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 39358 (sock=3) (peer 2.1.6) on 2022-05-04 12:34:05 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 45] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec   0.563 ms 0/19561 (0%) 5.078/-0.531/37.719/3.868 ms 1955 pps 566
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 511.30 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*46] local 10.0.23.217%eth0 port 60367 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*46] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec  0/0     1956 pps
[ 46] Sent 19561 datagrams
[ 46] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*46] 0.00-10.02 sec  27.3 MBytes  22.9 Mbits/sec   0.542 ms 52/19560 (0.27%) 19.807/0.990/81.644/0.368 ms 1951 pps 144
[ 47] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 48924 (sock=4) (peer 2.1.6) on 2022-05-04 12:34:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 47] 0.00-10.02 sec  28.6 MBytes  24.0 Mbits/sec   0.880 ms 0/20411 (0%) 3.138/-2.224/21.398/3.438 ms 2038 pps 955
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*48] local 10.0.23.217%eth0 port 40374 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*48] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec  0/0     2041 pps
[ 48] Sent 20411 datagrams
[ 48] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*48] 0.00-10.06 sec  27.9 MBytes  23.2 Mbits/sec   0.397 ms 535/20410 (2.6%) 29.206/1.809/122.655/0.195 ms 2029 pps 99
[ 49] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 56932 (sock=3) (peer 2.1.6) on 2022-05-04 12:34:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 49] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec   0.549 ms 0/21262 (0%) 7.789/2.469/31.198/3.815 ms 2125 pps 401
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 470.40 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*50] local 10.0.23.217%eth0 port 34160 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*50] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec  0/0     2126 pps
[ 50] Sent 21262 datagrams
[ 50] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*50] 0.00-10.01 sec  29.5 MBytes  24.7 Mbits/sec   0.570 ms 190/21261 (0.89%) -/-/-/- ms 2122 pps
[ 51] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46448 (sock=4) (peer 2.1.6) on 2022-05-04 12:35:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 51] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec   0.455 ms 0/22112 (0%) 8.150/2.398/33.622/3.795 ms 2211 pps 399
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 452.31 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*52] local 10.0.23.217%eth0 port 40692 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*52] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec  0/0     2211 pps
[ 52] Sent 22112 datagrams
[ 52] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*52] 0.00-10.01 sec  30.6 MBytes  25.7 Mbits/sec   0.337 ms 262/22111 (1.2%) -/-/-/- ms 2208 pps
[ 53] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 33521 (sock=3) (peer 2.1.6) on 2022-05-04 12:35:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 53] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec   0.444 ms 0/22962 (0%) 6.762/1.401/31.152/3.639 ms 2295 pps 499
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 435.56 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*54] local 10.0.23.217%eth0 port 60350 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*54] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec  0/0     2296 pps
[ 54] Sent 22962 datagrams
[ 54] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*54] 0.00-10.01 sec  30.5 MBytes  25.6 Mbits/sec   0.315 ms 1193/22961 (5.2%) 26.756/0.119/104.696/0.363 ms 2293 pps 119
[ 55] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 50356 (sock=4) (peer 2.1.6) on 2022-05-04 12:35:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 55] 0.00-9.99 sec  33.4 MBytes  28.0 Mbits/sec   0.349 ms 0/23813 (0%) 4.397/-1.956/25.603/3.566 ms 2383 pps 797
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 420.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*56] local 10.0.23.217%eth0 port 44365 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*56] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec  0/0     2381 pps
[ 56] Sent 23813 datagrams
[ 56] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*56] 0.00-10.04 sec  30.0 MBytes  25.1 Mbits/sec   0.434 ms 2401/23812 (10%) 37.678/0.727/121.105/0.204 ms 2370 pps 83
[ 57] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 59070 (sock=3) (peer 2.1.6) on 2022-05-04 12:36:08 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 57] 0.00-10.01 sec  34.6 MBytes  29.0 Mbits/sec   0.408 ms 0/24663 (0%) 8.061/-0.439/30.806/4.231 ms 2465 pps 449
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 405.52 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*58] local 10.0.23.217%eth0 port 60162 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*58] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec  0/0     2466 pps
[ 58] Sent 24663 datagrams
[ 58] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*58] 0.00-10.03 sec  31.9 MBytes  26.7 Mbits/sec   0.358 ms 1877/24662 (7.6%) -/-/-/- ms 2458 pps
[*58] 0.00-10.03 sec  1 datagrams received out-of-order
[ 59] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 34109 (sock=4) (peer 2.1.6) on 2022-05-04 12:36:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 59] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec   0.303 ms 0/25513 (0%) 9.640/3.023/31.845/3.867 ms 2550 pps 389
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1970 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 392.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*60] local 10.0.23.217%eth0 port 35230 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*60] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec  0/0     2551 pps
[ 60] Sent 25513 datagrams
[ 60] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*60] 0.00-10.03 sec  31.3 MBytes  26.2 Mbits/sec   0.794 ms 3165/25512 (12%) -/-/-/- ms 2543 pps
