------------------------------------------------------------
Server listening on UDP port 5001 with pid 1261
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 57428 (sock=3) (peer 2.1.6) on 2022-05-04 11:37:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  1.20 MBytes  1.00 Mbits/sec   2.915 ms 0/854 (0%) 4.792/2.312/24.483/2.904 ms 85 pps 26
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 49471 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   6.661 ms 0/853 (0%) -/-/-/- ms 85 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60823 (sock=5) (peer 2.1.6) on 2022-05-04 11:38:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   2.319 ms 0/1704 (0%) 5.996/3.767/24.674/2.398 ms 170 pps 42
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 33013 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   5.531 ms 0/1703 (0%) -/-/-/- ms 170 pps
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38925 (sock=3) (peer 2.1.6) on 2022-05-04 11:38:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   2.444 ms 0/2554 (0%) 4.887/2.351/18.318/2.257 ms 255 pps 77
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 45093 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   5.089 ms 0/2553 (0%) 11.626/0.291/68.558/1.173 ms 255 pps 32
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 42773 (sock=4) (peer 2.1.6) on 2022-05-04 11:38:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  4.77 MBytes  4.00 Mbits/sec   2.006 ms 0/3405 (0%) 5.702/1.651/31.726/3.233 ms 340 pps 88
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 48608 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.01 sec  4.77 MBytes  4.00 Mbits/sec   2.343 ms 0/3404 (0%) -/-/-/- ms 339 pps
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 34024 (sock=3) (peer 2.1.6) on 2022-05-04 11:39:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   1.550 ms 0/4255 (0%) 8.081/4.021/30.044/3.581 ms 425 pps 77
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 46948 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.02 sec  5.96 MBytes  4.99 Mbits/sec   3.382 ms 0/4254 (0%) -/-/-/- ms 424 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58013 (sock=4) (peer 2.1.6) on 2022-05-04 11:39:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   1.743 ms 0/5105 (0%) 7.534/3.363/36.783/3.809 ms 510 pps 100
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 33857 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  7.16 MBytes  6.00 Mbits/sec   2.712 ms 0/5104 (0%) -/-/-/- ms 509 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 37875 (sock=3) (peer 2.1.6) on 2022-05-04 11:39:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   1.482 ms 0/5956 (0%) 5.921/2.533/29.401/2.963 ms 596 pps 148
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 57072 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-9.99 sec  8.35 MBytes  7.01 Mbits/sec   2.078 ms 0/5955 (0%) -/-/-/- ms 595 pps
[ 15] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 49806 (sock=4) (peer 2.1.6) on 2022-05-04 11:40:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   1.540 ms 0/6806 (0%) 7.252/3.988/24.501/2.966 ms 681 pps 138
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.217%eth0 port 42510 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 16] Sent 6806 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.01 sec  9.54 MBytes  7.99 Mbits/sec   1.870 ms 0/6805 (0%) -/-/-/- ms 679 pps
[ 17] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38013 (sock=3) (peer 2.1.6) on 2022-05-04 11:40:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  10.7 MBytes  9.01 Mbits/sec   1.208 ms 0/7656 (0%) 7.044/3.553/28.360/3.227 ms 766 pps 160
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.217%eth0 port 52295 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 18] Sent 7656 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.03 sec  10.7 MBytes  8.98 Mbits/sec   2.488 ms 0/7655 (0%) -/-/-/- ms 763 pps
[ 19] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45631 (sock=4) (peer 2.1.6) on 2022-05-04 11:40:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec   1.254 ms 0/8507 (0%) 7.116/2.933/29.504/3.470 ms 851 pps 176
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.217%eth0 port 51391 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 20] Sent 8507 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.98 sec  11.9 MBytes  10.0 Mbits/sec   1.280 ms 0/8506 (0%) -/-/-/- ms 852 pps
[ 21] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 55188 (sock=3) (peer 2.1.6) on 2022-05-04 11:41:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.01 sec  13.1 MBytes  11.0 Mbits/sec   1.141 ms 0/9357 (0%) 7.458/2.292/26.063/3.432 ms 935 pps 184
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1069.09 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.217%eth0 port 35656 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec  0/0      936 pps
[ 22] Sent 9357 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.01 sec  13.1 MBytes  11.0 Mbits/sec   1.321 ms 0/9356 (0%) -/-/-/- ms 934 pps
[ 23] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51799 (sock=4) (peer 2.1.6) on 2022-05-04 11:41:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.01 sec  14.3 MBytes  12.0 Mbits/sec   1.014 ms 0/10207 (0%) 11.671/5.669/38.202/3.830 ms 1020 pps 128
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 980.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.217%eth0 port 43285 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec  0/0     1021 pps
[ 24] Sent 10207 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.01 sec  14.3 MBytes  12.0 Mbits/sec   1.394 ms 0/10206 (0%) -/-/-/- ms 1019 pps
[ 25] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35132 (sock=3) (peer 2.1.6) on 2022-05-04 11:41:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec   0.899 ms 0/11058 (0%) 11.250/6.019/33.122/3.686 ms 1105 pps 144
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 904.62 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.217%eth0 port 37316 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec  0/0     1106 pps
[ 26] Sent 11058 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.04 sec  15.5 MBytes  12.9 Mbits/sec   2.537 ms 0/11057 (0%) -/-/-/- ms 1101 pps
[ 27] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38830 (sock=4) (peer 2.1.6) on 2022-05-04 11:42:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec   0.772 ms 0/11908 (0%) 9.128/4.195/29.889/3.714 ms 1190 pps 192
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.217%eth0 port 47365 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec  0/0     1191 pps
[ 28] Sent 11908 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.03 sec  16.7 MBytes  14.0 Mbits/sec   1.674 ms 8/11907 (0.067%) -/-/-/- ms 1187 pps
[ 29] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 42912 (sock=3) (peer 2.1.6) on 2022-05-04 11:42:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.01 sec  17.9 MBytes  15.0 Mbits/sec   1.076 ms 0/12758 (0%) 13.395/7.691/41.351/4.357 ms 1275 pps 140
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.217%eth0 port 48822 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[ 30] Sent 12758 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.02 sec  17.9 MBytes  15.0 Mbits/sec   1.358 ms 11/12757 (0.086%) -/-/-/- ms 1272 pps
[ 31] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 59011 (sock=4) (peer 2.1.6) on 2022-05-04 11:42:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec   0.973 ms 0/13609 (0%) 13.601/7.734/39.628/4.232 ms 1361 pps 147
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 735.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.217%eth0 port 38264 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec  0/0     1361 pps
[ 32] Sent 13609 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.01 sec  19.1 MBytes  16.0 Mbits/sec   0.821 ms 5/13608 (0.037%) -/-/-/- ms 1358 pps
[ 33] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 56941 (sock=3) (peer 2.1.6) on 2022-05-04 11:43:16 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.01 sec  20.3 MBytes  17.0 Mbits/sec   1.016 ms 0/14459 (0%) 11.838/5.734/37.981/4.094 ms 1445 pps 179
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 691.76 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.217%eth0 port 44477 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec  0/0     1446 pps
[ 34] Sent 14459 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  19.7 MBytes  16.4 Mbits/sec   1.800 ms 400/14458 (2.8%) -/-/-/- ms 1438 pps
[ 35] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51668 (sock=4) (peer 2.1.6) on 2022-05-04 11:43:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.02 sec  21.5 MBytes  18.0 Mbits/sec   1.278 ms 0/15309 (0%) 10.816/5.521/38.191/3.982 ms 1529 pps 208
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 653.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.217%eth0 port 53205 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec  0/0     1531 pps
[ 36] Sent 15309 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  21.2 MBytes  17.7 Mbits/sec   0.858 ms 164/15308 (1.1%) -/-/-/- ms 1525 pps
[ 37] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40013 (sock=3) (peer 2.1.6) on 2022-05-04 11:43:57 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec   0.693 ms 0/16160 (0%) 9.036/2.122/32.827/4.274 ms 1615 pps 263
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 618.95 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.217%eth0 port 50532 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec  0/0     1616 pps
[ 38] Sent 16160 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  21.3 MBytes  17.8 Mbits/sec   0.850 ms 955/16159 (5.9%) -/-/-/- ms 1609 pps
[ 39] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 59643 (sock=4) (peer 2.1.6) on 2022-05-04 11:44:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 39] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec   0.576 ms 0/17010 (0%) 6.472/-0.436/38.514/4.531 ms 1700 pps 386
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 588.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*40] local 10.0.23.217%eth0 port 40025 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*40] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec  0/0     1701 pps
[ 40] Sent 17010 datagrams
[ 40] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*40] 0.00-10.16 sec  14.2 MBytes  11.8 Mbits/sec   1.072 ms 6855/17009 (40%) 63.377/0.292/240.063/0.562 ms 1673 pps 23
[ 41] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51992 (sock=3) (peer 2.1.6) on 2022-05-04 11:44:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 41] 0.00-10.01 sec  25.0 MBytes  21.0 Mbits/sec   0.539 ms 0/17860 (0%) 11.982/1.873/34.960/4.357 ms 1785 pps 219
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1261 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 560.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*42] local 10.0.23.217%eth0 port 52140 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ 43] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 41228 (sock=4) (peer 2.1.6) on 2022-05-04 11:44:48 (CEST)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec  0/0     1786 pps
[ 42] Sent 17860 datagrams
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 43] 0.00-10.97 sec  15.8 MBytes  12.1 Mbits/sec  56.330 ms 7537/18803 (40%) 84.850/14.337/986.570/14.429 ms 1027 pps 18
[SUM] 0.00-10.98 sec  40.8 MBytes  31.2 Mbits/sec  0/0     2652 pps
[SUM-2] Sent 36663 datagrams
[ 45] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45521 (sock=5) (peer 2.1.6) on 2022-05-04 11:44:59 (CEST)
------------------------------------------------------------
Server listening on UDP port 5001 with pid 1361
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 59551 (sock=3) (peer 2.1.6) on 2022-05-04 11:49:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.00 sec  25.0 MBytes  20.9 Mbits/sec   0.675 ms 46/17860 (0.26%) 7.877/1.102/42.738/5.356 ms 1781 pps 332
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1361 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 560.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 39734 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec  0/0     1786 pps
[  2] Sent 17860 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.06 sec  19.4 MBytes  16.2 Mbits/sec   2.095 ms 3994/17859 (22%) 46.257/1.470/126.982/0.471 ms 1775 pps 44
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40355 (sock=5) (peer 2.1.6) on 2022-05-04 11:49:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.02 sec  26.2 MBytes  22.0 Mbits/sec   1.228 ms 0/18711 (0%) 7.959/3.055/32.768/4.012 ms 1867 pps 345
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1361 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 534.55 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 53653 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec  0/0     1871 pps
[  4] Sent 18711 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  21.1 MBytes  17.7 Mbits/sec   0.371 ms 3638/18710 (19%) 45.504/0.655/135.580/0.227 ms 1869 pps 49
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 41406 (sock=3) (peer 2.1.6) on 2022-05-04 11:49:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  27.4 MBytes  23.0 Mbits/sec   0.765 ms 0/19561 (0%) 2.759/-4.817/24.409/4.801 ms 1953 pps 1041
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1361 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 511.30 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 44884 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec  0/0     1956 pps
[  6] Sent 19561 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.04 sec  23.6 MBytes  19.7 Mbits/sec   1.143 ms 2719/19560 (14%) 38.206/3.980/107.373/0.109 ms 1947 pps 65
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45323 (sock=4) (peer 2.1.6) on 2022-05-04 11:50:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  28.6 MBytes  24.0 Mbits/sec   0.419 ms 0/20411 (0%) 8.426/-0.907/35.154/4.797 ms 2040 pps 356
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1361 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 35883 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec  0/0     2041 pps
[  8] Sent 20411 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.04 sec  23.8 MBytes  19.9 Mbits/sec   0.984 ms 3417/20410 (17%) 37.841/0.237/117.005/0.152 ms 2032 pps 66
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 39310 (sock=3) (peer 2.1.6) on 2022-05-04 11:50:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.01 sec  29.8 MBytes  25.0 Mbits/sec   0.446 ms 0/21262 (0%) 12.942/1.761/37.625/5.289 ms 2123 pps 241
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1361 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 470.40 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 43657 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec  0/0     2126 pps
[ 10] Sent 21262 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.14 sec  25.9 MBytes  21.4 Mbits/sec   4.338 ms 2799/21261 (13%) -/-/-/- ms 2096 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53073 (sock=4) (peer 2.1.6) on 2022-05-04 11:50:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec   0.431 ms 5/22112 (0.023%) 13.299/6.574/38.022/4.520 ms 2210 pps 244
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1361 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 452.31 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 59917 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec  0/0     2211 pps
[ 12] Sent 22112 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.11 sec  16.5 MBytes  13.7 Mbits/sec   0.896 ms 10364/22111 (47%) -/-/-/- ms 2187 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 44914 (sock=3) (peer 2.1.6) on 2022-05-04 11:51:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.01 sec  32.1 MBytes  26.9 Mbits/sec   0.579 ms 47/22962 (0.2%) 10.766/1.915/34.978/5.443 ms 2289 pps 313
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1361 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 435.56 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 34093 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec  0/0     2296 pps
[ 14] Sent 22962 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.11 sec  11.1 MBytes  9.19 Mbits/sec   0.862 ms 15058/22961 (66%) 86.974/0.301/212.009/0.610 ms 2270 pps 13
[ 15] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51465 (sock=4) (peer 2.1.6) on 2022-05-04 11:51:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.02 sec  33.4 MBytes  27.9 Mbits/sec   0.628 ms 11/23813 (0.046%) 6.310/-1.342/29.147/4.293 ms 2376 pps 554
[ 17] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60337 (sock=3) (peer 2.1.6) on 2022-05-04 11:51:35 (CEST)
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1361 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 420.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.217%eth0 port 47696 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec  0/0     2381 pps
[ 16] Sent 23813 datagrams
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.11 sec  18.9 MBytes  15.7 Mbits/sec   1.004 ms 11204/24663 (45%) 68.836/2.792/111.304/7.388 ms 1332 pps 28
[ 19] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60337 (sock=5) (peer 2.1.6) on 2022-05-04 11:51:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-0.00 sec  0.003 MBytes  0.000 Mbits/sec   0.117 ms 24672/24674 (1e+02%) 131.930/130.994/132.865/131.001 ms 1069 pps 0
------------------------------------------------------------
Server listening on UDP port 5001 with pid 1429
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 39570 (sock=3) (peer 2.1.6) on 2022-05-04 11:53:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.00 sec  35.5 MBytes  29.8 Mbits/sec   0.290 ms 184/25513 (0.72%) 11.551/2.742/88.491/10.821 ms 2532 pps 322
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 1429 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 392.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 35973 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec  0/0     2551 pps
[  2] Sent 25513 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.03 sec  16.6 MBytes  13.8 Mbits/sec   1.538 ms 13696/25512 (54%) 95.723/18.256/206.452/0.425 ms 2542 pps 18
