------------------------------------------------------------
Server listening on UDP port 5001 with pid 2180
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34039 (sock=3) (peer 2.1.6) on 2022-05-13 13:00:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.084 ms 0/854 (0%) 2.398/2.089/5.315/0.245 ms 85 pps 52
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 56382 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.036 ms 0/853 (0%) 2.047/1.857/5.167/0.223 ms 85 pps 61
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42163 (sock=5) (peer 2.1.6) on 2022-05-13 13:01:09 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.012 ms 0/1279 (0%) 2.584/2.442/5.182/0.187 ms 128 pps 73
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 50744 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.028 ms 0/1278 (0%) 1.980/1.833/4.756/0.144 ms 127 pps 95
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37280 (sock=3) (peer 2.1.6) on 2022-05-13 13:01:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.012 ms 0/1704 (0%) 2.585/2.411/5.291/0.175 ms 170 pps 97
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 46289 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.080 ms 0/1703 (0%) 2.048/1.863/5.061/0.186 ms 170 pps 122
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49206 (sock=4) (peer 2.1.6) on 2022-05-13 13:01:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.013 ms 0/2129 (0%) 2.476/2.264/7.885/0.246 ms 213 pps 126
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 60261 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.055 ms 0/2128 (0%) 2.116/1.931/7.269/0.228 ms 212 pps 148
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40216 (sock=3) (peer 2.1.6) on 2022-05-13 13:02:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.016 ms 0/2554 (0%) 2.280/2.028/5.185/0.215 ms 255 pps 165
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 37043 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.175 ms 0/2553 (0%) 2.287/2.051/5.275/0.180 ms 255 pps 164
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52181 (sock=4) (peer 2.1.6) on 2022-05-13 13:02:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.026 ms 0/2980 (0%) 2.298/2.109/5.432/0.227 ms 298 pps 191
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 43624 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.288 ms 0/2979 (0%) 2.283/2.043/5.441/0.210 ms 297 pps 192
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45224 (sock=3) (peer 2.1.6) on 2022-05-13 13:02:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.029 ms 0/3405 (0%) 2.226/1.917/5.427/0.300 ms 340 pps 225
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 33859 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.017 ms 0/3404 (0%) 2.268/1.973/7.112/0.252 ms 340 pps 221
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56352 (sock=4) (peer 2.1.6) on 2022-05-13 13:03:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.017 ms 0/3830 (0%) 2.280/2.029/5.244/0.332 ms 383 pps 247
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 49070 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.084 ms 0/3829 (0%) 2.128/1.904/5.439/0.221 ms 382 pps 264
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43880 (sock=3) (peer 2.1.6) on 2022-05-13 13:03:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.053 ms 0/4255 (0%) 2.434/2.104/5.648/0.434 ms 425 pps 257
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 54716 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.030 ms 0/4254 (0%) 2.198/1.848/6.469/0.321 ms 425 pps 284
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59374 (sock=4) (peer 2.1.6) on 2022-05-13 13:03:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.017 ms 0/4680 (0%) 2.713/2.293/7.638/0.685 ms 468 pps 253
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 51374 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.067 ms 0/4679 (0%) 1.943/1.713/5.464/0.282 ms 467 pps 354
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35521 (sock=3) (peer 2.1.6) on 2022-05-13 13:04:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.040 ms 0/5105 (0%) 6.814/1.942/14.011/2.061 ms 510 pps 110
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 53422 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.026 ms 0/5104 (0%) 0.962/0.535/4.622/0.406 ms 510 pps 780
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45612 (sock=4) (peer 2.1.6) on 2022-05-13 13:04:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.01 sec  7.25 MBytes  6.08 Mbits/sec   0.233 ms 358/5531 (6.5%) 35.021/3.597/62.659/15.757 ms 517 pps 22
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 40579 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.96 sec  7.75 MBytes  6.53 Mbits/sec   0.029 ms 0/5530 (0%) 39.513/22.121/61.944/0.508 ms 554 pps 21
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38198 (sock=3) (peer 2.1.6) on 2022-05-13 13:04:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.09 sec  7.26 MBytes  6.04 Mbits/sec   0.424 ms 775/5956 (13%) -/-/-/- ms 514 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 33743 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   0.035 ms 0/5955 (0%) -/-/-/- ms 595 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34845 (sock=4) (peer 2.1.6) on 2022-05-13 13:05:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.03 sec  7.26 MBytes  6.07 Mbits/sec   0.544 ms 1202/6381 (19%) 55.788/7.829/67.817/11.793 ms 516 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 51778 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  8.74 MBytes  7.30 Mbits/sec   0.066 ms 148/6380 (2.3%) 80.811/36.138/99.977/0.273 ms 635 pps 11
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37215 (sock=3) (peer 2.1.6) on 2022-05-13 13:05:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.05 sec  7.28 MBytes  6.07 Mbits/sec   0.658 ms 1614/6806 (24%) -/-/-/- ms 516 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 50369 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.01 sec  8.72 MBytes  7.31 Mbits/sec   0.273 ms 584/6805 (8.6%) 55.582/35.657/76.447/0.584 ms 680 pps 16
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52194 (sock=4) (peer 2.1.6) on 2022-05-13 13:05:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.07 sec  7.27 MBytes  6.06 Mbits/sec   0.662 ms 2047/7231 (28%) 74.067/13.335/77.910/4.903 ms 515 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 43750 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.04 sec  8.74 MBytes  7.31 Mbits/sec   0.378 ms 994/7230 (14%) -/-/-/- ms 720 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50331 (sock=3) (peer 2.1.6) on 2022-05-13 13:06:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  7.26 MBytes  6.05 Mbits/sec   0.648 ms 2475/7656 (32%) 89.505/26.463/94.973/5.557 ms 515 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 51758 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  8.76 MBytes  7.31 Mbits/sec   0.431 ms 1407/7656 (18%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35728 (sock=4) (peer 2.1.6) on 2022-05-13 13:06:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  7.27 MBytes  6.06 Mbits/sec   0.603 ms 2894/8082 (36%) 93.438/35.338/95.365/4.043 ms 516 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 41516 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  8.78 MBytes  7.33 Mbits/sec   0.511 ms 1819/8081 (23%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55985 (sock=3) (peer 2.1.6) on 2022-05-13 13:06:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.06 sec  6.57 MBytes  5.48 Mbits/sec   0.538 ms 3819/8507 (45%) 90.978/32.296/163.679/6.675 ms 466 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2180 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 58368 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  8.76 MBytes  7.31 Mbits/sec   0.547 ms 2259/8506 (27%) -/-/-/- ms 846 pps
------------------------------------------------------------
Server listening on UDP port 5001 with pid 2233
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
