------------------------------------------------------------
Server listening on UDP port 5001 with pid 2477
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35288 (sock=3) (peer 2.1.6) on 2022-05-13 13:45:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.14 MBytes  0.957 Mbits/sec   0.040 ms 39/854 (4.6%) 1.604/1.243/4.531/0.328 ms 81 pps 75
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 33116 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.043 ms 0/853 (0%) 2.989/2.844/5.645/0.209 ms 85 pps 42
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39530 (sock=5) (peer 2.1.6) on 2022-05-13 13:45:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.75 MBytes  1.46 Mbits/sec   0.032 ms 34/1279 (2.7%) 1.505/1.400/4.251/0.186 ms 124 pps 121
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 37588 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.066 ms 0/1278 (0%) 2.815/2.633/4.835/0.172 ms 127 pps 67
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 32779 (sock=3) (peer 2.1.6) on 2022-05-13 13:45:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.34 MBytes  1.96 Mbits/sec   0.044 ms 36/1704 (2.1%) 1.609/1.382/4.325/0.210 ms 167 pps 152
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 49519 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.016 ms 0/1703 (0%) 2.764/2.568/6.034/0.205 ms 170 pps 90
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36910 (sock=4) (peer 2.1.6) on 2022-05-13 13:46:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.89 MBytes  2.42 Mbits/sec   0.012 ms 68/2129 (3.2%) 1.712/1.555/5.866/0.214 ms 206 pps 177
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 60030 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.044 ms 0/2128 (0%) 2.704/2.469/5.518/0.181 ms 212 pps 116
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50436 (sock=3) (peer 2.1.6) on 2022-05-13 13:46:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.44 MBytes  2.88 Mbits/sec   0.008 ms 102/2554 (4%) 1.846/1.677/4.597/0.182 ms 245 pps 195
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 57084 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.040 ms 0/2553 (0%) 2.287/2.077/5.449/0.191 ms 255 pps 164
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33360 (sock=4) (peer 2.1.6) on 2022-05-13 13:46:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.07 MBytes  3.41 Mbits/sec   0.126 ms 77/2980 (2.6%) 2.095/1.918/7.805/0.271 ms 290 pps 204
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 40852 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.035 ms 0/2979 (0%) 2.345/2.116/5.668/0.239 ms 297 pps 187
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60011 (sock=3) (peer 2.1.6) on 2022-05-13 13:47:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.63 MBytes  3.88 Mbits/sec   0.009 ms 100/3405 (2.9%) 1.966/1.640/6.978/0.313 ms 330 pps 247
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 57168 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.065 ms 0/3404 (0%) 2.454/2.190/5.611/0.215 ms 340 pps 204
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49128 (sock=4) (peer 2.1.6) on 2022-05-13 13:47:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.24 MBytes  4.39 Mbits/sec   0.058 ms 93/3830 (2.4%) 1.993/1.733/4.914/0.289 ms 374 pps 276
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 33185 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.051 ms 0/3829 (0%) 2.281/2.009/5.576/0.232 ms 382 pps 247
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38284 (sock=3) (peer 2.1.6) on 2022-05-13 13:47:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.85 MBytes  4.90 Mbits/sec   0.012 ms 83/4255 (2%) 2.152/1.857/6.867/0.438 ms 417 pps 285
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 34921 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.058 ms 0/4254 (0%) 2.228/1.968/5.347/0.250 ms 425 pps 281
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55232 (sock=4) (peer 2.1.6) on 2022-05-13 13:48:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.43 MBytes  5.39 Mbits/sec   0.012 ms 92/4680 (2%) 2.214/1.868/7.115/0.547 ms 459 pps 305
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 45543 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.007 ms 0/4679 (0%) 2.127/1.804/5.384/0.274 ms 467 pps 323
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40399 (sock=3) (peer 2.1.6) on 2022-05-13 13:48:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  6.88 MBytes  5.77 Mbits/sec   0.033 ms 199/5105 (3.9%) 2.720/2.002/7.353/1.017 ms 491 pps 265
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 56003 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.031 ms 0/5104 (0%) 2.098/1.822/5.154/0.302 ms 510 pps 358
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48335 (sock=4) (peer 2.1.6) on 2022-05-13 13:48:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.02 sec  7.34 MBytes  6.15 Mbits/sec   0.079 ms 294/5531 (5.3%) 36.780/2.508/59.336/12.554 ms 523 pps 21
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 58566 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.99 sec  7.75 MBytes  6.51 Mbits/sec   0.166 ms 0/5530 (0%) 44.929/28.173/62.870/0.446 ms 553 pps 18
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34260 (sock=3) (peer 2.1.6) on 2022-05-13 13:49:05 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.09 sec  7.36 MBytes  6.12 Mbits/sec   0.366 ms 704/5956 (12%) -/-/-/- ms 521 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 56699 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   0.037 ms 0/5955 (0%) -/-/-/- ms 595 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46123 (sock=4) (peer 2.1.6) on 2022-05-13 13:49:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.05 sec  7.19 MBytes  6.00 Mbits/sec   0.499 ms 1254/6381 (20%) 62.902/9.238/66.771/5.652 ms 510 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 43621 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  7.48 MBytes  6.25 Mbits/sec   0.035 ms 1046/6380 (16%) -/-/-/- ms 635 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50591 (sock=3) (peer 2.1.6) on 2022-05-13 13:49:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.00 sec  7.26 MBytes  6.09 Mbits/sec   0.569 ms 1624/6806 (24%) 34.865/6.019/62.262/15.436 ms 518 pps 22
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 45498 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.01 sec  9.00 MBytes  7.55 Mbits/sec   0.146 ms 382/6805 (5.6%) 82.028/54.529/107.439/0.535 ms 680 pps 12
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60026 (sock=4) (peer 2.1.6) on 2022-05-13 13:50:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.06 sec  7.27 MBytes  6.06 Mbits/sec   0.621 ms 2045/7231 (28%) 51.705/-6.590/55.933/4.960 ms 515 pps 15
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2477 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 42442 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-5.96 sec  6.04 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 4309 datagrams
------------------------------------------------------------
Server listening on UDP port 5001 with pid 3310
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56418 (sock=3) (peer 2.1.6) on 2022-05-13 14:25:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.07 sec  7.50 MBytes  6.25 Mbits/sec   0.628 ms 1882/7232 (26%) 1448.807/1388.682/1455.520/19.742 ms 531 pps 1
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3310 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 60346 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[  2] Sent 7231 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.04 sec  9.05 MBytes  7.56 Mbits/sec   0.342 ms 774/7230 (11%) -/-/-/- ms 720 pps
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56138 (sock=5) (peer 2.1.6) on 2022-05-13 14:26:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.07 sec  7.50 MBytes  6.25 Mbits/sec   0.637 ms 2309/7656 (30%) 1463.691/1403.284/1468.850/19.802 ms 531 pps 1
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3310 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 36669 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[  4] Sent 7656 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.03 sec  9.05 MBytes  7.57 Mbits/sec   0.394 ms 1199/7655 (16%) -/-/-/- ms 762 pps
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37532 (sock=3) (peer 2.1.6) on 2022-05-13 14:26:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.07 sec  7.51 MBytes  6.26 Mbits/sec   0.621 ms 2725/8082 (34%) 1478.441/1418.083/1483.283/20.027 ms 532 pps 1
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3310 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 55876 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[  6] Sent 8082 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.04 sec  9.06 MBytes  7.57 Mbits/sec   0.457 ms 1621/8081 (20%) -/-/-/- ms 804 pps
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34163 (sock=4) (peer 2.1.6) on 2022-05-13 14:26:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.07 sec  7.50 MBytes  6.25 Mbits/sec   0.576 ms 3156/8508 (37%) 1493.323/1432.810/1505.237/20.213 ms 532 pps 1
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3310 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 54904 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[  8] Sent 8507 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.04 sec  9.06 MBytes  7.57 Mbits/sec   0.504 ms 2047/8507 (24%) -/-/-/- ms 847 pps
