------------------------------------------------------------
Server listening on UDP port 5001 with pid 3780
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50564 (sock=3) (peer 2.1.6) on 2022-05-13 15:27:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.017 ms 0/854 (0%) 0.703/0.446/5.116/0.302 ms 85 pps 178
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 56689 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.056 ms 0/853 (0%) 3.827/3.535/5.085/0.217 ms 85 pps 33
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53046 (sock=5) (peer 2.1.6) on 2022-05-13 15:28:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.090 ms 0/1279 (0%) 0.887/0.763/3.564/0.154 ms 128 pps 212
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 53754 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.041 ms 0/1278 (0%) 3.522/3.276/6.284/0.200 ms 127 pps 53
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58068 (sock=3) (peer 2.1.6) on 2022-05-13 15:28:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.028 ms 0/1704 (0%) 1.236/1.084/3.960/0.185 ms 170 pps 203
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 50362 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.059 ms 0/1703 (0%) 3.191/2.917/6.335/0.218 ms 170 pps 78
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59937 (sock=4) (peer 2.1.6) on 2022-05-13 15:28:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.020 ms 0/2129 (0%) 1.438/1.204/5.131/0.225 ms 213 pps 218
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 54815 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.022 ms 0/2128 (0%) 3.006/2.802/6.116/0.204 ms 212 pps 104
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46543 (sock=3) (peer 2.1.6) on 2022-05-13 15:29:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.011 ms 0/2554 (0%) 1.582/1.404/4.642/0.206 ms 255 pps 237
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 41864 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.034 ms 0/2553 (0%) 2.899/2.657/6.050/0.207 ms 255 pps 129
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39982 (sock=4) (peer 2.1.6) on 2022-05-13 15:29:28 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.120 ms 0/2980 (0%) 1.700/1.571/4.744/0.223 ms 298 pps 258
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 53458 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.023 ms 0/2979 (0%) 2.683/2.431/5.842/0.198 ms 297 pps 163
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53228 (sock=3) (peer 2.1.6) on 2022-05-13 15:29:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.090 ms 0/3405 (0%) 1.912/1.671/6.269/0.278 ms 340 pps 262
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 60692 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.141 ms 0/3404 (0%) 2.664/2.390/6.479/0.277 ms 340 pps 188
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37298 (sock=4) (peer 2.1.6) on 2022-05-13 15:30:09 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.055 ms 0/3830 (0%) 1.889/1.656/5.413/0.349 ms 383 pps 298
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 55808 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.039 ms 0/3829 (0%) 2.452/2.172/5.693/0.245 ms 382 pps 229
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53445 (sock=3) (peer 2.1.6) on 2022-05-13 15:30:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.040 ms 1/4255 (0.024%) 2.109/1.811/5.465/0.450 ms 425 pps 296
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 38201 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.029 ms 0/4254 (0%) 2.473/2.188/5.771/0.260 ms 425 pps 253
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36298 (sock=4) (peer 2.1.6) on 2022-05-13 15:30:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.125 ms 0/4680 (0%) 2.190/1.745/8.926/0.733 ms 468 pps 314
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 36272 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.028 ms 0/4679 (0%) 2.389/1.960/9.541/0.455 ms 467 pps 288
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34516 (sock=3) (peer 2.1.6) on 2022-05-13 15:31:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.038 ms 0/5105 (0%) 4.595/-0.272/10.984/2.521 ms 510 pps 163
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 43308 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.155 ms 0/5104 (0%) 3.718/2.777/7.866/0.700 ms 510 pps 202
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44663 (sock=4) (peer 2.1.6) on 2022-05-13 15:31:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.06 sec  7.25 MBytes  6.05 Mbits/sec   0.263 ms 356/5531 (6.4%) 58.831/1.844/62.649/9.164 ms 514 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 37479 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.028 ms 0/5530 (0%) 1.994/1.770/6.556/0.419 ms 553 pps 408
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52580 (sock=3) (peer 2.1.6) on 2022-05-13 15:31:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.410 ms 776/5956 (13%) 60.575/2.847/63.078/6.808 ms 515 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 45674 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   0.041 ms 0/5955 (0%) 2.054/1.632/6.676/0.720 ms 595 pps 426
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51013 (sock=4) (peer 2.1.6) on 2022-05-13 15:32:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.07 sec  7.26 MBytes  6.05 Mbits/sec   0.765 ms 1202/6382 (19%) 61.232/2.832/66.948/5.694 ms 515 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 54482 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.05 sec  8.76 MBytes  7.31 Mbits/sec   0.092 ms 133/6380 (2.1%) 45.977/2.480/52.319/0.755 ms 635 pps 20
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52864 (sock=3) (peer 2.1.6) on 2022-05-13 15:32:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.08 sec  7.28 MBytes  6.06 Mbits/sec   0.620 ms 1615/6806 (24%) 75.626/7.231/87.216/8.560 ms 515 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 36050 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.05 sec  8.76 MBytes  7.32 Mbits/sec   0.235 ms 555/6805 (8.2%) -/-/-/- ms 677 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42262 (sock=4) (peer 2.1.6) on 2022-05-13 15:32:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.663 ms 2054/7231 (28%) 86.207/27.511/88.156/4.570 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 58454 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.04 sec  8.75 MBytes  7.31 Mbits/sec   0.356 ms 986/7230 (14%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54416 (sock=3) (peer 2.1.6) on 2022-05-13 15:33:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.03 sec  7.27 MBytes  6.08 Mbits/sec   0.652 ms 2473/7657 (32%) 68.578/27.550/87.156/10.550 ms 517 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 58323 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.02 sec  8.75 MBytes  7.32 Mbits/sec   0.456 ms 1416/7655 (18%) 47.317/13.988/61.548/0.369 ms 763 pps 19
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46261 (sock=4) (peer 2.1.6) on 2022-05-13 15:33:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.07 sec  7.27 MBytes  6.05 Mbits/sec   0.599 ms 2898/8082 (36%) 81.488/15.911/89.311/6.339 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 50239 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  8.77 MBytes  7.32 Mbits/sec   0.519 ms 1828/8081 (23%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34191 (sock=3) (peer 2.1.6) on 2022-05-13 15:33:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.518 ms 3328/8507 (39%) 88.152/29.722/90.217/3.926 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3780 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 56571 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  8.78 MBytes  7.33 Mbits/sec   0.524 ms 2242/8507 (26%) -/-/-/- ms 846 pps
