------------------------------------------------------------
Server listening on UDP port 5001 with pid 4481
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 49751 (sock=3) (peer 2.1.6) on 2022-05-10 14:03:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  17.8 MBytes  15.0 Mbits/sec   1.116 ms 28/12758 (0.22%) 7.420/2.949/52.337/5.603 ms 1272 pps 252
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4481 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 57435 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[  2] Sent 12758 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.04 sec  17.9 MBytes  14.9 Mbits/sec   2.511 ms 0/12757 (0%) -/-/-/- ms 1271 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51348 (sock=5) (peer 2.1.6) on 2022-05-10 14:03:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec   0.771 ms 0/13609 (0%) 9.626/5.100/31.550/3.525 ms 1360 pps 208
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4481 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 735.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 39789 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec  0/0     1361 pps
[  4] Sent 13609 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.05 sec  19.1 MBytes  15.9 Mbits/sec   2.334 ms 0/13608 (0%) -/-/-/- ms 1353 pps
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36327 (sock=3) (peer 2.1.6) on 2022-05-10 14:03:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  20.3 MBytes  17.0 Mbits/sec   0.947 ms 0/14459 (0%) 11.176/5.162/38.998/3.596 ms 1444 pps 190
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4481 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 691.76 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 57559 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec  0/0     1446 pps
[  6] Sent 14459 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.04 sec  20.2 MBytes  16.9 Mbits/sec   0.668 ms 69/14458 (0.48%) -/-/-/- ms 1440 pps
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 43557 (sock=4) (peer 2.1.6) on 2022-05-10 14:04:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec   0.684 ms 4/15309 (0.026%) 14.406/8.600/38.496/3.660 ms 1531 pps 156
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4481 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 653.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 34886 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec  0/0     1531 pps
[  8] Sent 15309 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.43 sec  12.2 MBytes  9.83 Mbits/sec  43.351 ms 6593/15308 (43%) -/-/-/- ms 1467 pps
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 34987 (sock=3) (peer 2.1.6) on 2022-05-10 14:04:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-9.99 sec  21.2 MBytes  17.8 Mbits/sec   0.671 ms 1040/16160 (6.4%) 24.753/4.929/114.956/26.175 ms 1513 pps 90
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 41292 (sock=4) (peer 2.1.6) on 2022-05-10 14:04:45 (CEST)
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4481 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 618.95 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 47236 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.10 sec  19.4 MBytes  16.1 Mbits/sec   0.642 ms 3202/17010 (19%) 99.403/10.708/132.164/24.633 ms 1367 pps 20
------------------------------------------------------------
Server listening on UDP port 5001 with pid 4523
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 43201 (sock=3) (peer 2.1.6) on 2022-05-10 14:06:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   1.899 ms 0/854 (0%) 3.882/1.820/22.490/2.203 ms 85 pps 32
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 43546 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.03 sec  1.20 MBytes  1.00 Mbits/sec  10.189 ms 0/853 (0%) 8.323/0.621/49.782/2.162 ms 85 pps 15
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 55947 (sock=5) (peer 2.1.6) on 2022-05-10 14:06:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.00 sec  2.39 MBytes  2.00 Mbits/sec   1.729 ms 0/1704 (0%) 4.239/2.072/28.646/2.316 ms 170 pps 59
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 46168 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   5.125 ms 0/1703 (0%) -/-/-/- ms 170 pps
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 56203 (sock=3) (peer 2.1.6) on 2022-05-10 14:06:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  3.58 MBytes  3.00 Mbits/sec   1.380 ms 0/2554 (0%) 7.894/4.858/26.263/2.497 ms 255 pps 48
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 54163 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.02 sec  3.58 MBytes  3.00 Mbits/sec   4.966 ms 0/2553 (0%) -/-/-/- ms 254 pps
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 52649 (sock=4) (peer 2.1.6) on 2022-05-10 14:07:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  4.77 MBytes  4.00 Mbits/sec   1.986 ms 0/3405 (0%) 8.494/5.453/25.912/2.645 ms 340 pps 59
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 55388 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.03 sec  4.77 MBytes  3.99 Mbits/sec   3.909 ms 0/3404 (0%) -/-/-/- ms 339 pps
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 41421 (sock=3) (peer 2.1.6) on 2022-05-10 14:07:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.683 ms 0/4255 (0%) 9.505/6.465/22.650/2.440 ms 425 pps 66
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 35031 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.03 sec  5.96 MBytes  4.99 Mbits/sec   3.992 ms 0/4254 (0%) -/-/-/- ms 424 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36088 (sock=4) (peer 2.1.6) on 2022-05-10 14:07:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   1.339 ms 0/5105 (0%) 6.753/3.554/30.214/2.620 ms 510 pps 111
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 56480 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  7.16 MBytes  6.00 Mbits/sec   2.786 ms 0/5104 (0%) -/-/-/- ms 510 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53519 (sock=3) (peer 2.1.6) on 2022-05-10 14:08:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   1.666 ms 0/5956 (0%) 8.171/5.061/32.886/3.109 ms 595 pps 107
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 32784 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.02 sec  8.35 MBytes  6.99 Mbits/sec   2.589 ms 0/5955 (0%) -/-/-/- ms 594 pps
[ 15] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36560 (sock=4) (peer 2.1.6) on 2022-05-10 14:08:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   1.654 ms 0/6806 (0%) 6.902/3.770/24.376/2.723 ms 680 pps 145
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.217%eth0 port 58729 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 16] Sent 6806 datagrams
[ 17] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 55289 (sock=3) (peer 2.1.6) on 2022-05-10 14:08:58 (CEST)
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.03 sec  9.54 MBytes  7.98 Mbits/sec   3.369 ms 0/6805 (0%) -/-/-/- ms 678 pps
[ 17] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec   1.287 ms 0/7656 (0%) 8.769/5.040/26.787/3.058 ms 766 pps 128
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[SUM] 0.00-20.31 sec  20.3 MBytes  8.37 Mbits/sec  0/0      712 pps
[SUM-2] Sent 14462 datagrams
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.217%eth0 port 36386 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 18] Sent 7656 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.04 sec  10.7 MBytes  8.97 Mbits/sec   2.206 ms 0/7655 (0%) -/-/-/- ms 762 pps
[ 19] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53479 (sock=5) (peer 2.1.6) on 2022-05-10 14:09:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec   1.034 ms 0/8507 (0%) 7.979/4.511/26.392/3.119 ms 850 pps 157
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.217%eth0 port 39421 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 20] Sent 8507 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.01 sec  11.9 MBytes  10.0 Mbits/sec   1.536 ms 0/8506 (0%) -/-/-/- ms 849 pps
[ 21] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 39936 (sock=3) (peer 2.1.6) on 2022-05-10 14:09:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.01 sec  13.1 MBytes  11.0 Mbits/sec   1.210 ms 0/9357 (0%) 10.798/6.843/32.638/3.315 ms 935 pps 127
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1069.09 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.217%eth0 port 37192 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec  0/0      936 pps
[ 22] Sent 9357 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.02 sec  13.1 MBytes  11.0 Mbits/sec   1.695 ms 0/9356 (0%) -/-/-/- ms 933 pps
[ 23] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 42506 (sock=4) (peer 2.1.6) on 2022-05-10 14:09:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec   0.897 ms 0/10207 (0%) 10.512/6.547/33.631/3.250 ms 1021 pps 143
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 980.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.217%eth0 port 50291 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec  0/0     1021 pps
[ 24] Sent 10207 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.01 sec  14.3 MBytes  12.0 Mbits/sec   1.372 ms 0/10206 (0%) -/-/-/- ms 1019 pps
[ 25] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 54738 (sock=3) (peer 2.1.6) on 2022-05-10 14:10:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec   0.863 ms 0/11058 (0%) 8.230/4.892/26.561/2.899 ms 1106 pps 198
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 904.62 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.217%eth0 port 47414 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec  0/0     1106 pps
[ 26] Sent 11058 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec   1.159 ms 0/11057 (0%) -/-/-/- ms 1105 pps
[ 27] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60373 (sock=4) (peer 2.1.6) on 2022-05-10 14:10:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.01 sec  16.7 MBytes  14.0 Mbits/sec   1.170 ms 0/11908 (0%) 9.863/5.545/27.941/3.045 ms 1190 pps 177
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.217%eth0 port 37030 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec  0/0     1191 pps
[ 28] Sent 11908 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.01 sec  16.7 MBytes  14.0 Mbits/sec   0.917 ms 0/11907 (0%) -/-/-/- ms 1189 pps
[ 29] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58097 (sock=3) (peer 2.1.6) on 2022-05-10 14:11:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec   0.832 ms 0/12758 (0%) 10.811/5.922/32.063/3.298 ms 1276 pps 173
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.217%eth0 port 38709 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[ 30] Sent 12758 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.02 sec  17.9 MBytes  15.0 Mbits/sec   1.720 ms 0/12757 (0%) -/-/-/- ms 1272 pps
[ 31] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 37815 (sock=4) (peer 2.1.6) on 2022-05-10 14:11:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.01 sec  19.1 MBytes  16.0 Mbits/sec   1.194 ms 0/13609 (0%) 9.608/4.971/34.308/3.346 ms 1360 pps 208
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 735.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.217%eth0 port 39146 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec  0/0     1361 pps
[ 32] Sent 13609 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.01 sec  19.1 MBytes  16.0 Mbits/sec   1.157 ms 0/13608 (0%) -/-/-/- ms 1358 pps
[ 33] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58940 (sock=3) (peer 2.1.6) on 2022-05-10 14:11:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec   0.838 ms 0/14459 (0%) 9.482/4.068/32.598/3.448 ms 1446 pps 224
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 691.76 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.217%eth0 port 58162 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec  0/0     1446 pps
[ 34] Sent 14459 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  20.3 MBytes  16.9 Mbits/sec   1.966 ms 0/14458 (0%) -/-/-/- ms 1439 pps
[ 35] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 52942 (sock=4) (peer 2.1.6) on 2022-05-10 14:12:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.01 sec  21.5 MBytes  18.0 Mbits/sec   0.875 ms 0/15309 (0%) 8.043/2.140/26.940/3.411 ms 1529 pps 279
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 653.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.217%eth0 port 60554 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec  0/0     1531 pps
[ 36] Sent 15309 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-9.97 sec  21.3 MBytes  17.9 Mbits/sec   0.625 ms 132/15308 (0.86%) -/-/-/- ms 1535 pps
[ 37] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60838 (sock=3) (peer 2.1.6) on 2022-05-10 14:12:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec   0.713 ms 0/16160 (0%) 14.506/9.452/34.903/3.732 ms 1616 pps 164
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 618.95 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.217%eth0 port 51467 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec  0/0     1616 pps
[ 38] Sent 16160 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.06 sec  18.8 MBytes  15.7 Mbits/sec   0.866 ms 2773/16159 (17%) -/-/-/- ms 1607 pps
[ 39] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53659 (sock=4) (peer 2.1.6) on 2022-05-10 14:12:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 39] 0.00-10.01 sec  23.8 MBytes  20.0 Mbits/sec   0.793 ms 0/17010 (0%) 11.499/1.982/36.612/4.393 ms 1700 pps 217
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 588.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*40] local 10.0.23.217%eth0 port 50621 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*40] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec  0/0     1701 pps
[ 40] Sent 17010 datagrams
[ 40] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*40] 0.00-10.01 sec  23.0 MBytes  19.3 Mbits/sec   0.528 ms 611/17009 (3.6%) -/-/-/- ms 1699 pps
[ 41] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 33437 (sock=3) (peer 2.1.6) on 2022-05-10 14:13:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 41] 0.00-10.01 sec  25.0 MBytes  21.0 Mbits/sec   0.827 ms 0/17860 (0%) 14.773/8.479/43.727/4.039 ms 1785 pps 178
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 560.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*42] local 10.0.23.217%eth0 port 32868 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec  0/0     1786 pps
[ 42] Sent 17860 datagrams
[ 42] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*42] 0.00-10.04 sec  25.0 MBytes  20.9 Mbits/sec   0.666 ms 60/17859 (0.34%) -/-/-/- ms 1779 pps
[ 43] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45551 (sock=4) (peer 2.1.6) on 2022-05-10 14:13:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 43] 0.00-10.01 sec  26.2 MBytes  22.0 Mbits/sec   0.528 ms 0/18711 (0%) 7.724/1.704/31.908/3.331 ms 1870 pps 356
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 534.55 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*44] local 10.0.23.217%eth0 port 38673 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*44] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec  0/0     1871 pps
[ 44] Sent 18711 datagrams
[ 44] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*44] 0.00-10.01 sec  25.4 MBytes  21.3 Mbits/sec   0.448 ms 611/18710 (3.3%) -/-/-/- ms 1868 pps
[ 45] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 54240 (sock=3) (peer 2.1.6) on 2022-05-10 14:13:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 45] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec   0.494 ms 0/19561 (0%) 9.704/2.415/31.595/4.099 ms 1956 pps 296
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 511.30 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*46] local 10.0.23.217%eth0 port 34074 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*46] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec  0/0     1956 pps
[ 46] Sent 19561 datagrams
[ 46] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*46] 0.00-10.02 sec  25.5 MBytes  21.3 Mbits/sec   0.736 ms 1370/19560 (7%) -/-/-/- ms 1951 pps
[ 47] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46962 (sock=4) (peer 2.1.6) on 2022-05-10 14:14:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 47] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec   0.455 ms 0/20411 (0%) 12.807/4.022/34.839/4.178 ms 2041 pps 234
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*48] local 10.0.23.217%eth0 port 49190 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*48] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec  0/0     2041 pps
[ 48] Sent 20411 datagrams
[ 48] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*48] 0.00-10.05 sec  20.5 MBytes  17.1 Mbits/sec   0.859 ms 5762/20410 (28%) -/-/-/- ms 2031 pps
[ 49] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 59903 (sock=3) (peer 2.1.6) on 2022-05-10 14:14:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 49] 0.00-10.01 sec  29.8 MBytes  25.0 Mbits/sec   0.392 ms 0/21262 (0%) 12.522/3.305/39.297/4.884 ms 2124 pps 249
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 470.40 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*50] local 10.0.23.217%eth0 port 42004 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*50] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec  0/0     2126 pps
[ 50] Sent 21262 datagrams
[ 50] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*50] 0.00-10.05 sec  25.9 MBytes  21.6 Mbits/sec   0.659 ms 2784/21261 (13%) -/-/-/- ms 2116 pps
[ 51] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 52754 (sock=4) (peer 2.1.6) on 2022-05-10 14:14:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 51] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec   0.446 ms 0/22112 (0%) 11.959/5.623/36.912/3.931 ms 2212 pps 272
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 452.31 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*52] local 10.0.23.217%eth0 port 42833 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*52] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec  0/0     2211 pps
[ 52] Sent 22112 datagrams
[ 52] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*52] 0.00-10.06 sec  25.0 MBytes  20.8 Mbits/sec   0.990 ms 4300/22111 (19%) -/-/-/- ms 2198 pps
[ 53] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45790 (sock=3) (peer 2.1.6) on 2022-05-10 14:15:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 53] 0.00-10.01 sec  32.2 MBytes  27.0 Mbits/sec   0.364 ms 0/22963 (0%) 11.205/-1.737/42.158/5.812 ms 2293 pps 301
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 435.56 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*54] local 10.0.23.217%eth0 port 58525 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*54] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec  0/0     2296 pps
[ 54] Sent 22962 datagrams
[ 54] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*54] 0.00-10.05 sec  24.2 MBytes  20.2 Mbits/sec   0.526 ms 5676/22961 (25%) -/-/-/- ms 2283 pps
[ 55] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 57514 (sock=4) (peer 2.1.6) on 2022-05-10 14:15:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 55] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec   0.399 ms 0/23813 (0%) 15.364/6.837/37.049/4.125 ms 2380 pps 228
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 420.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*56] local 10.0.23.217%eth0 port 53909 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*56] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec  0/0     2381 pps
[ 56] Sent 23813 datagrams
[ 56] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*56] 0.00-10.08 sec  19.7 MBytes  16.4 Mbits/sec   1.414 ms 9735/23812 (41%) -/-/-/- ms 2362 pps
[ 57] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38186 (sock=3) (peer 2.1.6) on 2022-05-10 14:15:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 57] 0.00-10.02 sec  34.6 MBytes  28.9 Mbits/sec   0.975 ms 0/24663 (0%) 6.081/0.283/26.815/4.000 ms 2461 pps 595
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 405.52 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*58] local 10.0.23.217%eth0 port 60940 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*58] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec  0/0     2466 pps
[ 58] Sent 24663 datagrams
[ 58] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*58] 0.00-10.13 sec  9.80 MBytes  8.11 Mbits/sec   2.703 ms 17675/24662 (72%) 118.127/1.024/297.633/0.454 ms 2435 pps 9
[ 59] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35413 (sock=4) (peer 2.1.6) on 2022-05-10 14:16:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 59] 0.00-10.01 sec  35.8 MBytes  30.0 Mbits/sec   0.680 ms 0/25514 (0%) 3.014/-3.944/27.578/4.588 ms 2548 pps 1242
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4523 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 392.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*60] local 10.0.23.217%eth0 port 49333 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*60] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec  0/0     2551 pps
[ 60] Sent 25513 datagrams
[ 60] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*60] 0.00-10.09 sec  8.29 MBytes  6.89 Mbits/sec   0.850 ms 19599/25512 (77%) 132.910/30.681/410.926/0.475 ms 2528 pps 6
