------------------------------------------------------------
Server listening on UDP port 5001 with pid 3534
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45212 (sock=3) (peer 2.1.6) on 2022-05-13 14:52:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.092 ms 0/854 (0%) -2.734/-2.990/0.437/0.300 ms 85 pps -46
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 44872 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.050 ms 0/853 (0%) 7.321/6.904/8.912/0.371 ms 85 pps 17
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35437 (sock=5) (peer 2.1.6) on 2022-05-13 14:52:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.016 ms 0/1279 (0%) -1.762/-2.022/3.144/0.268 ms 128 pps -107
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 40416 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.035 ms 0/1278 (0%) 6.323/5.939/10.094/0.323 ms 127 pps 30
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38599 (sock=3) (peer 2.1.6) on 2022-05-13 14:53:08 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.072 ms 0/1704 (0%) -1.138/-1.382/2.386/0.248 ms 170 pps -220
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 56311 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.031 ms 0/1703 (0%) 5.605/5.239/8.856/0.283 ms 170 pps 45
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57372 (sock=4) (peer 2.1.6) on 2022-05-13 14:53:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.029 ms 0/2129 (0%) -0.273/-0.406/2.849/0.207 ms 213 pps -1146
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 34812 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.019 ms 0/2128 (0%) 4.944/4.595/8.304/0.255 ms 212 pps 63
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34573 (sock=3) (peer 2.1.6) on 2022-05-13 14:53:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.088 ms 0/2554 (0%) 0.364/0.182/4.506/0.284 ms 255 pps 1032
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 56315 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.070 ms 0/2553 (0%) 4.366/4.041/8.654/0.299 ms 255 pps 86
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55550 (sock=4) (peer 2.1.6) on 2022-05-13 14:54:09 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.043 ms 0/2980 (0%) 0.717/0.407/4.050/0.344 ms 298 pps 610
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 37786 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.032 ms 0/2979 (0%) 4.122/3.786/7.514/0.280 ms 297 pps 106
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56084 (sock=3) (peer 2.1.6) on 2022-05-13 14:54:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.010 ms 0/3405 (0%) 0.792/0.519/4.457/0.391 ms 340 pps 632
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 37335 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.018 ms 0/3404 (0%) 4.090/3.702/7.629/0.299 ms 340 pps 122
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45125 (sock=4) (peer 2.1.6) on 2022-05-13 14:54:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.018 ms 0/3830 (0%) 1.184/0.886/6.511/0.617 ms 383 pps 475
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 42846 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.087 ms 0/3829 (0%) 3.607/3.221/7.072/0.329 ms 382 pps 156
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40216 (sock=3) (peer 2.1.6) on 2022-05-13 14:55:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.020 ms 0/4255 (0%) 1.870/1.261/7.538/0.968 ms 425 pps 334
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 40705 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.119 ms 0/4254 (0%) 3.337/2.925/7.083/0.368 ms 425 pps 187
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53496 (sock=4) (peer 2.1.6) on 2022-05-13 14:55:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.02 sec  6.37 MBytes  5.33 Mbits/sec   0.081 ms 136/4680 (2.9%) 43.501/2.017/67.418/13.822 ms 453 pps 15
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 55747 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.96 sec  6.56 MBytes  5.52 Mbits/sec   0.214 ms 0/4679 (0%) 31.613/17.980/55.740/0.724 ms 469 pps 22
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53344 (sock=3) (peer 2.1.6) on 2022-05-13 14:55:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.09 sec  6.38 MBytes  5.31 Mbits/sec   0.454 ms 553/5105 (11%) -/-/-/- ms 451 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 43632 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-9.99 sec  7.16 MBytes  6.01 Mbits/sec   0.035 ms 0/5104 (0%) -/-/-/- ms 510 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37461 (sock=4) (peer 2.1.6) on 2022-05-13 14:56:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.584 ms 980/5532 (18%) 73.163/10.018/77.942/6.897 ms 452 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 47073 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.04 sec  6.49 MBytes  5.42 Mbits/sec   0.035 ms 902/5530 (16%) 34.449/0.784/1687.946/0.485 ms 551 pps 20
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41517 (sock=3) (peer 2.1.6) on 2022-05-13 14:56:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.05 sec  6.38 MBytes  5.32 Mbits/sec   0.937 ms 1405/5956 (24%) 68.827/4.348/73.133/7.436 ms 453 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 49670 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.03 sec  7.84 MBytes  6.56 Mbits/sec   0.175 ms 360/5955 (6%) 58.688/19.610/72.900/0.783 ms 593 pps 14
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56466 (sock=4) (peer 2.1.6) on 2022-05-13 14:56:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.03 sec  6.39 MBytes  5.34 Mbits/sec   0.749 ms 1827/6382 (29%) 58.884/12.489/79.797/12.027 ms 454 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 46975 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.03 sec  7.85 MBytes  6.57 Mbits/sec   0.342 ms 778/6381 (12%) 88.107/39.664/107.538/0.847 ms 636 pps 9
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36244 (sock=3) (peer 2.1.6) on 2022-05-13 14:57:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.11 sec  6.41 MBytes  5.32 Mbits/sec   0.742 ms 2233/6806 (33%) 81.320/-7.376/104.705/14.940 ms 452 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 40815 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.04 sec  7.85 MBytes  6.56 Mbits/sec   0.561 ms 1204/6805 (18%) -/-/-/- ms 677 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51088 (sock=4) (peer 2.1.6) on 2022-05-13 14:57:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.05 sec  6.38 MBytes  5.33 Mbits/sec   0.659 ms 2678/7231 (37%) 110.960/53.311/121.250/6.667 ms 453 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 52901 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  7.88 MBytes  6.58 Mbits/sec   0.552 ms 1608/7231 (22%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54357 (sock=3) (peer 2.1.6) on 2022-05-13 14:57:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.579 ms 3105/7657 (41%) 101.737/34.428/104.231/4.839 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 42410 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  7.87 MBytes  6.57 Mbits/sec   0.614 ms 2041/7655 (27%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51222 (sock=4) (peer 2.1.6) on 2022-05-13 14:58:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.397 ms 3527/8082 (44%) 101.929/35.256/103.943/4.763 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 51886 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  7.88 MBytes  6.57 Mbits/sec   0.591 ms 2461/8081 (30%) -/-/-/- ms 803 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47008 (sock=3) (peer 2.1.6) on 2022-05-13 14:58:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.264 ms 3951/8507 (46%) 101.541/34.480/103.479/4.721 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3534 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 33252 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  7.88 MBytes  6.58 Mbits/sec   0.581 ms 2884/8506 (34%) -/-/-/- ms 846 pps
