------------------------------------------------------------
Server listening on UDP port 5001 with pid 2003
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58230 (sock=3) (peer 2.1.6) on 2022-05-13 12:30:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.036 ms 0/854 (0%) 2.380/2.258/5.029/0.214 ms 85 pps 53
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 47786 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.030 ms 0/853 (0%) 2.162/2.027/5.072/0.218 ms 85 pps 58
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59543 (sock=5) (peer 2.1.6) on 2022-05-13 12:30:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.046 ms 0/1279 (0%) 2.297/2.175/4.803/0.185 ms 128 pps 82
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 60206 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.023 ms 0/1278 (0%) 2.110/1.960/4.212/0.144 ms 127 pps 89
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46866 (sock=3) (peer 2.1.6) on 2022-05-13 12:31:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.026 ms 0/1704 (0%) 2.125/1.941/5.208/0.205 ms 170 pps 118
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 55733 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.068 ms 0/1703 (0%) 2.172/1.991/4.926/0.168 ms 170 pps 115
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44438 (sock=4) (peer 2.1.6) on 2022-05-13 12:31:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.014 ms 0/2129 (0%) 2.266/2.145/5.213/0.190 ms 213 pps 138
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 35657 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.029 ms 0/2128 (0%) 2.129/1.951/5.142/0.187 ms 212 pps 147
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46552 (sock=3) (peer 2.1.6) on 2022-05-13 12:31:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.013 ms 0/2554 (0%) 2.225/2.034/7.401/0.266 ms 255 pps 169
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 33741 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.047 ms 0/2553 (0%) 2.290/2.061/7.147/0.236 ms 255 pps 164
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51313 (sock=4) (peer 2.1.6) on 2022-05-13 12:32:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.008 ms 0/2980 (0%) 2.269/2.150/5.099/0.216 ms 298 pps 193
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 54286 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.101 ms 0/2979 (0%) 2.026/1.835/5.351/0.228 ms 297 pps 216
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41267 (sock=3) (peer 2.1.6) on 2022-05-13 12:32:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.039 ms 0/3405 (0%) 2.239/2.056/6.158/0.259 ms 340 pps 223
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 45383 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.020 ms 0/3404 (0%) 2.146/1.951/5.615/0.201 ms 340 pps 233
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46988 (sock=4) (peer 2.1.6) on 2022-05-13 12:32:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.033 ms 0/3830 (0%) 2.257/2.057/5.279/0.284 ms 383 pps 249
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 35644 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.040 ms 0/3829 (0%) 2.074/1.826/7.649/0.261 ms 382 pps 271
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58778 (sock=3) (peer 2.1.6) on 2022-05-13 12:33:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.043 ms 0/4255 (0%) 2.348/1.986/5.513/0.402 ms 425 pps 266
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 53459 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.219 ms 0/4254 (0%) 2.129/1.814/5.482/0.260 ms 425 pps 294
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60455 (sock=4) (peer 2.1.6) on 2022-05-13 12:33:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.029 ms 0/4680 (0%) 2.407/2.102/5.892/0.514 ms 468 pps 286
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 34267 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.083 ms 0/4679 (0%) 1.905/1.512/5.199/0.301 ms 467 pps 361
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53121 (sock=3) (peer 2.1.6) on 2022-05-13 12:33:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.015 ms 0/5105 (0%) 3.166/2.501/6.968/1.016 ms 510 pps 237
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 43760 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.072 ms 0/5104 (0%) 1.660/1.229/6.784/0.406 ms 510 pps 452
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36494 (sock=4) (peer 2.1.6) on 2022-05-13 12:34:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.05 sec  7.52 MBytes  6.28 Mbits/sec   0.081 ms 171/5532 (3.1%) 48.713/3.091/59.276/9.773 ms 534 pps 16
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 59904 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.99 sec  7.75 MBytes  6.51 Mbits/sec   0.023 ms 0/5530 (0%) 11.541/6.666/19.836/0.742 ms 553 pps 70
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34596 (sock=3) (peer 2.1.6) on 2022-05-13 12:34:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.03 sec  7.52 MBytes  6.29 Mbits/sec   0.351 ms 595/5956 (10%) 39.577/-2.205/55.109/9.291 ms 534 pps 20
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 51562 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.97 sec  8.35 MBytes  7.02 Mbits/sec   0.029 ms 0/5955 (0%) 22.772/12.340/40.190/0.361 ms 596 pps 39
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34095 (sock=4) (peer 2.1.6) on 2022-05-13 12:34:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.07 sec  7.52 MBytes  6.26 Mbits/sec   0.528 ms 1020/6381 (16%) 55.647/-7.514/63.999/7.315 ms 532 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 44841 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.00 sec  8.94 MBytes  7.51 Mbits/sec   0.131 ms 0/6380 (0%) -/-/-/- ms 638 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57231 (sock=3) (peer 2.1.6) on 2022-05-13 12:35:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.06 sec  7.54 MBytes  6.29 Mbits/sec   0.578 ms 1427/6806 (21%) 63.797/8.526/66.204/4.677 ms 535 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 41170 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.04 sec  9.02 MBytes  7.54 Mbits/sec   0.165 ms 371/6805 (5.5%) 43.058/2.305/46.442/0.779 ms 677 pps 22
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52810 (sock=4) (peer 2.1.6) on 2022-05-13 12:35:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.08 sec  7.52 MBytes  6.26 Mbits/sec   0.627 ms 1868/7231 (26%) 76.381/10.254/86.932/7.816 ms 532 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 47283 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  9.03 MBytes  7.54 Mbits/sec   0.312 ms 788/7230 (11%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60640 (sock=3) (peer 2.1.6) on 2022-05-13 12:35:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.06 sec  7.53 MBytes  6.28 Mbits/sec   0.648 ms 2288/7656 (30%) 85.568/29.274/87.678/4.439 ms 534 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 55450 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.04 sec  9.03 MBytes  7.54 Mbits/sec   0.382 ms 1212/7655 (16%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57558 (sock=4) (peer 2.1.6) on 2022-05-13 12:36:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  7.53 MBytes  6.28 Mbits/sec   0.611 ms 2714/8082 (34%) 85.259/28.412/86.860/4.164 ms 534 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 55410 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  9.02 MBytes  7.54 Mbits/sec   0.486 ms 1644/8081 (20%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49582 (sock=3) (peer 2.1.6) on 2022-05-13 12:36:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.06 sec  7.51 MBytes  6.27 Mbits/sec   0.578 ms 3149/8508 (37%) 84.552/28.537/86.333/3.571 ms 533 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 2003 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 57498 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  9.03 MBytes  7.54 Mbits/sec   0.555 ms 2064/8506 (24%) -/-/-/- ms 846 pps
