------------------------------------------------------------
Server listening on UDP port 5001 with pid 5011
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 33284 (sock=3) (peer 2.1.6) on 2022-05-10 14:53:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   3.774 ms 0/854 (0%) 7.088/2.989/37.785/4.656 ms 85 pps 18
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 58372 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.01 sec  1.20 MBytes  1.00 Mbits/sec   6.247 ms 0/853 (0%) -/-/-/- ms 85 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 55041 (sock=5) (peer 2.1.6) on 2022-05-10 14:53:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   2.602 ms 0/1704 (0%) 6.808/3.006/35.196/3.899 ms 170 pps 37
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 55449 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.03 sec  2.39 MBytes  2.00 Mbits/sec   7.709 ms 0/1703 (0%) -/-/-/- ms 169 pps
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 47140 (sock=3) (peer 2.1.6) on 2022-05-10 14:54:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.02 sec  3.58 MBytes  3.00 Mbits/sec   2.178 ms 0/2554 (0%) 8.693/4.161/48.756/5.042 ms 255 pps 43
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 36866 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.02 sec  3.58 MBytes  3.00 Mbits/sec   5.129 ms 0/2553 (0%) -/-/-/- ms 254 pps
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36005 (sock=4) (peer 2.1.6) on 2022-05-10 14:54:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  4.77 MBytes  4.00 Mbits/sec   2.839 ms 0/3405 (0%) 8.960/5.730/51.547/3.880 ms 340 pps 56
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 44905 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.01 sec  4.77 MBytes  4.00 Mbits/sec   3.662 ms 0/3404 (0%) -/-/-/- ms 340 pps
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 32937 (sock=3) (peer 2.1.6) on 2022-05-10 14:54:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.02 sec  5.97 MBytes  5.00 Mbits/sec   2.357 ms 0/4255 (0%) 8.700/4.693/36.458/4.403 ms 425 pps 72
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 47837 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.01 sec  5.96 MBytes  5.00 Mbits/sec   3.411 ms 0/4254 (0%) -/-/-/- ms 424 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 55172 (sock=4) (peer 2.1.6) on 2022-05-10 14:55:08 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   1.479 ms 0/5105 (0%) 9.464/4.331/62.434/5.839 ms 510 pps 79
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 46007 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-9.99 sec  7.16 MBytes  6.01 Mbits/sec   1.944 ms 0/5104 (0%) -/-/-/- ms 511 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51948 (sock=3) (peer 2.1.6) on 2022-05-10 14:55:28 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   1.656 ms 0/5956 (0%) 7.006/3.740/30.477/3.580 ms 595 pps 125
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 49672 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.02 sec  8.35 MBytes  6.99 Mbits/sec   2.546 ms 0/5955 (0%) -/-/-/- ms 594 pps
[ 15] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 34697 (sock=4) (peer 2.1.6) on 2022-05-10 14:55:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   1.380 ms 0/6806 (0%) 8.081/3.843/41.849/4.254 ms 680 pps 124
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.217%eth0 port 36530 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 16] Sent 6806 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.01 sec  9.54 MBytes  7.99 Mbits/sec   2.438 ms 0/6805 (0%) -/-/-/- ms 679 pps
[ 17] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35084 (sock=3) (peer 2.1.6) on 2022-05-10 14:56:09 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.01 sec  10.7 MBytes  9.00 Mbits/sec   1.410 ms 0/7656 (0%) 12.499/4.794/185.262/17.848 ms 765 pps 90
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.217%eth0 port 42969 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 18] Sent 7656 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec   1.671 ms 0/7655 (0%) -/-/-/- ms 765 pps
[ 19] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 48226 (sock=4) (peer 2.1.6) on 2022-05-10 14:56:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec   1.412 ms 0/8507 (0%) 8.482/3.851/46.337/5.118 ms 850 pps 147
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.217%eth0 port 50039 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 20] Sent 8507 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.01 sec  11.9 MBytes  9.99 Mbits/sec   1.978 ms 0/8506 (0%) -/-/-/- ms 849 pps
[ 21] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38625 (sock=3) (peer 2.1.6) on 2022-05-10 14:56:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec   1.204 ms 0/9357 (0%) 7.625/3.999/60.355/4.660 ms 935 pps 180
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1069.09 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.217%eth0 port 36203 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec  0/0      936 pps
[ 22] Sent 9357 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec   1.228 ms 33/9356 (0.35%) -/-/-/- ms 935 pps
[ 23] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46385 (sock=4) (peer 2.1.6) on 2022-05-10 14:57:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec   0.904 ms 0/10207 (0%) 10.213/4.463/80.858/6.669 ms 1021 pps 147
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 980.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.217%eth0 port 58013 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec  0/0     1021 pps
[ 24] Sent 10207 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.01 sec  14.3 MBytes  12.0 Mbits/sec   1.286 ms 0/10206 (0%) -/-/-/- ms 1020 pps
[ 25] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45457 (sock=3) (peer 2.1.6) on 2022-05-10 14:57:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec   0.923 ms 0/11058 (0%) 9.507/5.132/49.825/4.806 ms 1106 pps 171
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 904.62 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.217%eth0 port 43457 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec  0/0     1106 pps
[ 26] Sent 11058 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.03 sec  15.5 MBytes  13.0 Mbits/sec   3.528 ms 0/11057 (0%) -/-/-/- ms 1101 pps
[ 27] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 52907 (sock=4) (peer 2.1.6) on 2022-05-10 14:57:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec   0.942 ms 0/11908 (0%) 8.187/4.319/36.182/4.443 ms 1191 pps 214
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.217%eth0 port 48786 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec  0/0     1191 pps
[ 28] Sent 11908 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.02 sec  16.7 MBytes  14.0 Mbits/sec   1.320 ms 0/11907 (0%) -/-/-/- ms 1188 pps
[ 29] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 57602 (sock=3) (peer 2.1.6) on 2022-05-10 14:58:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec   0.836 ms 0/12758 (0%) 7.884/3.637/31.733/4.012 ms 1276 pps 238
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.217%eth0 port 56703 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[ 30] Sent 12758 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.01 sec  17.9 MBytes  15.0 Mbits/sec   1.282 ms 0/12757 (0%) -/-/-/- ms 1273 pps
[ 31] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 37441 (sock=4) (peer 2.1.6) on 2022-05-10 14:58:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.00 sec  18.6 MBytes  15.6 Mbits/sec   0.852 ms 364/13609 (2.7%) 13.912/3.505/303.166/30.704 ms 1324 pps 140
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 735.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.217%eth0 port 52227 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec  0/0     1361 pps
[ 32] Sent 13609 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.02 sec  18.6 MBytes  15.6 Mbits/sec   1.135 ms 320/13608 (2.4%) -/-/-/- ms 1357 pps
[ 33] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36091 (sock=3) (peer 2.1.6) on 2022-05-10 14:58:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec   0.727 ms 0/14459 (0%) 6.426/1.763/31.015/4.157 ms 1446 pps 331
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 691.76 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.217%eth0 port 58745 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec  0/0     1446 pps
[ 34] Sent 14459 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.01 sec  20.3 MBytes  17.0 Mbits/sec   0.758 ms 0/14458 (0%) -/-/-/- ms 1445 pps
[ 35] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 50705 (sock=4) (peer 2.1.6) on 2022-05-10 14:59:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.01 sec  21.5 MBytes  18.0 Mbits/sec   1.049 ms 0/15309 (0%) 10.219/4.357/38.753/4.523 ms 1530 pps 220
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 653.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.217%eth0 port 54455 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec  0/0     1531 pps
[ 36] Sent 15309 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.00 sec  21.3 MBytes  17.9 Mbits/sec   0.674 ms 134/15308 (0.88%) -/-/-/- ms 1531 pps
[ 37] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53661 (sock=3) (peer 2.1.6) on 2022-05-10 14:59:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.01 sec  22.6 MBytes  19.0 Mbits/sec   1.161 ms 22/16160 (0.14%) 9.050/3.634/99.241/7.655 ms 1613 pps 262
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 618.95 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.217%eth0 port 45844 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec  0/0     1616 pps
[ 38] Sent 16160 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.01 sec  22.7 MBytes  19.0 Mbits/sec   0.943 ms 0/16159 (0%) -/-/-/- ms 1614 pps
[ 39] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 44684 (sock=4) (peer 2.1.6) on 2022-05-10 14:59:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 39] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec   0.639 ms 0/17010 (0%) 8.146/3.673/36.699/4.354 ms 1701 pps 307
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 588.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*40] local 10.0.23.217%eth0 port 51803 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*40] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec  0/0     1701 pps
[ 40] Sent 17010 datagrams
[ 40] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*40] 0.00-10.02 sec  23.8 MBytes  20.0 Mbits/sec   1.606 ms 0/17009 (0%) -/-/-/- ms 1697 pps
[ 41] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36895 (sock=3) (peer 2.1.6) on 2022-05-10 15:00:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 41] 0.00-10.01 sec  25.0 MBytes  21.0 Mbits/sec   1.163 ms 0/17860 (0%) 8.024/3.362/42.060/4.136 ms 1784 pps 327
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 560.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*42] local 10.0.23.217%eth0 port 36614 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec  0/0     1786 pps
[ 42] Sent 17860 datagrams
[ 42] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*42] 0.00-9.95 sec  25.0 MBytes  21.1 Mbits/sec   0.584 ms 0/17859 (0%) -/-/-/- ms 1794 pps
[ 43] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40539 (sock=4) (peer 2.1.6) on 2022-05-10 15:00:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 43] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec   0.577 ms 0/18711 (0%) 9.047/4.647/42.967/5.144 ms 1871 pps 304
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 534.55 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*44] local 10.0.23.217%eth0 port 58723 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*44] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec  0/0     1871 pps
[ 44] Sent 18711 datagrams
[ 44] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*44] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec   0.453 ms 0/18710 (0%) -/-/-/- ms 1870 pps
[ 45] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51651 (sock=3) (peer 2.1.6) on 2022-05-10 15:00:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 45] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec   0.557 ms 0/19561 (0%) 7.718/4.206/31.681/3.446 ms 1956 pps 373
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 511.30 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*46] local 10.0.23.217%eth0 port 50981 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*46] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec  0/0     1956 pps
[ 46] Sent 19561 datagrams
[ 46] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*46] 0.00-10.02 sec  27.4 MBytes  23.0 Mbits/sec   0.823 ms 0/19560 (0%) -/-/-/- ms 1952 pps
[ 47] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 56624 (sock=4) (peer 2.1.6) on 2022-05-10 15:01:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 47] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec   0.440 ms 0/20411 (0%) 7.026/3.278/34.823/3.942 ms 2041 pps 427
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*48] local 10.0.23.217%eth0 port 46733 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*48] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec  0/0     2041 pps
[ 48] Sent 20411 datagrams
[ 48] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*48] 0.00-10.02 sec  28.6 MBytes  23.9 Mbits/sec   0.397 ms 0/20410 (0%) -/-/-/- ms 2036 pps
[ 49] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35048 (sock=3) (peer 2.1.6) on 2022-05-10 15:01:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 49] 0.00-10.01 sec  29.8 MBytes  25.0 Mbits/sec   0.713 ms 0/21262 (0%) 8.788/2.590/33.757/4.116 ms 2124 pps 355
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 470.40 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*50] local 10.0.23.217%eth0 port 34504 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*50] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec  0/0     2126 pps
[ 50] Sent 21262 datagrams
[ 50] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*50] 0.00-9.99 sec  29.8 MBytes  25.0 Mbits/sec   0.424 ms 0/21261 (0%) -/-/-/- ms 2127 pps
[ 51] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58611 (sock=4) (peer 2.1.6) on 2022-05-10 15:01:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 51] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec   0.691 ms 0/22112 (0%) 9.832/4.967/50.700/4.302 ms 2211 pps 330
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 452.31 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*52] local 10.0.23.217%eth0 port 38154 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*52] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec  0/0     2211 pps
[ 52] Sent 22112 datagrams
[ 52] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*52] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec   0.344 ms 0/22111 (0%) -/-/-/- ms 2210 pps
[ 53] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38246 (sock=3) (peer 2.1.6) on 2022-05-10 15:02:16 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 53] 0.00-10.02 sec  30.4 MBytes  25.4 Mbits/sec   0.768 ms 1292/22962 (5.6%) 19.074/4.800/535.080/36.527 ms 2163 pps 167
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 435.56 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*54] local 10.0.23.217%eth0 port 51600 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*54] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec  0/0     2296 pps
[ 54] Sent 22962 datagrams
[ 54] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*54] 0.00-10.01 sec  31.8 MBytes  26.6 Mbits/sec   0.840 ms 293/22961 (1.3%) -/-/-/- ms 2292 pps
[ 55] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38437 (sock=4) (peer 2.1.6) on 2022-05-10 15:02:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 55] 0.00-10.02 sec  32.8 MBytes  27.4 Mbits/sec   0.946 ms 447/23813 (1.9%) 18.200/8.056/119.701/11.032 ms 2332 pps 188
[ 57] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60605 (sock=3) (peer 2.1.6) on 2022-05-10 15:02:47 (CEST)
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5011 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 420.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*56] local 10.0.23.217%eth0 port 51942 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 57] 0.00-10.01 sec  33.7 MBytes  28.3 Mbits/sec   0.463 ms 611/24663 (2.5%) 15.197/6.647/75.086/8.283 ms 2403 pps 232
------------------------------------------------------------
Server listening on UDP port 5001 with pid 5125
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 39537 (sock=3) (peer 2.1.6) on 2022-05-10 15:03:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec   0.431 ms 0/24663 (0%) 7.080/1.538/57.344/6.195 ms 2467 pps 512
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5125 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 405.52 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 56887 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec  0/0     2466 pps
[  2] Sent 24663 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.00 sec  34.5 MBytes  29.0 Mbits/sec   0.317 ms 47/24662 (0.19%) -/-/-/- ms 2467 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60746 (sock=5) (peer 2.1.6) on 2022-05-10 15:04:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec   0.354 ms 0/25513 (0%) 11.172/4.101/47.835/5.781 ms 2551 pps 336
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 5125 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 392.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 37560 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec  0/0     2551 pps
[  4] Sent 25513 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.13 sec  27.6 MBytes  22.9 Mbits/sec   3.907 ms 5791/25512 (23%) -/-/-/- ms 2517 pps
