------------------------------------------------------------
Server listening on UDP port 5001 with pid 3836
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49708 (sock=3) (peer 2.1.6) on 2022-05-13 15:35:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.021 ms 0/854 (0%) 2.092/1.850/5.246/0.276 ms 85 pps 60
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 34093 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.043 ms 0/853 (0%) 2.925/2.653/6.491/0.271 ms 85 pps 43
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33924 (sock=5) (peer 2.1.6) on 2022-05-13 15:35:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.032 ms 0/1279 (0%) 2.233/2.057/4.885/0.206 ms 128 pps 84
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 38590 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.024 ms 0/1278 (0%) 2.765/2.503/5.906/0.210 ms 127 pps 68
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37705 (sock=3) (peer 2.1.6) on 2022-05-13 15:36:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.064 ms 0/1704 (0%) 2.305/2.056/5.502/0.242 ms 170 pps 109
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 52748 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.337 ms 0/1703 (0%) 2.643/2.408/6.369/0.198 ms 170 pps 95
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52294 (sock=4) (peer 2.1.6) on 2022-05-13 15:36:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.022 ms 0/2129 (0%) 2.429/2.205/5.931/0.228 ms 213 pps 129
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 52847 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.142 ms 0/2128 (0%) 2.617/2.376/5.655/0.205 ms 212 pps 119
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54759 (sock=3) (peer 2.1.6) on 2022-05-13 15:36:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.041 ms 0/2554 (0%) 2.367/2.097/7.040/0.291 ms 255 pps 159
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 55422 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.124 ms 0/2553 (0%) 2.598/2.308/6.347/0.282 ms 255 pps 144
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43046 (sock=4) (peer 2.1.6) on 2022-05-13 15:37:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.071 ms 0/2980 (0%) 2.508/2.237/6.119/0.317 ms 298 pps 175
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 51022 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.025 ms 0/2979 (0%) 2.522/2.273/6.367/0.236 ms 297 pps 174
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35220 (sock=3) (peer 2.1.6) on 2022-05-13 15:37:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.077 ms 0/3405 (0%) 2.402/2.096/5.908/0.403 ms 340 pps 208
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 37592 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.092 ms 0/3404 (0%) 2.483/2.161/6.680/0.307 ms 340 pps 201
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58317 (sock=4) (peer 2.1.6) on 2022-05-13 15:38:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.01 sec  5.37 MBytes  4.50 Mbits/sec   0.286 ms 0/3830 (0%) 2.440/2.122/6.241/0.547 ms 383 pps 231
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 60119 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.023 ms 0/3829 (0%) 2.440/2.167/6.510/0.311 ms 382 pps 231
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59127 (sock=3) (peer 2.1.6) on 2022-05-13 15:38:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.021 ms 0/4255 (0%) 2.898/2.302/7.130/0.902 ms 425 pps 216
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 55633 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.045 ms 0/4254 (0%) 2.345/1.960/6.223/0.375 ms 425 pps 267
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41267 (sock=4) (peer 2.1.6) on 2022-05-13 15:38:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.03 sec  6.37 MBytes  5.32 Mbits/sec   0.081 ms 140/4681 (3%) 47.327/2.966/68.176/13.101 ms 453 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 40258 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.97 sec  6.56 MBytes  5.52 Mbits/sec   0.124 ms 0/4679 (0%) 30.398/17.232/51.057/0.566 ms 469 pps 23
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58409 (sock=3) (peer 2.1.6) on 2022-05-13 15:39:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.09 sec  6.38 MBytes  5.31 Mbits/sec   0.422 ms 554/5105 (11%) -/-/-/- ms 451 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 53884 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  5.99 MBytes  5.03 Mbits/sec   0.025 ms 830/5104 (16%) -/-/-/- ms 510 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55935 (sock=4) (peer 2.1.6) on 2022-05-13 15:39:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.06 sec  6.37 MBytes  5.31 Mbits/sec   0.634 ms 984/5531 (18%) 73.592/10.736/78.473/6.804 ms 452 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 45257 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.02 sec  6.49 MBytes  5.43 Mbits/sec   0.043 ms 901/5530 (16%) 40.318/0.377/1685.885/0.760 ms 551 pps 17
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60923 (sock=3) (peer 2.1.6) on 2022-05-13 15:39:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.02 sec  6.38 MBytes  5.34 Mbits/sec   0.746 ms 1406/5956 (24%) 47.555/5.276/73.124/14.453 ms 454 pps 14
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 32790 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.01 sec  7.83 MBytes  6.56 Mbits/sec   0.236 ms 371/5955 (6.2%) 76.996/53.428/101.448/0.094 ms 595 pps 11
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60501 (sock=4) (peer 2.1.6) on 2022-05-13 15:40:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.08 sec  6.38 MBytes  5.31 Mbits/sec   0.756 ms 1830/6381 (29%) 74.983/2.740/103.665/7.104 ms 451 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 59416 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  7.88 MBytes  6.58 Mbits/sec   0.349 ms 762/6380 (12%) -/-/-/- ms 635 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49501 (sock=3) (peer 2.1.6) on 2022-05-13 15:40:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.08 sec  6.42 MBytes  5.34 Mbits/sec   0.739 ms 2227/6806 (33%) 97.802/26.076/104.313/6.747 ms 454 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 60736 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.05 sec  7.85 MBytes  6.55 Mbits/sec   0.656 ms 1205/6805 (18%) -/-/-/- ms 676 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44043 (sock=4) (peer 2.1.6) on 2022-05-13 15:40:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.670 ms 2676/7232 (37%) 103.927/38.305/108.099/5.078 ms 453 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 43558 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  7.86 MBytes  6.55 Mbits/sec   0.561 ms 1626/7230 (22%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44063 (sock=3) (peer 2.1.6) on 2022-05-13 15:41:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.562 ms 3102/7656 (41%) 102.193/35.030/108.375/4.983 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 37950 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  7.87 MBytes  6.57 Mbits/sec   0.641 ms 2043/7655 (27%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 44665 (sock=4) (peer 2.1.6) on 2022-05-13 15:41:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.461 ms 3524/8083 (44%) 102.038/35.083/104.006/4.775 ms 453 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 50129 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.06 sec  7.89 MBytes  6.58 Mbits/sec   0.615 ms 2457/8082 (30%) -/-/-/- ms 803 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42591 (sock=3) (peer 2.1.6) on 2022-05-13 15:41:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.07 sec  5.77 MBytes  4.81 Mbits/sec   0.437 ms 4389/8508 (52%) 102.271/34.655/175.228/7.191 ms 409 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3836 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 49003 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  7.88 MBytes  6.58 Mbits/sec   0.578 ms 2882/8506 (34%) -/-/-/- ms 846 pps
