------------------------------------------------------------
Server listening on UDP port 5001 with pid 3653
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54243 (sock=3) (peer 2.1.6) on 2022-05-13 15:09:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.085 ms 0/854 (0%) 1.841/1.683/4.591/0.194 ms 85 pps 68
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 53820 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.052 ms 0/853 (0%) 2.197/2.050/3.656/0.137 ms 85 pps 57
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58779 (sock=5) (peer 2.1.6) on 2022-05-13 15:10:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.011 ms 0/1279 (0%) 1.852/1.699/3.670/0.156 ms 128 pps 101
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 36963 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.040 ms 0/1278 (0%) 2.221/2.049/4.914/0.168 ms 127 pps 84
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48966 (sock=3) (peer 2.1.6) on 2022-05-13 15:10:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.012 ms 0/1704 (0%) 1.962/1.865/4.621/0.168 ms 170 pps 128
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 36837 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.045 ms 0/1703 (0%) 2.193/2.020/4.858/0.175 ms 170 pps 114
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48577 (sock=4) (peer 2.1.6) on 2022-05-13 15:11:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.029 ms 0/2129 (0%) 1.892/1.708/6.433/0.194 ms 213 pps 165
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 39596 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.039 ms 0/2128 (0%) 2.193/1.988/4.809/0.158 ms 212 pps 143
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45570 (sock=3) (peer 2.1.6) on 2022-05-13 15:11:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.152 ms 1/2554 (0.039%) 1.819/1.593/4.117/0.168 ms 255 pps 206
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 46624 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.072 ms 0/2553 (0%) 2.273/2.030/4.902/0.167 ms 255 pps 165
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58962 (sock=4) (peer 2.1.6) on 2022-05-13 15:11:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.011 ms 0/2980 (0%) 1.859/1.698/9.208/0.278 ms 298 pps 236
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 50875 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.034 ms 0/2979 (0%) 2.152/1.945/5.448/0.202 ms 297 pps 203
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56170 (sock=3) (peer 2.1.6) on 2022-05-13 15:12:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.013 ms 0/3405 (0%) 1.894/1.696/7.097/0.232 ms 340 pps 264
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 47522 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.01 sec  4.77 MBytes  4.00 Mbits/sec   0.167 ms 0/3404 (0%) 2.074/1.862/4.931/0.183 ms 340 pps 241
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57259 (sock=4) (peer 2.1.6) on 2022-05-13 15:12:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.056 ms 0/3830 (0%) 1.919/1.651/4.618/0.253 ms 383 pps 293
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 38446 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.051 ms 0/3829 (0%) 2.189/1.936/4.947/0.194 ms 382 pps 257
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54708 (sock=3) (peer 2.1.6) on 2022-05-13 15:12:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.024 ms 0/4255 (0%) 1.927/1.769/7.324/0.302 ms 425 pps 324
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 54111 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.031 ms 0/4254 (0%) 2.133/1.907/4.894/0.186 ms 425 pps 293
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34774 (sock=4) (peer 2.1.6) on 2022-05-13 15:13:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.201 ms 0/4680 (0%) 1.973/1.686/8.318/0.393 ms 468 pps 349
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 60357 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.043 ms 0/4679 (0%) 2.003/1.716/4.454/0.215 ms 467 pps 343
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36959 (sock=3) (peer 2.1.6) on 2022-05-13 15:13:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.248 ms 0/5105 (0%) 2.102/1.763/5.279/0.439 ms 510 pps 357
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 42949 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.021 ms 0/5104 (0%) 2.025/1.780/4.958/0.229 ms 510 pps 371
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40303 (sock=4) (peer 2.1.6) on 2022-05-13 15:13:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.025 ms 0/5531 (0%) 2.173/1.721/6.196/0.648 ms 553 pps 374
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 40932 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec   0.043 ms 0/5530 (0%) 2.004/1.716/4.884/0.268 ms 552 pps 405
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 55328 (sock=3) (peer 2.1.6) on 2022-05-13 15:14:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.03 sec  8.35 MBytes  6.98 Mbits/sec   0.040 ms 2/5956 (0.034%) 25.661/2.296/39.258/9.817 ms 593 pps 34
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 57567 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-9.98 sec  8.35 MBytes  7.02 Mbits/sec   0.234 ms 0/5955 (0%) 10.147/4.253/25.185/0.297 ms 596 pps 86
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35678 (sock=4) (peer 2.1.6) on 2022-05-13 15:14:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  8.39 MBytes  7.00 Mbits/sec   0.190 ms 393/6381 (6.2%) 50.517/-0.120/55.585/8.160 ms 595 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 33193 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec   0.032 ms 0/6380 (0%) -/-/-/- ms 638 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53700 (sock=3) (peer 2.1.6) on 2022-05-13 15:14:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.05 sec  8.44 MBytes  7.04 Mbits/sec   0.333 ms 786/6806 (12%) 52.994/3.674/64.138/5.777 ms 599 pps 17
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 47711 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.00 sec  7.88 MBytes  6.61 Mbits/sec   0.029 ms 1184/6805 (17%) 19.808/1.084/1788.289/0.429 ms 680 pps 42
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46870 (sock=4) (peer 2.1.6) on 2022-05-13 15:15:05 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.01 sec  8.40 MBytes  7.04 Mbits/sec   0.541 ms 1239/7231 (17%) 32.208/3.070/54.237/12.401 ms 599 pps 27
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 36364 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.01 sec  9.85 MBytes  8.25 Mbits/sec   0.072 ms 201/7230 (2.8%) 68.985/46.858/84.775/0.262 ms 722 pps 15
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47623 (sock=3) (peer 2.1.6) on 2022-05-13 15:15:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.05 sec  8.40 MBytes  7.01 Mbits/sec   0.513 ms 1664/7656 (22%) -/-/-/- ms 596 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 40715 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.02 sec  9.86 MBytes  8.25 Mbits/sec   0.199 ms 625/7655 (8.2%) 52.206/25.812/63.416/0.347 ms 764 pps 20
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45254 (sock=4) (peer 2.1.6) on 2022-05-13 15:15:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.08 sec  8.40 MBytes  6.99 Mbits/sec   0.545 ms 2093/8083 (26%) 68.379/6.530/80.761/8.111 ms 594 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 43687 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  9.88 MBytes  8.26 Mbits/sec   0.316 ms 1030/8081 (13%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47057 (sock=3) (peer 2.1.6) on 2022-05-13 15:16:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.05 sec  8.41 MBytes  7.02 Mbits/sec   0.575 ms 2505/8507 (29%) 79.284/29.228/85.810/3.769 ms 597 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3653 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 60908 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  9.89 MBytes  8.26 Mbits/sec   0.373 ms 1454/8506 (17%) -/-/-/- ms 846 pps
