------------------------------------------------------------
Server listening on UDP port 5001 with pid 1615
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36294 (sock=3) (peer 2.1.6) on 2022-05-13 11:24:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.016 ms 0/854 (0%) -0.678/-0.973/0.986/0.228 ms 85 pps -185
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 39374 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.044 ms 0/853 (0%) 4.564/4.251/7.284/0.309 ms 85 pps 27
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45329 (sock=5) (peer 2.1.6) on 2022-05-13 11:24:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.031 ms 0/1279 (0%) 0.274/0.129/2.859/0.173 ms 128 pps 686
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 38520 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.080 ms 0/1278 (0%) 4.026/3.740/6.927/0.224 ms 127 pps 47
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51503 (sock=3) (peer 2.1.6) on 2022-05-13 11:25:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.017 ms 0/1704 (0%) 0.714/0.549/3.329/0.182 ms 170 pps 351
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 46124 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.026 ms 0/1703 (0%) 3.646/3.398/6.642/0.208 ms 170 pps 69
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57234 (sock=4) (peer 2.1.6) on 2022-05-13 11:25:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.028 ms 0/2129 (0%) 1.016/0.904/4.097/0.182 ms 213 pps 308
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 48520 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.032 ms 0/2128 (0%) 3.380/3.146/9.882/0.241 ms 212 pps 93
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56653 (sock=3) (peer 2.1.6) on 2022-05-13 11:25:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.235 ms 0/2554 (0%) 1.278/1.079/4.158/0.205 ms 255 pps 294
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 56435 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.013 ms 0/2553 (0%) 3.082/2.842/6.118/0.209 ms 255 pps 122
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54986 (sock=4) (peer 2.1.6) on 2022-05-13 11:26:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.014 ms 0/2980 (0%) 1.461/1.287/4.291/0.221 ms 298 pps 300
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 34807 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.035 ms 0/2979 (0%) 2.799/2.552/5.720/0.216 ms 297 pps 156
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43187 (sock=3) (peer 2.1.6) on 2022-05-13 11:26:28 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.034 ms 0/3405 (0%) 1.567/1.339/4.422/0.268 ms 340 pps 319
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 41398 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.044 ms 0/3404 (0%) 2.734/2.480/6.534/0.245 ms 340 pps 183
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36113 (sock=4) (peer 2.1.6) on 2022-05-13 11:26:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.016 ms 0/3830 (0%) 1.814/1.567/9.235/0.433 ms 383 pps 310
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 49204 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.133 ms 0/3829 (0%) 2.541/2.241/6.444/0.275 ms 382 pps 221
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51339 (sock=3) (peer 2.1.6) on 2022-05-13 11:27:08 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.074 ms 0/4255 (0%) 2.015/1.646/5.563/0.450 ms 425 pps 310
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 35110 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.025 ms 0/4254 (0%) 2.586/2.292/7.214/0.283 ms 425 pps 242
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 33427 (sock=4) (peer 2.1.6) on 2022-05-13 11:27:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.028 ms 0/4680 (0%) 2.189/1.787/9.294/0.727 ms 468 pps 314
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 51131 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.042 ms 0/4679 (0%) 2.447/2.081/5.707/0.308 ms 467 pps 281
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50135 (sock=3) (peer 2.1.6) on 2022-05-13 11:27:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.030 ms 0/5105 (0%) 7.283/1.922/12.424/1.987 ms 510 pps 103
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 40004 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.076 ms 0/5104 (0%) 2.261/1.592/6.883/0.698 ms 510 pps 332
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35359 (sock=4) (peer 2.1.6) on 2022-05-13 11:28:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.199 ms 351/5531 (6.3%) 59.639/2.833/63.322/8.685 ms 515 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 59330 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.99 sec  7.75 MBytes  6.51 Mbits/sec   0.046 ms 0/5530 (0%) 1.965/1.692/10.661/0.592 ms 553 pps 414
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36017 (sock=3) (peer 2.1.6) on 2022-05-13 11:28:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.495 ms 778/5956 (13%) 60.875/2.772/63.273/6.147 ms 515 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 50817 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.02 sec  6.81 MBytes  5.70 Mbits/sec   0.139 ms 1098/5955 (18%) 21.054/1.499/1896.977/0.844 ms 594 pps 34
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54517 (sock=4) (peer 2.1.6) on 2022-05-13 11:28:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.584 ms 1201/6381 (19%) 61.112/2.914/63.768/5.764 ms 515 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 59209 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  8.74 MBytes  7.30 Mbits/sec   0.115 ms 148/6380 (2.3%) 45.743/6.588/58.536/0.434 ms 635 pps 20
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42024 (sock=3) (peer 2.1.6) on 2022-05-13 11:29:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.08 sec  7.28 MBytes  6.06 Mbits/sec   0.706 ms 1617/6807 (24%) 74.095/8.972/83.898/7.078 ms 515 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 52114 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.04 sec  8.76 MBytes  7.32 Mbits/sec   0.222 ms 555/6805 (8.2%) -/-/-/- ms 677 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58511 (sock=4) (peer 2.1.6) on 2022-05-13 11:29:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.06 sec  7.27 MBytes  6.06 Mbits/sec   0.587 ms 2048/7232 (28%) 87.241/30.174/90.063/4.690 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 50332 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  8.76 MBytes  7.31 Mbits/sec   0.442 ms 982/7230 (14%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52719 (sock=3) (peer 2.1.6) on 2022-05-13 11:29:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.06 sec  7.26 MBytes  6.06 Mbits/sec   0.660 ms 2476/7656 (32%) 86.163/27.498/110.847/4.698 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 46284 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  8.76 MBytes  7.31 Mbits/sec   0.448 ms 1406/7655 (18%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60749 (sock=4) (peer 2.1.6) on 2022-05-13 11:30:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  7.26 MBytes  6.06 Mbits/sec   0.613 ms 2901/8083 (36%) 86.320/27.651/87.999/4.337 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 38370 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  8.75 MBytes  7.31 Mbits/sec   0.531 ms 1837/8081 (23%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50272 (sock=3) (peer 2.1.6) on 2022-05-13 11:30:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.06 sec  7.27 MBytes  6.06 Mbits/sec   0.553 ms 3322/8508 (39%) 86.378/27.429/88.299/3.875 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1615 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 58638 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  8.77 MBytes  7.32 Mbits/sec   0.578 ms 2250/8506 (26%) -/-/-/- ms 846 pps
