------------------------------------------------------------
Server listening on UDP port 5001 with pid 4054
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37701 (sock=3) (peer 2.1.6) on 2022-05-13 16:06:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  4.17 MBytes  3.50 Mbits/sec   0.022 ms 2/2980 (0.067%) -5.767/-6.014/-2.569/0.254 ms 298 pps -76
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 43424 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[  2] Sent 2980 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.00 sec  4.18 MBytes  3.50 Mbits/sec   0.041 ms 0/2979 (0%) 9.253/8.699/12.397/0.379 ms 297 pps 47
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45933 (sock=5) (peer 2.1.6) on 2022-05-13 16:07:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  4.77 MBytes  4.00 Mbits/sec   0.036 ms 6/3405 (0.18%) -4.238/-4.452/-1.144/0.283 ms 340 pps -118
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 44527 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  4] Sent 3405 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.066 ms 0/3404 (0%) 8.025/7.463/11.158/0.379 ms 340 pps 62
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57727 (sock=3) (peer 2.1.6) on 2022-05-13 16:07:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  5.35 MBytes  4.48 Mbits/sec   0.249 ms 16/3830 (0.42%) -2.967/-3.274/2.708/0.389 ms 381 pps -189
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 32857 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[  6] Sent 3830 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.053 ms 0/3829 (0%) 7.032/6.410/10.300/0.407 ms 382 pps 80
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 32789 (sock=4) (peer 2.1.6) on 2022-05-13 16:07:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  5.95 MBytes  4.99 Mbits/sec   0.011 ms 12/4255 (0.28%) -1.979/-2.178/4.205/0.425 ms 424 pps -315
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 43069 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[  8] Sent 4255 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.046 ms 0/4254 (0%) 5.849/5.335/9.147/0.352 ms 425 pps 107
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52555 (sock=3) (peer 2.1.6) on 2022-05-13 16:08:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  6.55 MBytes  5.49 Mbits/sec   0.105 ms 10/4680 (0.21%) -0.839/-1.108/2.955/0.504 ms 467 pps -818
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 42343 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 10] Sent 4680 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.038 ms 0/4679 (0%) 4.832/4.448/7.747/0.317 ms 467 pps 142
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42602 (sock=4) (peer 2.1.6) on 2022-05-13 16:08:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.84 sec  5.28 MBytes  4.09 Mbits/sec  50.379 ms 1412/5180 (27%) 40.489/-4.901/1791.049/236.641 ms 347 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 50929 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-9.99 sec  7.16 MBytes  6.01 Mbits/sec   0.026 ms 0/5104 (0%) 6.661/5.366/18.040/0.371 ms 510 pps 113
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42722 (sock=3) (peer 2.1.6) on 2022-05-13 16:08:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.03 sec  7.51 MBytes  6.28 Mbits/sec   0.136 ms 174/5531 (3.1%) 37.499/-1.022/55.028/10.980 ms 534 pps 21
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 48747 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 14] Sent 5531 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-9.98 sec  7.75 MBytes  6.52 Mbits/sec   0.020 ms 0/5530 (0%) 27.869/16.881/42.672/0.703 ms 554 pps 29
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41974 (sock=4) (peer 2.1.6) on 2022-05-13 16:09:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.07 sec  7.49 MBytes  6.24 Mbits/sec   0.396 ms 613/5956 (10%) -/-/-/- ms 530 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 38250 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 16] Sent 5956 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   0.038 ms 0/5955 (0%) 1.375/0.719/4.910/0.523 ms 595 pps 637
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34253 (sock=3) (peer 2.1.6) on 2022-05-13 16:09:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.06 sec  7.49 MBytes  6.25 Mbits/sec   0.475 ms 1036/6381 (16%) 58.654/2.934/61.211/5.895 ms 531 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 33620 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 18] Sent 6381 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.04 sec  7.48 MBytes  6.25 Mbits/sec   0.037 ms 1046/6380 (16%) 28.860/1.930/1689.889/0.792 ms 635 pps 27
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40907 (sock=4) (peer 2.1.6) on 2022-05-13 16:09:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.06 sec  7.53 MBytes  6.28 Mbits/sec   0.570 ms 1436/6806 (21%) 58.917/2.413/64.515/5.084 ms 534 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 49452 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 20] Sent 6806 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.04 sec  9.02 MBytes  7.54 Mbits/sec   0.211 ms 371/6805 (5.5%) 44.204/2.933/55.092/0.330 ms 677 pps 21
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46320 (sock=3) (peer 2.1.6) on 2022-05-13 16:10:05 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.07 sec  7.51 MBytes  6.26 Mbits/sec   0.649 ms 1871/7231 (26%) 77.035/13.157/85.772/6.561 ms 532 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 37094 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 22] Sent 7231 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.04 sec  9.05 MBytes  7.56 Mbits/sec   0.304 ms 778/7230 (11%) -/-/-/- ms 719 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 32819 (sock=4) (peer 2.1.6) on 2022-05-13 16:10:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.06 sec  7.51 MBytes  6.26 Mbits/sec   0.652 ms 2300/7656 (30%) 83.795/27.495/85.839/4.274 ms 533 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 36159 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 24] Sent 7656 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.04 sec  9.04 MBytes  7.55 Mbits/sec   0.422 ms 1207/7655 (16%) -/-/-/- ms 762 pps
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41574 (sock=3) (peer 2.1.6) on 2022-05-13 16:10:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.03 sec  7.50 MBytes  6.27 Mbits/sec   0.623 ms 2730/8082 (34%) 71.879/26.890/84.504/7.295 ms 533 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 59723 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 26] Sent 8082 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.05 sec  9.01 MBytes  7.52 Mbits/sec   0.473 ms 1654/8081 (20%) 53.205/2.561/61.066/0.669 ms 804 pps 18
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54712 (sock=4) (peer 2.1.6) on 2022-05-13 16:11:05 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.08 sec  7.47 MBytes  6.21 Mbits/sec   0.582 ms 3183/8508 (37%) 74.363/6.398/86.566/7.844 ms 528 pps 10
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 4054 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 34373 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 28] Sent 8507 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  9.03 MBytes  7.54 Mbits/sec   0.506 ms 2064/8506 (24%) -/-/-/- ms 846 pps
