------------------------------------------------------------
Server listening on UDP port 5001 with pid 2413
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
------------------------------------------------------------
Server listening on UDP port 5001 with pid 3345
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 41048 (sock=3) (peer 2.1.6) on 2022-05-13 14:28:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.03 sec  1.20 MBytes  1.00 Mbits/sec   0.019 ms 0/854 (0%) 1523.326/1519.684/1526.986/52.088 ms 85 pps 0
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 45440 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.01 sec  1.20 MBytes  1.00 Mbits/sec   0.043 ms 0/853 (0%) -/-/-/- ms 85 pps
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56560 (sock=5) (peer 2.1.6) on 2022-05-13 14:29:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.02 sec  1.79 MBytes  1.50 Mbits/sec   0.041 ms 0/1279 (0%) 1538.377/1534.663/1542.899/42.992 ms 128 pps 0
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 55752 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.00 sec  1.79 MBytes  1.50 Mbits/sec   0.021 ms 0/1278 (0%) -/-/-/- ms 127 pps
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 60111 (sock=3) (peer 2.1.6) on 2022-05-13 14:29:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.02 sec  2.39 MBytes  2.00 Mbits/sec   0.020 ms 0/1704 (0%) 1553.231/1549.537/1558.057/37.610 ms 170 pps 0
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 41918 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.00 sec  2.39 MBytes  2.00 Mbits/sec   0.026 ms 0/1703 (0%) -/-/-/- ms 170 pps
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50219 (sock=4) (peer 2.1.6) on 2022-05-13 14:29:43 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.161 ms 0/2129 (0%) 1568.257/1564.556/1574.388/33.989 ms 213 pps 0
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 35735 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.057 ms 0/2128 (0%) -/-/-/- ms 212 pps
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47055 (sock=3) (peer 2.1.6) on 2022-05-13 14:30:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.01 sec  3.58 MBytes  3.00 Mbits/sec   0.076 ms 0/2554 (0%) 1583.160/1579.422/1599.322/31.341 ms 255 pps 0
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 57980 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.031 ms 0/2553 (0%) -/-/-/- ms 255 pps
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 58797 (sock=4) (peer 2.1.6) on 2022-05-13 14:30:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.012 ms 0/2980 (0%) 1597.983/1594.255/1603.870/29.290 ms 298 pps 0
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 38557 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-11.60 sec  4.18 MBytes  3.02 Mbits/sec   0.070 ms 0/2979 (0%) -/-/-/- ms 256 pps
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46165 (sock=3) (peer 2.1.6) on 2022-05-13 14:30:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.017 ms 0/3405 (0%) 2.733/2.359/6.359/0.433 ms 340 pps 183
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 48833 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.180 ms 0/3404 (0%) 2.155/1.900/7.121/0.313 ms 340 pps 232
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43391 (sock=4) (peer 2.1.6) on 2022-05-13 14:31:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.039 ms 0/3830 (0%) 2.886/2.554/7.232/0.573 ms 383 pps 195
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 47428 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.035 ms 0/3829 (0%) 2.124/1.873/5.754/0.276 ms 382 pps 265
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59682 (sock=3) (peer 2.1.6) on 2022-05-13 14:31:25 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.016 ms 0/4255 (0%) 2.992/2.331/7.792/0.954 ms 425 pps 209
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 38752 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-9.98 sec  5.96 MBytes  5.01 Mbits/sec   0.052 ms 0/4254 (0%) 2.551/2.059/21.265/0.631 ms 426 pps 246
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52842 (sock=4) (peer 2.1.6) on 2022-05-13 14:31:45 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.04 sec  6.37 MBytes  5.32 Mbits/sec   0.105 ms 137/4680 (2.9%) 50.761/2.861/68.197/11.811 ms 453 pps 13
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 55305 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.98 sec  6.56 MBytes  5.51 Mbits/sec   0.033 ms 0/4679 (0%) 31.914/19.796/47.235/0.180 ms 468 pps 22
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56244 (sock=3) (peer 2.1.6) on 2022-05-13 14:32:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.09 sec  6.38 MBytes  5.30 Mbits/sec   0.839 ms 556/5105 (11%) -/-/-/- ms 451 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 52136 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-9.99 sec  7.16 MBytes  6.01 Mbits/sec   0.071 ms 0/5104 (0%) -/-/-/- ms 510 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50904 (sock=4) (peer 2.1.6) on 2022-05-13 14:32:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.641 ms 979/5531 (18%) 73.028/8.238/76.361/6.921 ms 452 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 38934 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.02 sec  6.49 MBytes  5.43 Mbits/sec   0.074 ms 903/5530 (16%) -/-/-/- ms 551 pps
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 40309 (sock=3) (peer 2.1.6) on 2022-05-13 14:32:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.04 sec  6.38 MBytes  5.33 Mbits/sec   0.692 ms 1408/5957 (24%) 59.308/8.223/76.102/9.941 ms 453 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 34896 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.04 sec  7.86 MBytes  6.57 Mbits/sec   0.192 ms 345/5955 (5.8%) 85.860/32.581/102.294/0.848 ms 592 pps 10
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37580 (sock=4) (peer 2.1.6) on 2022-05-13 14:33:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.12 sec  6.38 MBytes  5.29 Mbits/sec   0.741 ms 1830/6382 (29%) -/-/-/- ms 450 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 33006 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  7.86 MBytes  6.56 Mbits/sec   0.362 ms 776/6380 (12%) -/-/-/- ms 635 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48904 (sock=3) (peer 2.1.6) on 2022-05-13 14:33:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.06 sec  6.41 MBytes  5.34 Mbits/sec   0.743 ms 2235/6806 (33%) 103.811/41.293/109.146/5.354 ms 454 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 54769 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.611 ms 1197/6805 (18%) -/-/-/- ms 676 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39773 (sock=4) (peer 2.1.6) on 2022-05-13 14:33:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.07 sec  5.77 MBytes  4.81 Mbits/sec   0.672 ms 3114/7231 (43%) 100.623/34.425/186.116/8.557 ms 409 pps 6
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 58640 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.546 ms 1621/7231 (22%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 57234 (sock=3) (peer 2.1.6) on 2022-05-13 14:34:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.626 ms 3106/7657 (41%) 99.780/32.996/102.551/4.939 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 60263 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  7.88 MBytes  6.58 Mbits/sec   0.613 ms 2032/7655 (27%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 50214 (sock=4) (peer 2.1.6) on 2022-05-13 14:34:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.429 ms 3530/8082 (44%) 99.673/32.662/101.713/4.793 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 49819 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.04 sec  7.88 MBytes  6.58 Mbits/sec   0.598 ms 2460/8081 (30%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51669 (sock=3) (peer 2.1.6) on 2022-05-13 14:34:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.318 ms 3951/8508 (46%) 99.690/32.561/104.535/4.654 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3345 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 38706 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.06 sec  7.89 MBytes  6.58 Mbits/sec   0.594 ms 2881/8507 (34%) -/-/-/- ms 845 pps
