------------------------------------------------------------
Server listening on UDP port 5001 with pid 2237
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 53053 (sock=3) (peer 2.1.6) on 2022-05-04 12:51:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.00 sec  1.20 MBytes  1.00 Mbits/sec   4.626 ms 0/854 (0%) 12.701/7.700/45.448/5.289 ms 85 pps 10
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 50964 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.04 sec  1.20 MBytes  0.999 Mbits/sec   6.259 ms 0/853 (0%) -/-/-/- ms 84 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46019 (sock=5) (peer 2.1.6) on 2022-05-04 12:52:08 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   3.023 ms 0/1704 (0%) 10.490/6.528/53.284/5.089 ms 170 pps 24
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 59814 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   3.789 ms 0/1703 (0%) -/-/-/- ms 170 pps
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 42731 (sock=3) (peer 2.1.6) on 2022-05-04 12:52:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   1.939 ms 0/2554 (0%) 10.567/6.248/49.517/4.558 ms 255 pps 36
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 47731 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   2.029 ms 0/2553 (0%) -/-/-/- ms 255 pps
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 32875 (sock=4) (peer 2.1.6) on 2022-05-04 12:52:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.02 sec  4.77 MBytes  4.00 Mbits/sec   3.638 ms 0/3405 (0%) 8.571/4.634/38.882/4.329 ms 340 pps 58
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 47721 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.02 sec  4.77 MBytes  4.00 Mbits/sec   3.171 ms 0/3404 (0%) -/-/-/- ms 339 pps
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 56765 (sock=3) (peer 2.1.6) on 2022-05-04 12:53:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   2.198 ms 0/4255 (0%) 7.151/3.886/30.675/3.317 ms 425 pps 87
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 38554 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   2.700 ms 0/4254 (0%) -/-/-/- ms 425 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 56078 (sock=4) (peer 2.1.6) on 2022-05-04 12:53:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  7.16 MBytes  6.00 Mbits/sec   1.255 ms 0/5105 (0%) 7.253/3.467/28.345/3.795 ms 510 pps 103
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 51800 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-9.99 sec  7.16 MBytes  6.01 Mbits/sec   1.723 ms 0/5104 (0%) -/-/-/- ms 510 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38406 (sock=3) (peer 2.1.6) on 2022-05-04 12:53:50 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.01 sec  8.35 MBytes  7.00 Mbits/sec   1.854 ms 0/5956 (0%) 7.322/3.271/36.170/4.292 ms 595 pps 119
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 35503 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   1.528 ms 0/5955 (0%) -/-/-/- ms 595 pps
[ 15] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 49445 (sock=4) (peer 2.1.6) on 2022-05-04 12:54:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   1.253 ms 0/6806 (0%) 6.271/2.687/28.486/3.805 ms 680 pps 159
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.217%eth0 port 59589 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 16] Sent 6806 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.01 sec  9.54 MBytes  7.99 Mbits/sec   2.278 ms 0/6805 (0%) -/-/-/- ms 679 pps
[ 17] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36714 (sock=3) (peer 2.1.6) on 2022-05-04 12:54:31 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec   1.176 ms 0/7656 (0%) 6.206/2.665/29.663/3.911 ms 765 pps 181
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.217%eth0 port 51928 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 18] Sent 7656 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec   2.160 ms 0/7655 (0%) -/-/-/- ms 765 pps
[ 19] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 48907 (sock=4) (peer 2.1.6) on 2022-05-04 12:54:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec   1.237 ms 0/8507 (0%) 6.449/2.282/23.614/3.907 ms 851 pps 194
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.217%eth0 port 34896 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 20] Sent 8507 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.99 sec  11.9 MBytes  10.0 Mbits/sec   1.141 ms 0/8506 (0%) 4.861/0.115/40.086/0.626 ms 851 pps 257
[ 21] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35117 (sock=3) (peer 2.1.6) on 2022-05-04 12:55:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec   1.059 ms 0/9357 (0%) 5.748/2.056/29.154/3.596 ms 935 pps 239
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1069.09 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.217%eth0 port 47025 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec  0/0      936 pps
[ 22] Sent 9357 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.05 sec  13.1 MBytes  11.0 Mbits/sec   3.563 ms 0/9356 (0%) 5.412/0.103/56.217/0.250 ms 931 pps 253
[ 23] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58321 (sock=4) (peer 2.1.6) on 2022-05-04 12:55:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec   1.259 ms 0/10207 (0%) 5.991/2.211/35.551/3.849 ms 1020 pps 250
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 980.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.217%eth0 port 41021 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec  0/0     1021 pps
[ 24] Sent 10207 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec   1.291 ms 0/10206 (0%) 5.521/0.225/32.784/0.288 ms 1021 pps 272
[ 25] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 58189 (sock=3) (peer 2.1.6) on 2022-05-04 12:55:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.01 sec  15.5 MBytes  13.0 Mbits/sec   1.168 ms 0/11058 (0%) 6.410/1.942/34.136/4.113 ms 1105 pps 253
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 904.62 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.217%eth0 port 38773 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec  0/0     1106 pps
[ 26] Sent 11058 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.01 sec  15.5 MBytes  13.0 Mbits/sec   1.410 ms 0/11057 (0%) 8.169/0.311/51.870/0.405 ms 1104 pps 199
[ 27] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 37392 (sock=4) (peer 2.1.6) on 2022-05-04 12:56:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec   0.902 ms 0/11908 (0%) 6.952/2.464/35.402/4.114 ms 1191 pps 252
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.217%eth0 port 59553 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec  0/0     1191 pps
[ 28] Sent 11908 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.01 sec  16.7 MBytes  14.0 Mbits/sec   1.228 ms 0/11907 (0%) -/-/-/- ms 1190 pps
[ 29] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45372 (sock=3) (peer 2.1.6) on 2022-05-04 12:56:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec   1.087 ms 0/12758 (0%) 7.528/2.982/34.685/4.031 ms 1276 pps 249
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.217%eth0 port 56706 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[ 30] Sent 12758 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.01 sec  17.9 MBytes  15.0 Mbits/sec   1.371 ms 0/12757 (0%) -/-/-/- ms 1274 pps
[ 31] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46541 (sock=4) (peer 2.1.6) on 2022-05-04 12:56:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec   1.111 ms 0/13609 (0%) 5.967/1.764/28.956/3.878 ms 1361 pps 335
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 735.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.217%eth0 port 55912 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec  0/0     1361 pps
[ 32] Sent 13609 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec   1.180 ms 0/13608 (0%) 5.977/0.032/48.538/0.426 ms 1360 pps 335
[ 33] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51782 (sock=3) (peer 2.1.6) on 2022-05-04 12:57:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec   0.796 ms 0/14459 (0%) 6.044/1.660/28.901/4.094 ms 1445 pps 352
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 691.76 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.217%eth0 port 40765 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec  0/0     1446 pps
[ 34] Sent 14459 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec   1.004 ms 0/14458 (0%) 7.621/1.067/46.194/0.300 ms 1445 pps 279
[ 35] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 59969 (sock=4) (peer 2.1.6) on 2022-05-04 12:57:35 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec   0.669 ms 0/15309 (0%) 5.940/1.434/28.084/4.312 ms 1531 pps 379
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 653.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.217%eth0 port 46347 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec  0/0     1531 pps
[ 36] Sent 15309 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.03 sec  21.5 MBytes  18.0 Mbits/sec   1.648 ms 0/15308 (0%) 9.218/1.106/49.314/0.126 ms 1526 pps 243
[ 37] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45733 (sock=3) (peer 2.1.6) on 2022-05-04 12:57:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec   0.833 ms 0/16160 (0%) 6.891/1.777/35.683/4.654 ms 1615 pps 345
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 618.95 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.217%eth0 port 45553 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec  0/0     1616 pps
[ 38] Sent 16160 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec   0.709 ms 0/16159 (0%) 8.373/0.300/48.801/0.176 ms 1615 pps 284
[ 39] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 42967 (sock=4) (peer 2.1.6) on 2022-05-04 12:58:16 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 39] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec   0.667 ms 0/17010 (0%) 7.219/2.354/35.883/4.337 ms 1701 pps 346
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 588.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*40] local 10.0.23.217%eth0 port 33204 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*40] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec  0/0     1701 pps
[ 40] Sent 17010 datagrams
[ 40] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*40] 0.00-10.02 sec  23.8 MBytes  20.0 Mbits/sec   1.168 ms 0/17009 (0%) -/-/-/- ms 1698 pps
[ 41] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 45082 (sock=3) (peer 2.1.6) on 2022-05-04 12:58:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 41] 0.00-10.01 sec  25.0 MBytes  21.0 Mbits/sec   0.564 ms 0/17861 (0%) 7.007/2.777/28.921/3.767 ms 1785 pps 375
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 560.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*42] local 10.0.23.217%eth0 port 57572 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec  0/0     1786 pps
[ 42] Sent 17860 datagrams
[ 42] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec   0.688 ms 0/17859 (0%) 5.889/0.069/41.361/0.437 ms 1785 pps 446
[ 43] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60421 (sock=4) (peer 2.1.6) on 2022-05-04 12:58:57 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 43] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec   0.518 ms 0/18711 (0%) 7.133/3.012/30.265/3.829 ms 1871 pps 386
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 534.55 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*44] local 10.0.23.217%eth0 port 42274 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*44] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec  0/0     1871 pps
[ 44] Sent 18711 datagrams
[ 44] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*44] 0.00-10.01 sec  26.2 MBytes  22.0 Mbits/sec   0.795 ms 0/18710 (0%) -/-/-/- ms 1869 pps
[ 45] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 59427 (sock=3) (peer 2.1.6) on 2022-05-04 12:59:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 45] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec   0.560 ms 0/19561 (0%) 6.347/2.118/34.596/3.801 ms 1956 pps 453
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 511.30 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*46] local 10.0.23.217%eth0 port 47202 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*46] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec  0/0     1956 pps
[ 46] Sent 19561 datagrams
[ 46] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*46] 0.00-10.01 sec  27.4 MBytes  23.0 Mbits/sec   1.048 ms 0/19560 (0%) 7.140/0.920/44.113/0.396 ms 1954 pps 402
[ 47] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40963 (sock=4) (peer 2.1.6) on 2022-05-04 12:59:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 47] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec   0.544 ms 0/20411 (0%) 6.235/2.019/34.592/3.917 ms 2041 pps 481
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*48] local 10.0.23.217%eth0 port 54461 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*48] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec  0/0     2041 pps
[ 48] Sent 20411 datagrams
[ 48] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*48] 0.00-10.01 sec  28.6 MBytes  24.0 Mbits/sec   0.644 ms 0/20410 (0%) 5.574/0.198/36.671/0.351 ms 2039 pps 538
[ 49] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51089 (sock=3) (peer 2.1.6) on 2022-05-04 12:59:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 49] 0.00-9.99 sec  29.8 MBytes  25.0 Mbits/sec   0.726 ms 0/21262 (0%) 7.229/1.627/41.421/4.962 ms 2128 pps 433
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 470.40 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*50] local 10.0.23.217%eth0 port 45970 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*50] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec  0/0     2126 pps
[ 50] Sent 21262 datagrams
[ 50] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*50] 0.00-10.01 sec  29.8 MBytes  25.0 Mbits/sec   1.117 ms 0/21261 (0%) 6.441/0.626/41.033/0.271 ms 2123 pps 485
[ 51] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36151 (sock=4) (peer 2.1.6) on 2022-05-04 13:00:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 51] 0.00-9.99 sec  31.0 MBytes  26.0 Mbits/sec   0.465 ms 0/22112 (0%) 7.293/1.911/28.890/4.155 ms 2213 pps 446
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 452.31 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*52] local 10.0.23.217%eth0 port 47626 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*52] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec  0/0     2211 pps
[ 52] Sent 22112 datagrams
[ 52] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*52] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec   0.561 ms 0/22111 (0%) -/-/-/- ms 2210 pps
[ 53] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51932 (sock=3) (peer 2.1.6) on 2022-05-04 13:00:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 53] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec   0.382 ms 0/22962 (0%) 8.011/2.945/29.731/4.090 ms 2296 pps 421
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 435.56 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*54] local 10.0.23.217%eth0 port 50783 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*54] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec  0/0     2296 pps
[ 54] Sent 22962 datagrams
[ 54] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*54] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec   0.442 ms 0/22961 (0%) 6.205/0.304/43.832/0.175 ms 2295 pps 544
[ 55] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 50141 (sock=4) (peer 2.1.6) on 2022-05-04 13:00:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 55] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec   0.516 ms 0/23813 (0%) 6.710/2.185/35.308/4.040 ms 2380 pps 522
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 420.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*56] local 10.0.23.217%eth0 port 43224 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*56] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec  0/0     2381 pps
[ 56] Sent 23813 datagrams
[ 56] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*56] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec   0.452 ms 0/23812 (0%) 5.570/0.002/42.194/0.227 ms 2380 pps 628
[ 57] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46027 (sock=3) (peer 2.1.6) on 2022-05-04 13:01:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 57] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec   0.754 ms 0/24663 (0%) 6.444/2.173/29.801/3.700 ms 2466 pps 563
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 405.52 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*58] local 10.0.23.217%eth0 port 52915 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*58] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec  0/0     2466 pps
[ 58] Sent 24663 datagrams
[ 58] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*58] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec   0.424 ms 0/24662 (0%) 6.347/0.186/42.876/0.287 ms 2466 pps 571
[ 59] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40584 (sock=4) (peer 2.1.6) on 2022-05-04 13:01:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 59] 0.00-10.01 sec  35.8 MBytes  30.0 Mbits/sec   0.676 ms 0/25513 (0%) 6.355/2.198/29.431/3.893 ms 2550 pps 590
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 2237 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 392.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*60] local 10.0.23.217%eth0 port 34435 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*60] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec  0/0     2551 pps
[ 60] Sent 25513 datagrams
[ 60] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*60] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec   0.660 ms 0/25512 (0%) 6.813/1.140/53.415/0.279 ms 2550 pps 550
