------------------------------------------------------------
Server listening on UDP port 5001 with pid 1671
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37565 (sock=3) (peer 2.1.6) on 2022-05-13 11:32:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.196 ms 0/854 (0%) 1.723/1.549/3.765/0.162 ms 85 pps 73
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 41369 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.036 ms 0/853 (0%) 3.123/2.945/6.452/0.249 ms 85 pps 40
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52302 (sock=5) (peer 2.1.6) on 2022-05-13 11:33:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.016 ms 0/1279 (0%) 1.809/1.643/6.452/0.248 ms 128 pps 104
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 51479 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.035 ms 0/1278 (0%) 3.099/2.872/5.892/0.214 ms 127 pps 61
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 51208 (sock=3) (peer 2.1.6) on 2022-05-13 11:33:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.010 ms 0/1704 (0%) 1.834/1.602/5.074/0.242 ms 170 pps 137
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 50813 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.076 ms 0/1703 (0%) 2.973/2.711/6.453/0.260 ms 170 pps 84
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43841 (sock=4) (peer 2.1.6) on 2022-05-13 11:33:41 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.017 ms 0/2129 (0%) 2.043/1.828/5.200/0.233 ms 213 pps 153
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 44554 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.078 ms 0/2128 (0%) 2.941/2.685/6.469/0.231 ms 212 pps 106
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47861 (sock=3) (peer 2.1.6) on 2022-05-13 11:34:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.024 ms 0/2554 (0%) 2.064/1.785/5.248/0.267 ms 255 pps 182
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 53184 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.030 ms 0/2553 (0%) 2.875/2.587/6.174/0.221 ms 255 pps 131
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 47758 (sock=4) (peer 2.1.6) on 2022-05-13 11:34:22 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.127 ms 0/2980 (0%) 2.076/1.845/5.645/0.321 ms 298 pps 211
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 36445 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.167 ms 0/2979 (0%) 2.790/2.518/6.565/0.250 ms 297 pps 157
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59453 (sock=3) (peer 2.1.6) on 2022-05-13 11:34:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.035 ms 0/3405 (0%) 2.276/2.057/6.143/0.394 ms 340 pps 220
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 37962 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.032 ms 0/3404 (0%) 2.537/2.175/6.257/0.295 ms 340 pps 197
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56188 (sock=4) (peer 2.1.6) on 2022-05-13 11:35:03 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.059 ms 0/3830 (0%) 2.643/2.235/7.268/0.554 ms 383 pps 213
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 58332 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.032 ms 0/3829 (0%) 2.496/2.248/6.110/0.289 ms 382 pps 225
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 42696 (sock=3) (peer 2.1.6) on 2022-05-13 11:35:23 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   0.026 ms 0/4255 (0%) 2.705/2.035/7.021/0.918 ms 425 pps 231
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 39333 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.032 ms 0/4254 (0%) 2.611/2.218/6.143/0.372 ms 425 pps 239
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 54188 (sock=4) (peer 2.1.6) on 2022-05-13 11:35:44 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.03 sec  6.37 MBytes  5.33 Mbits/sec   0.108 ms 138/4680 (2.9%) 45.040/2.735/68.406/13.407 ms 453 pps 15
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 50282 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-9.97 sec  6.56 MBytes  5.52 Mbits/sec   0.041 ms 0/4679 (0%) 30.647/17.458/49.263/0.936 ms 469 pps 23
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 36458 (sock=3) (peer 2.1.6) on 2022-05-13 11:36:04 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.09 sec  6.38 MBytes  5.31 Mbits/sec   0.422 ms 551/5105 (11%) -/-/-/- ms 452 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 45217 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-9.99 sec  7.16 MBytes  6.01 Mbits/sec   0.034 ms 0/5104 (0%) -/-/-/- ms 510 pps
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38022 (sock=4) (peer 2.1.6) on 2022-05-13 11:36:24 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.07 sec  6.38 MBytes  5.31 Mbits/sec   0.579 ms 981/5531 (18%) 71.319/5.524/73.819/7.171 ms 452 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 57813 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-11.47 sec  7.50 MBytes  5.49 Mbits/sec  29.453 ms 243/5596 (4.3%) -/-/-/- ms 487 pps
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 34155 (sock=3) (peer 2.1.6) on 2022-05-13 11:36:46 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.07 sec  6.38 MBytes  5.31 Mbits/sec   0.743 ms 1406/5956 (24%) 71.774/5.251/75.469/6.225 ms 452 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 37089 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.05 sec  7.85 MBytes  6.56 Mbits/sec   0.197 ms 352/5955 (5.9%) 51.000/3.069/61.257/0.432 ms 592 pps 16
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53295 (sock=4) (peer 2.1.6) on 2022-05-13 11:37:06 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.09 sec  6.38 MBytes  5.30 Mbits/sec   0.745 ms 1831/6381 (29%) 90.032/13.334/101.872/8.977 ms 451 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 57105 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.06 sec  7.86 MBytes  6.56 Mbits/sec   0.347 ms 771/6381 (12%) -/-/-/- ms 634 pps
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35540 (sock=3) (peer 2.1.6) on 2022-05-13 11:37:26 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.07 sec  6.42 MBytes  5.35 Mbits/sec   0.720 ms 2230/6806 (33%) 99.507/33.417/101.559/5.365 ms 455 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 34067 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.06 sec  7.86 MBytes  6.56 Mbits/sec   0.476 ms 1195/6805 (18%) -/-/-/- ms 676 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39482 (sock=4) (peer 2.1.6) on 2022-05-13 11:37:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.688 ms 2676/7232 (37%) 99.299/34.630/101.932/4.920 ms 453 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 37010 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  7.87 MBytes  6.57 Mbits/sec   0.549 ms 1618/7231 (22%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 38194 (sock=3) (peer 2.1.6) on 2022-05-13 11:38:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.07 sec  6.38 MBytes  5.32 Mbits/sec   0.615 ms 3104/7656 (41%) 99.119/32.156/102.194/4.955 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 34800 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.05 sec  7.86 MBytes  6.56 Mbits/sec   0.604 ms 2046/7655 (27%) -/-/-/- ms 761 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49404 (sock=4) (peer 2.1.6) on 2022-05-13 11:38:27 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.465 ms 3525/8083 (44%) 98.937/31.778/100.776/4.814 ms 453 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 38699 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  7.87 MBytes  6.57 Mbits/sec   0.625 ms 2468/8081 (31%) -/-/-/- ms 803 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 39977 (sock=3) (peer 2.1.6) on 2022-05-13 11:38:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.07 sec  6.39 MBytes  5.32 Mbits/sec   0.262 ms 3952/8507 (46%) 99.021/32.929/103.887/4.585 ms 452 pps 7
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 1671 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 42293 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.05 sec  7.88 MBytes  6.58 Mbits/sec   0.596 ms 2882/8506 (34%) -/-/-/- ms 846 pps
