------------------------------------------------------------
Server listening on UDP port 5001 with pid 4645
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60532 (sock=3) (peer 2.1.6) on 2022-05-10 14:18:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.01 sec  1.20 MBytes  1.00 Mbits/sec   1.596 ms 0/854 (0%) 6.704/3.792/29.428/3.001 ms 85 pps 19
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 43357 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.03 sec  1.20 MBytes  1.00 Mbits/sec   7.113 ms 0/853 (0%) -/-/-/- ms 85 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 43520 (sock=5) (peer 2.1.6) on 2022-05-10 14:18:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.02 sec  2.39 MBytes  2.00 Mbits/sec   1.828 ms 0/1704 (0%) 5.102/2.581/18.483/2.129 ms 170 pps 49
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 45662 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  4] Sent 1704 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   6.920 ms 0/1703 (0%) -/-/-/- ms 170 pps
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60853 (sock=3) (peer 2.1.6) on 2022-05-10 14:18:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   2.160 ms 0/2554 (0%) 5.101/2.750/23.214/2.285 ms 255 pps 74
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 56882 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[  6] Sent 2554 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   3.417 ms 0/2553 (0%) -/-/-/- ms 255 pps
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 51036 (sock=4) (peer 2.1.6) on 2022-05-10 14:19:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   1.926 ms 0/3405 (0%) 4.899/2.577/27.756/2.382 ms 340 pps 102
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 41427 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[  8] Sent 3405 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.01 sec  4.77 MBytes  4.00 Mbits/sec   3.736 ms 0/3404 (0%) -/-/-/- ms 340 pps
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 37532 (sock=3) (peer 2.1.6) on 2022-05-10 14:19:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  5.97 MBytes  5.00 Mbits/sec   1.713 ms 0/4255 (0%) 4.578/2.444/22.849/2.220 ms 425 pps 137
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 45476 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 10] Sent 4255 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-9.99 sec  5.96 MBytes  5.01 Mbits/sec   2.958 ms 0/4254 (0%) -/-/-/- ms 425 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36124 (sock=4) (peer 2.1.6) on 2022-05-10 14:19:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.743 ms 0/5105 (0%) 4.845/2.260/21.901/2.419 ms 510 pps 155
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 50189 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 12] Sent 5105 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  7.16 MBytes  6.00 Mbits/sec   2.634 ms 0/5104 (0%) -/-/-/- ms 509 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 49574 (sock=3) (peer 2.1.6) on 2022-05-10 14:20:13 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   1.459 ms 0/5956 (0%) 6.403/3.528/24.594/2.588 ms 595 pps 137
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 51046 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 14] Sent 5956 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec   2.287 ms 0/5955 (0%) -/-/-/- ms 595 pps
[ 15] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60261 (sock=4) (peer 2.1.6) on 2022-05-10 14:20:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.01 sec  9.54 MBytes  8.00 Mbits/sec   0.784 ms 0/6806 (0%) 9.611/5.549/33.289/2.859 ms 680 pps 104
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.217%eth0 port 52280 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 16] Sent 6806 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec   1.526 ms 0/6805 (0%) -/-/-/- ms 680 pps
[ 17] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 56136 (sock=3) (peer 2.1.6) on 2022-05-10 14:20:54 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec   1.370 ms 0/7656 (0%) 9.027/5.758/71.618/4.282 ms 766 pps 125
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.217%eth0 port 34803 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 18] Sent 7656 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.01 sec  10.7 MBytes  8.99 Mbits/sec   1.752 ms 0/7655 (0%) -/-/-/- ms 764 pps
[ 19] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 42407 (sock=4) (peer 2.1.6) on 2022-05-10 14:21:14 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec   0.913 ms 0/8507 (0%) 9.130/6.395/33.451/2.519 ms 851 pps 137
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.217%eth0 port 38941 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 20] Sent 8507 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.04 sec  11.9 MBytes  9.97 Mbits/sec   3.185 ms 0/8506 (0%) -/-/-/- ms 847 pps
[ 21] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46716 (sock=3) (peer 2.1.6) on 2022-05-10 14:21:34 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec   1.237 ms 0/9357 (0%) 9.049/6.375/26.949/2.453 ms 936 pps 152
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1069.09 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.217%eth0 port 53132 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  13.1 MBytes  11.0 Mbits/sec  0/0      936 pps
[ 22] Sent 9357 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.02 sec  13.1 MBytes  11.0 Mbits/sec   1.983 ms 0/9356 (0%) -/-/-/- ms 934 pps
[ 23] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46197 (sock=4) (peer 2.1.6) on 2022-05-10 14:21:55 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec   0.882 ms 0/10207 (0%) 7.748/5.038/28.636/2.464 ms 1021 pps 194
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 980.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.217%eth0 port 34856 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  14.3 MBytes  12.0 Mbits/sec  0/0     1021 pps
[ 24] Sent 10207 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-10.01 sec  14.3 MBytes  12.0 Mbits/sec   1.462 ms 0/10206 (0%) -/-/-/- ms 1020 pps
[ 25] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 34446 (sock=3) (peer 2.1.6) on 2022-05-10 14:22:15 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec   0.893 ms 0/11058 (0%) 8.645/6.074/27.036/2.653 ms 1106 pps 188
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 904.62 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.217%eth0 port 38847 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec  0/0     1106 pps
[ 26] Sent 11058 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.00 sec  15.5 MBytes  13.0 Mbits/sec   0.906 ms 0/11057 (0%) -/-/-/- ms 1105 pps
[ 27] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 36850 (sock=4) (peer 2.1.6) on 2022-05-10 14:22:36 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec   0.892 ms 0/11908 (0%) 7.096/3.903/31.163/2.769 ms 1191 pps 247
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.217%eth0 port 39136 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  16.7 MBytes  14.0 Mbits/sec  0/0     1191 pps
[ 28] Sent 11908 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.02 sec  16.7 MBytes  14.0 Mbits/sec   1.348 ms 0/11907 (0%) -/-/-/- ms 1188 pps
[ 29] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 54318 (sock=3) (peer 2.1.6) on 2022-05-10 14:22:56 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.01 sec  17.9 MBytes  15.0 Mbits/sec   1.317 ms 0/12758 (0%) 7.571/4.836/26.216/2.616 ms 1275 pps 248
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 784.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.217%eth0 port 40497 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  17.9 MBytes  15.0 Mbits/sec  0/0     1276 pps
[ 30] Sent 12758 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.04 sec  17.9 MBytes  14.9 Mbits/sec   1.102 ms 0/12757 (0%) -/-/-/- ms 1270 pps
[ 31] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 57827 (sock=4) (peer 2.1.6) on 2022-05-10 14:23:17 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-9.99 sec  19.1 MBytes  16.0 Mbits/sec   0.772 ms 0/13609 (0%) 7.397/4.664/25.426/2.480 ms 1362 pps 271
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 735.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.217%eth0 port 49511 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec  0/0     1361 pps
[ 32] Sent 13609 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.00 sec  19.1 MBytes  16.0 Mbits/sec   1.079 ms 0/13608 (0%) -/-/-/- ms 1360 pps
[ 33] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40194 (sock=3) (peer 2.1.6) on 2022-05-10 14:23:37 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec   0.750 ms 0/14459 (0%) 7.320/3.776/25.478/2.740 ms 1446 pps 290
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 691.76 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.217%eth0 port 34577 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec  0/0     1446 pps
[ 34] Sent 14459 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.00 sec  20.3 MBytes  17.0 Mbits/sec   0.778 ms 0/14458 (0%) -/-/-/- ms 1445 pps
[ 35] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 57073 (sock=4) (peer 2.1.6) on 2022-05-10 14:23:58 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-9.99 sec  21.5 MBytes  18.0 Mbits/sec   0.657 ms 1/15309 (0.0065%) 6.983/3.604/32.029/2.896 ms 1532 pps 322
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 653.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.217%eth0 port 48979 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  21.5 MBytes  18.0 Mbits/sec  0/0     1531 pps
[ 36] Sent 15309 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.03 sec  21.5 MBytes  18.0 Mbits/sec   0.783 ms 0/15308 (0%) -/-/-/- ms 1526 pps
[ 37] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 47824 (sock=3) (peer 2.1.6) on 2022-05-10 14:24:18 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec   0.615 ms 0/16160 (0%) 7.850/4.461/37.457/3.093 ms 1616 pps 303
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 618.95 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.217%eth0 port 46239 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  22.7 MBytes  19.0 Mbits/sec  0/0     1616 pps
[ 38] Sent 16160 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  22.7 MBytes  18.9 Mbits/sec   2.710 ms 0/16159 (0%) -/-/-/- ms 1610 pps
[ 39] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 33809 (sock=4) (peer 2.1.6) on 2022-05-10 14:24:38 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 39] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec   0.626 ms 0/17010 (0%) 7.150/3.850/29.485/3.095 ms 1701 pps 350
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 588.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*40] local 10.0.23.217%eth0 port 36616 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*40] 0.00-10.00 sec  23.8 MBytes  20.0 Mbits/sec  0/0     1701 pps
[ 40] Sent 17010 datagrams
[ 40] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*40] 0.00-10.02 sec  23.8 MBytes  20.0 Mbits/sec   1.096 ms 0/17009 (0%) -/-/-/- ms 1697 pps
[ 41] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 60136 (sock=3) (peer 2.1.6) on 2022-05-10 14:24:59 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 41] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec   0.631 ms 0/17860 (0%) 8.418/4.786/26.969/2.935 ms 1786 pps 312
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 560.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*42] local 10.0.23.217%eth0 port 32980 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec  0/0     1786 pps
[ 42] Sent 17860 datagrams
[ 42] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*42] 0.00-10.00 sec  25.0 MBytes  21.0 Mbits/sec   0.516 ms 0/17859 (0%) -/-/-/- ms 1785 pps
[ 43] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 40153 (sock=4) (peer 2.1.6) on 2022-05-10 14:25:19 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 43] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec   0.730 ms 0/18711 (0%) 7.157/3.919/26.081/2.991 ms 1871 pps 384
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 534.55 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*44] local 10.0.23.217%eth0 port 33521 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*44] 0.00-10.00 sec  26.2 MBytes  22.0 Mbits/sec  0/0     1871 pps
[ 44] Sent 18711 datagrams
[ 44] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*44] 0.00-10.06 sec  26.2 MBytes  21.9 Mbits/sec   2.813 ms 0/18710 (0%) -/-/-/- ms 1860 pps
[ 45] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 34925 (sock=3) (peer 2.1.6) on 2022-05-10 14:25:39 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 45] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec   0.516 ms 0/19561 (0%) 9.209/4.947/38.116/3.322 ms 1956 pps 312
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 511.30 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*46] local 10.0.23.217%eth0 port 33383 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*46] 0.00-10.00 sec  27.4 MBytes  23.0 Mbits/sec  0/0     1956 pps
[ 46] Sent 19561 datagrams
[ 46] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*46] 0.00-10.02 sec  27.4 MBytes  22.9 Mbits/sec   0.757 ms 9/19560 (0.046%) -/-/-/- ms 1951 pps
[ 47] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 47137 (sock=4) (peer 2.1.6) on 2022-05-10 14:26:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 47] 0.00-10.12 sec  26.9 MBytes  22.3 Mbits/sec   1.396 ms 1252/20411 (6.1%) 11.986/3.781/179.816/16.205 ms 1894 pps 232
[ 49] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 47137 (sock=3) (peer 2.1.6) on 2022-05-10 14:26:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 49] 0.00-0.00 sec  0.003 MBytes   nan Mbits/sec   0.009 ms 20420/20422 (1e+02%) 130.814/130.742/130.885/130.885 ms -13986 pps nan
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*48] local 10.0.23.217%eth0 port 48737 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4645 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*50] local 10.0.23.217%eth0 port 57473 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
------------------------------------------------------------
Server listening on UDP port 5001 with pid 4749
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 50684 (sock=3) (peer 2.1.6) on 2022-05-10 14:28:00 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec   0.521 ms 0/20412 (0%) 5.269/1.713/23.875/3.136 ms 2041 pps 570
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4749 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 490.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.217%eth0 port 39970 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.00 sec  28.6 MBytes  24.0 Mbits/sec  0/0     2041 pps
[  2] Sent 20411 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  28.6 MBytes  24.0 Mbits/sec   1.156 ms 0/20410 (0%) -/-/-/- ms 2037 pps
[  3] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 38601 (sock=5) (peer 2.1.6) on 2022-05-10 14:28:20 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec   0.455 ms 0/21262 (0%) 8.158/4.579/26.217/3.000 ms 2127 pps 383
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4749 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 470.40 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.217%eth0 port 36779 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.00 sec  29.8 MBytes  25.0 Mbits/sec  0/0     2126 pps
[  4] Sent 21262 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.02 sec  29.7 MBytes  24.8 Mbits/sec   0.670 ms 90/21261 (0.42%) -/-/-/- ms 2121 pps
[  5] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 46833 (sock=3) (peer 2.1.6) on 2022-05-10 14:28:40 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec   0.447 ms 0/22112 (0%) 7.413/2.913/29.073/3.105 ms 2211 pps 438
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4749 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 452.31 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.217%eth0 port 43206 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.00 sec  31.0 MBytes  26.0 Mbits/sec  0/0     2211 pps
[  6] Sent 22112 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  30.7 MBytes  25.7 Mbits/sec   0.837 ms 220/22111 (0.99%) -/-/-/- ms 2209 pps
[  7] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 35785 (sock=4) (peer 2.1.6) on 2022-05-10 14:29:01 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec   0.476 ms 0/22962 (0%) 6.878/3.479/28.817/3.094 ms 2297 pps 491
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4749 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 435.56 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.217%eth0 port 51345 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.00 sec  32.2 MBytes  27.0 Mbits/sec  0/0     2296 pps
[  8] Sent 22962 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.03 sec  32.0 MBytes  26.8 Mbits/sec   0.384 ms 103/22961 (0.45%) -/-/-/- ms 2288 pps
[  9] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 49593 (sock=3) (peer 2.1.6) on 2022-05-10 14:29:21 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec   0.412 ms 0/23813 (0%) 6.461/1.768/32.060/3.147 ms 2381 pps 542
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4749 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 420.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.217%eth0 port 48678 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  33.4 MBytes  28.0 Mbits/sec  0/0     2381 pps
[ 10] Sent 23813 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.02 sec  32.9 MBytes  27.5 Mbits/sec   0.411 ms 365/23812 (1.5%) -/-/-/- ms 2376 pps
[ 11] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 49513 (sock=4) (peer 2.1.6) on 2022-05-10 14:29:42 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec   0.391 ms 0/24663 (0%) 6.620/1.333/25.464/3.004 ms 2465 pps 547
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4749 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 405.52 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.217%eth0 port 47948 connected with 10.0.20.220 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.00 sec  34.6 MBytes  29.0 Mbits/sec  0/0     2466 pps
[ 12] Sent 24663 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  33.9 MBytes  28.4 Mbits/sec   0.254 ms 509/24662 (2.1%) -/-/-/- ms 2464 pps
[ 13] local 10.0.23.217%eth0 port 5001 connected with 10.0.20.220 port 55345 (sock=3) (peer 2.1.6) on 2022-05-10 14:30:02 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.01 sec  35.8 MBytes  30.0 Mbits/sec   0.762 ms 0/25513 (0%) 11.609/4.160/32.206/3.775 ms 2548 pps 323
------------------------------------------------------------
Client connecting to 10.0.20.220, UDP port 5001 with pid 4749 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 392.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.217%eth0 port 48010 connected with 10.0.20.220 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  35.8 MBytes  30.0 Mbits/sec  0/0     2551 pps
[ 14] Sent 25513 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-9.96 sec  32.4 MBytes  27.3 Mbits/sec   0.239 ms 2379/25512 (9.3%) -/-/-/- ms 2562 pps
