------------------------------------------------------------
Server listening on UDP port 5001 with pid 2417
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
------------------------------------------------------------
Server listening on UDP port 5001 with pid 3424
Read buffer size: 0.001 MByte (Dist bin width= 183 Byte)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[  1] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37512 (sock=3) (peer 2.1.6) on 2022-05-13 14:36:47 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  1] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.042 ms 0/854 (0%) 1.380/1.208/4.286/0.227 ms 85 pps 91
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 11760.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *2] local 10.0.23.60%eth0 port 37400 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec  0/0       85 pps
[  2] Sent 854 datagrams
[  2] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *2] 0.00-10.02 sec  1.20 MBytes  1.00 Mbits/sec   0.047 ms 0/853 (0%) 2.798/2.553/4.820/0.203 ms 85 pps 45
[  3] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 48374 (sock=5) (peer 2.1.6) on 2022-05-13 14:37:07 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  3] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.011 ms 0/1279 (0%) 1.871/1.718/4.977/0.187 ms 128 pps 100
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 7840.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *4] local 10.0.23.60%eth0 port 33056 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec  0/0      128 pps
[  4] Sent 1279 datagrams
[  4] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *4] 0.00-10.01 sec  1.79 MBytes  1.50 Mbits/sec   0.070 ms 0/1278 (0%) 2.579/2.339/5.716/0.233 ms 127 pps 73
[  5] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49468 (sock=3) (peer 2.1.6) on 2022-05-13 14:37:28 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  5] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.019 ms 0/1704 (0%) 2.138/1.846/5.290/0.208 ms 170 pps 117
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 5880.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *6] local 10.0.23.60%eth0 port 34726 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec  0/0      170 pps
[  6] Sent 1704 datagrams
[  6] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *6] 0.00-10.01 sec  2.39 MBytes  2.00 Mbits/sec   0.028 ms 0/1703 (0%) 2.554/2.286/5.322/0.185 ms 170 pps 98
[  7] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46519 (sock=4) (peer 2.1.6) on 2022-05-13 14:37:48 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  7] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec   0.023 ms 0/2129 (0%) 2.070/1.895/5.006/0.191 ms 213 pps 151
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 4704.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[ *8] local 10.0.23.60%eth0 port 34475 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[ *8] 0.00-10.01 sec  2.98 MBytes  2.50 Mbits/sec  0/0      213 pps
[  8] Sent 2129 datagrams
[  8] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ *8] 0.00-10.00 sec  2.98 MBytes  2.50 Mbits/sec   0.030 ms 0/2128 (0%) 2.451/2.236/7.104/0.199 ms 212 pps 128
[  9] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 43767 (sock=3) (peer 2.1.6) on 2022-05-13 14:38:08 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[  9] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.045 ms 0/2554 (0%) 2.078/1.802/4.794/0.207 ms 255 pps 181
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3920.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*10] local 10.0.23.60%eth0 port 47079 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec  0/0      255 pps
[ 10] Sent 2554 datagrams
[ 10] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*10] 0.00-10.00 sec  3.58 MBytes  3.00 Mbits/sec   0.027 ms 0/2553 (0%) 2.503/2.250/5.423/0.200 ms 255 pps 150
[ 11] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56053 (sock=4) (peer 2.1.6) on 2022-05-13 14:38:29 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 11] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.033 ms 0/2980 (0%) 2.015/1.775/4.846/0.236 ms 298 pps 217
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 3360.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*12] local 10.0.23.60%eth0 port 42970 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec  0/0      298 pps
[ 12] Sent 2980 datagrams
[ 12] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*12] 0.00-10.01 sec  4.18 MBytes  3.50 Mbits/sec   0.072 ms 0/2979 (0%) 2.560/2.240/5.390/0.223 ms 297 pps 171
[ 13] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53827 (sock=3) (peer 2.1.6) on 2022-05-13 14:38:49 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 13] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.014 ms 0/3405 (0%) 2.074/1.901/9.781/0.360 ms 340 pps 241
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2940.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*14] local 10.0.23.60%eth0 port 45892 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec  0/0      340 pps
[ 14] Sent 3405 datagrams
[ 14] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*14] 0.00-10.00 sec  4.77 MBytes  4.00 Mbits/sec   0.042 ms 0/3404 (0%) 2.273/2.026/6.529/0.235 ms 340 pps 220
[ 15] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56796 (sock=4) (peer 2.1.6) on 2022-05-13 14:39:10 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 15] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.008 ms 0/3830 (0%) 2.328/2.082/5.091/0.316 ms 383 pps 242
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2613.33 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*16] local 10.0.23.60%eth0 port 35278 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec  0/0      383 pps
[ 16] Sent 3830 datagrams
[ 16] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*16] 0.00-10.00 sec  5.37 MBytes  4.50 Mbits/sec   0.079 ms 0/3829 (0%) 2.195/1.960/5.457/0.232 ms 382 pps 256
[ 17] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53196 (sock=3) (peer 2.1.6) on 2022-05-13 14:39:30 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 17] 0.00-10.01 sec  5.97 MBytes  5.00 Mbits/sec   0.318 ms 0/4255 (0%) 2.361/2.093/5.549/0.429 ms 425 pps 265
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2352.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*18] local 10.0.23.60%eth0 port 40612 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec  0/0      425 pps
[ 18] Sent 4255 datagrams
[ 18] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*18] 0.00-10.00 sec  5.96 MBytes  5.00 Mbits/sec   0.031 ms 0/4254 (0%) 2.181/1.843/6.723/0.269 ms 425 pps 287
[ 19] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 52325 (sock=4) (peer 2.1.6) on 2022-05-13 14:39:51 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 19] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.218 ms 0/4680 (0%) 2.489/2.054/8.505/0.746 ms 468 pps 276
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 2138.18 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*20] local 10.0.23.60%eth0 port 33916 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec  0/0      468 pps
[ 20] Sent 4680 datagrams
[ 20] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*20] 0.00-10.00 sec  6.56 MBytes  5.50 Mbits/sec   0.043 ms 0/4679 (0%) 2.247/1.957/7.259/0.322 ms 467 pps 306
[ 21] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 45906 (sock=3) (peer 2.1.6) on 2022-05-13 14:40:11 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 21] 0.00-10.01 sec  7.16 MBytes  6.00 Mbits/sec   0.095 ms 0/5105 (0%) 4.121/1.261/8.835/1.533 ms 510 pps 182
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1960.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*22] local 10.0.23.60%eth0 port 41755 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec  0/0      510 pps
[ 22] Sent 5105 datagrams
[ 22] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*22] 0.00-10.00 sec  7.16 MBytes  6.00 Mbits/sec   0.034 ms 0/5104 (0%) 2.637/2.030/6.226/0.455 ms 510 pps 285
[ 23] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 37977 (sock=4) (peer 2.1.6) on 2022-05-13 14:40:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 23] 0.00-10.01 sec  7.26 MBytes  6.08 Mbits/sec   0.257 ms 354/5531 (6.4%) 34.475/2.413/61.953/15.490 ms 517 pps 22
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1809.23 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*24] local 10.0.23.60%eth0 port 49535 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*24] 0.00-10.00 sec  7.75 MBytes  6.50 Mbits/sec  0/0      553 pps
[ 24] Sent 5531 datagrams
[ 24] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*24] 0.00-9.97 sec  7.75 MBytes  6.52 Mbits/sec   0.051 ms 0/5530 (0%) 46.046/26.793/68.183/0.840 ms 554 pps 18
[ 25] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 49896 (sock=3) (peer 2.1.6) on 2022-05-13 14:40:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 25] 0.00-10.09 sec  7.26 MBytes  6.04 Mbits/sec   0.451 ms 777/5956 (13%) -/-/-/- ms 513 pps
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1680.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*26] local 10.0.23.60%eth0 port 55688 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*26] 0.00-10.00 sec  8.35 MBytes  7.00 Mbits/sec  0/0      595 pps
[ 26] Sent 5956 datagrams
[ 26] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*26] 0.00-10.02 sec  6.98 MBytes  5.84 Mbits/sec   0.103 ms 974/5955 (16%) -/-/-/- ms 594 pps
[ 27] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 46697 (sock=4) (peer 2.1.6) on 2022-05-13 14:41:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 27] 0.00-10.06 sec  7.27 MBytes  6.06 Mbits/sec   0.517 ms 1196/6381 (19%) 64.559/7.157/67.022/5.676 ms 515 pps 12
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1568.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*28] local 10.0.23.60%eth0 port 34389 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*28] 0.00-10.00 sec  8.94 MBytes  7.50 Mbits/sec  0/0      638 pps
[ 28] Sent 6381 datagrams
[ 28] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*28] 0.00-10.04 sec  8.75 MBytes  7.31 Mbits/sec   0.059 ms 135/6380 (2.1%) 43.351/2.510/50.664/0.771 ms 635 pps 21
[ 29] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53493 (sock=3) (peer 2.1.6) on 2022-05-13 14:41:32 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 29] 0.00-10.07 sec  7.28 MBytes  6.07 Mbits/sec   0.606 ms 1611/6807 (24%) 71.443/9.409/76.908/5.958 ms 516 pps 11
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1470.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*30] local 10.0.23.60%eth0 port 51132 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*30] 0.00-10.00 sec  9.54 MBytes  8.00 Mbits/sec  0/0      680 pps
[ 30] Sent 6806 datagrams
[ 30] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*30] 0.00-10.04 sec  8.76 MBytes  7.32 Mbits/sec   0.234 ms 558/6805 (8.2%) -/-/-/- ms 677 pps
[ 31] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 59497 (sock=4) (peer 2.1.6) on 2022-05-13 14:41:52 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 31] 0.00-10.06 sec  7.26 MBytes  6.05 Mbits/sec   0.668 ms 2050/7231 (28%) 85.334/24.505/108.534/5.049 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1383.53 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*32] local 10.0.23.60%eth0 port 43966 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*32] 0.00-10.00 sec  10.1 MBytes  8.50 Mbits/sec  0/0      723 pps
[ 32] Sent 7231 datagrams
[ 32] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*32] 0.00-10.05 sec  8.75 MBytes  7.31 Mbits/sec   0.342 ms 988/7231 (14%) -/-/-/- ms 719 pps
[ 33] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 35527 (sock=3) (peer 2.1.6) on 2022-05-13 14:42:12 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 33] 0.00-10.06 sec  7.26 MBytes  6.06 Mbits/sec   0.648 ms 2474/7656 (32%) 88.750/29.757/90.820/4.571 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1306.67 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*34] local 10.0.23.60%eth0 port 48054 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*34] 0.00-10.00 sec  10.7 MBytes  9.00 Mbits/sec  0/0      765 pps
[ 34] Sent 7656 datagrams
[ 34] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*34] 0.00-10.04 sec  8.77 MBytes  7.32 Mbits/sec   0.457 ms 1401/7655 (18%) -/-/-/- ms 762 pps
[ 35] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 53310 (sock=4) (peer 2.1.6) on 2022-05-13 14:42:33 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 35] 0.00-10.06 sec  7.27 MBytes  6.06 Mbits/sec   0.607 ms 2896/8082 (36%) 89.032/30.960/90.606/4.220 ms 515 pps 9
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1237.89 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*36] local 10.0.23.60%eth0 port 59913 connected with 10.0.23.61 port 5001 (reverse) (sock=4) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*36] 0.00-10.00 sec  11.3 MBytes  9.50 Mbits/sec  0/0      808 pps
[ 36] Sent 8082 datagrams
[ 36] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*36] 0.00-10.05 sec  8.78 MBytes  7.33 Mbits/sec   0.493 ms 1820/8081 (23%) -/-/-/- ms 804 pps
[ 37] local 10.0.23.60%eth0 port 5001 connected with 10.0.23.61 port 56192 (sock=3) (peer 2.1.6) on 2022-05-13 14:42:53 (CEST)
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[ 37] 0.00-10.16 sec  6.64 MBytes  5.48 Mbits/sec   4.547 ms 3777/8511 (44%) 89.806/29.877/241.626/12.901 ms 466 pps 8
------------------------------------------------------------
Client connecting to 10.0.23.61, UDP port 5001 with pid 3424 (1 flows)
TOS set to 0x0 (Nagle on)
Sending 1470 byte datagrams, IPG target: 1176.00 us (kalman adjust)
UDP buffer size:  176 KByte (default)
------------------------------------------------------------
[*38] local 10.0.23.60%eth0 port 47828 connected with 10.0.23.61 port 5001 (reverse) (sock=3) (peer 2.1.6)
[ ID] Interval        Transfer     Bandwidth      Write/Err  PPS
[*38] 0.00-10.00 sec  11.9 MBytes  10.0 Mbits/sec  0/0      851 pps
[ 38] Sent 8507 datagrams
[ 38] Server Report:
[ ID] Interval        Transfer     Bandwidth        Jitter   Lost/Total  Latency avg/min/max/stdev PPS NetPwr
[*38] 0.00-10.04 sec  8.77 MBytes  7.32 Mbits/sec   0.532 ms 2251/8506 (26%) -/-/-/- ms 846 pps
