<config configVersion="1.1" device="PIC32MM0256GPM028" coreVersion="4.45">
   <usedClasses class="java.util.HashMap">
      <entry>
         <string>SPI1</string>
         <string>class com.microchip.mcc.mcu16.modules.spi_pb.SPI</string>
      </entry>
      <entry>
         <string>CORETIMER</string>
         <string>class com.microchip.mcc.mcu16.modules.coreTimer.CoreTimer</string>
      </entry>
      <entry>
         <string>USB</string>
         <string>class com.microchip.mcc.modules.mcu16.MLAUSBDevice.MLAUSBDevice</string>
      </entry>
      <entry>
         <string>UART2</string>
         <string>class com.microchip.mcc.mcu16.modules.uart_irda_upb.UART</string>
      </entry>
      <entry>
         <string>WATCHDOG</string>
         <string>class com.microchip.mcc.mcu16.systemManager.wdt.Wdt</string>
      </entry>
      <entry>
         <string>UART3</string>
         <string>class com.microchip.mcc.mcu16.modules.uart_irda_upb.UART</string>
      </entry>
      <entry>
         <string>Pin Module</string>
         <string>class com.microchip.mcc.mcu16.pinManager.PinManager</string>
      </entry>
      <entry>
         <string>ICD</string>
         <string>class com.microchip.mcc.mcu16.systemManager.icd.Icd</string>
      </entry>
      <entry>
         <string>Interrupt Module</string>
         <string>class com.microchip.mcc.mcu16.interruptManager_PIC32MM.InterruptManager_PIC32MM</string>
      </entry>
      <entry>
         <string>System Module</string>
         <string>class com.microchip.mcc.mcu16.systemManager.DefaultSystemManagerMcu16</string>
      </entry>
      <entry>
         <string>CDCDevice</string>
         <string>class com.microchip.mcc.modules.mcu16.deviceclass.CDCDevice.CDCDevice</string>
      </entry>
      <entry>
         <string>INTERNAL OSCILLATOR</string>
         <string>class com.microchip.mcc.mcu16.systemManager.clk.Clock</string>
      </entry>
      <entry>
         <string>VendorDevice</string>
         <string>class com.microchip.mcc.modules.mcu16.deviceclass.VendorDevice.VendorDevice</string>
      </entry>
      <entry>
         <string>TMR2</string>
         <string>class com.microchip.mcc.mcu16.modules.tmr_classa_pb.TMR</string>
      </entry>
      <entry>
         <string>TMR1</string>
         <string>class com.microchip.mcc.mcu16.modules.tmr_classa_pb.TMR</string>
      </entry>
   </usedClasses>
   <usedLibraries class="java.util.ArrayList">
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.mcu16.Mcu16PeripheralLibrary" version="1.54"/>
      <ILibraryFile class="com.microchip.mcc.core.library.BaseLibraryFile" libraryClass="com.microchip.mcc.USBDEVICELite.USBDEVICELite" version="1.25.5"/>
   </usedLibraries>
   <tokenMap class="java.util.HashMap">
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="CLKSEL"/>
         <value>PBCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="CLKSEL"/>
         <value>PBCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllGraphicsSelect"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPHSHK3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV" alias="1:256"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPRXEN0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITUR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPSTALL8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPCONDIS8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="USBI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DMPULDWN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ACTIVE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPTXEN2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="SIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB4"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="BaudRateError"/>
         <value>-0.160</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS"/>
         <value>PS1048576</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPTXEN12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTCLK" alias="LPRC"/>
         <value>24576</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="tickerFactor"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMSYPW" alias="One-Character"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB4" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPHSHK14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMERREN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL"/>
         <value>SYSCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTCLK"/>
         <value>LPRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR7" settingAlias="ICM6R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="EXTR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="SIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UPWRC" settingAlias="USBPWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="BTSEE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="inputMode"/>
         <value>periodMode</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR3" settingAlias="RP13R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="BaudRateError"/>
         <value>0.160</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="FERR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="FERR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBRK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNAI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MCLKSEL" alias="PBCLK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TWDIS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPHSHK6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="T1MSECIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="PERR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SPDIVRDY"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="SIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSCHG"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="OERR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="OERR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VSS4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="IDIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN"/>
         <value>BOR3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SRXISEL" alias="Buffer is more than half full"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ACTIVE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="ABAUD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="SIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR11"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ACTIVE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="GNMI"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsOutput"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="ADDEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="RSLP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="combinedTimer"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="inputMode"/>
         <value>periodMode</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FOSCSEL"/>
         <value>50065</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="CORETIMER" registerAlias="CTI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB2"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="ADDEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UBRG" settingAlias="BRG"/>
         <value>312</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UTOK" settingAlias="PID"/>
         <value>OUT (TX) token type transaction</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UBRG" settingAlias="BRG"/>
         <value>103</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXBF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="IDLEIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR10"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXDA" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="SBOREN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="UERRIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="RESUMEIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="ORNG" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="OE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="OVFDIS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPSTALL12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VUSB3V3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="combinedTimer"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPSTALL12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIR" settingAlias="URSTIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="CLKSEL" alias="REFCLKO"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIBUSY"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIE" settingAlias="UERRIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPHSHK11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPHSHK3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="STEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="RIDLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureRefClkOutoutEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB3"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC"/>
         <value>LPRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="CRC5EF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDMOD" alias="enabled"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPRXEN3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS16384"/>
         <value>14</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPHSHK0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="UARTEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_SOSC"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPRXEN13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLICLK"/>
         <value>FRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIR" settingAlias="IDLEIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="USBRST" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="SWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNDI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS" alias="1:8"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="VBUSVD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="prescaledFreq"/>
         <value>24000000.00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="TransferCompleteHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPCONDIS0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCON" settingAlias="WDTWINEN"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="SOSC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPCONDIS8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="BTOEE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA3" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPHSHK3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR4" settingAlias="RP18R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="IREN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPTXEN8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="Autotune"/>
         <value>Use USB Host clock reference</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UPWRC" settingAlias="USBPWR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR6" settingAlias="TCKIBR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="SIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="IREN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RA1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR12" settingAlias="CLCINAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UBDTP2" settingAlias="BDTPTRH" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSwitching"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SSEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_ROSEL"/>
         <value>SYSCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS"/>
         <value>PGx1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="T1MSECIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPTXEN13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="PLLSRC"/>
         <value>FRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscalerClock"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_COMPLETE"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCEN" alias="ON"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DMPULUP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB7"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXISEL"/>
         <value>RX_ONE_CHAR</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB8"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXISEL"/>
         <value>RX_ONE_CHAR</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB6"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB2"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB0"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="SBOREN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPTXEN2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="prescaledFreq"/>
         <value>3000000.00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UTXI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR1" settingAlias="RP7R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="FUSBIDIO"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="POSCMOD" alias="XT"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXDA" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPRXEN0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DMPULDWN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV" alias="FRC/64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPCONDIS2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPSTALL15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPRXEN15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RXINV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RC9"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_BUF_EMPTY"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="RIDLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="RIDLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="CORETIMER" registerAlias="Count" settingAlias="Count"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="DISSDO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="POSCMOD"/>
         <value>NONE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="URSTIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS65536"/>
         <value>4096</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="ABAUD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="NonstandardEP0ReqHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR12"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPTXEN12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO" alias="ON"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="PERR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="RIDLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_USB"/>
         <value>48000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPTXEN15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="PERR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="DIVSWEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UTXI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Switch is Complete"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIR" settingAlias="STALLIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="CLKSEL" alias="PBCLK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="USBI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPTXEN5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="UERRIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV" alias="FRC/32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPCONDIS5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB3" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNDI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DMPULUP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="VREGS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FCKSM" alias="CSECME"/>
         <value>49152</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FCKSM" alias="CSECMD"/>
         <value>16384</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="TRMT" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UTOK" settingAlias="EP"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="System PLL"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF"/>
         <value>No Clock Failure</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DMPULUP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBRK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXBRK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCON" settingAlias="JSTATE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPHSHK0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="IDIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RTSMD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="STXISEL"/>
         <value>Complete</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3"/>
         <value>set</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="RTSMD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="actualPeriod"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="RETVR" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="ClockInput"/>
         <value>32000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="BTSEE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNAI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPCONDIS5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPSTALL12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RXINV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TNI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="URSTIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="FSCM has detected clock failure"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS256"/>
         <value>2048</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TWDIS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR2" registerAlias="PR32"/>
         <value>732</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="PKTDIS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="LPBOREN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR1" registerAlias="TMR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TNI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR2" registerAlias="TMR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SSEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTCLK" alias="FRC"/>
         <value>16384</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPRXEN12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RSWRST" settingAlias="SWRST"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV" alias="FRC/16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="ORNG" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPCONDIS12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPHSHK11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="CNSTYLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPCONDIS7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="IDLEIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="PERR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPRXEN4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="BTOEE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIR" settingAlias="UERRIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPTXEN4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV"/>
         <value>FRC/1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="actualPeriod"/>
         <value>0.000015</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="LOCK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR5" settingAlias="RP22R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MODE16"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="OE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SPI1_SPIIISRFunction"/>
         <value>ISR_SPI1_SPII</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="SYSCLK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="tickerFactor"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR1" registerAlias="TCON"/>
         <value>32784</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPSTALL1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR2" registerAlias="TCON"/>
         <value>32776</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPITXI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ACTIVE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="FERR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MODE16" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UBDTP2" settingAlias="BDTPTRH" alias="enabled"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="SLPEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPCONDIS15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscClock"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPRXEN15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="SIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="SIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPCONDIS6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPTXEN8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="RETEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BOR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCON" settingAlias="RESUME"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="LSTATE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SDO1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="IDLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MCLKSEL" alias="REFCLKO"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR3" settingAlias="RP15R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPSTALL15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1048576"/>
         <value>5120</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="OVFDIS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="ACTIVE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="URXI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ACTIVE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="LSTATEIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS"/>
         <value>SOSC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="TRNIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS131072"/>
         <value>4352</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="SIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP0" settingAlias="RETRYDIS0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RSWRST" settingAlias="SWRST" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SOSCHP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEIE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_COMPLETE"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS2048"/>
         <value>11</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="PS25_0"/>
         <value>96</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ODCA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="FVBUSIO" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VCAP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SPIFE" alias="Frame Sync pulse precedes"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="minPeriod"/>
         <value>0.0000003333</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMSYPW" alias="One-Clock"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS"/>
         <value>1:8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIR" settingAlias="SOFIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR1" settingAlias="RP5R"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="SWTXBufferSize"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="URSTIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BCFGFAIL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="AllInterrupts"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="ENHBUF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="FERR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="CNSTYLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPSTALL13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="customPR"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCS"/>
         <value>PBCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="RXBUFELM" alias="enabled"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="RXBUFELM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCS"/>
         <value>PBCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="T1MSECIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="RIDLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="WAKE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="LSTATEIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureSoscEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPRXEN12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLMULT" alias="12x"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPRXEN12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C" alias="OFF"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="ACTIVE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RSWRST" settingAlias="SWRST" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_BUF_EMPTY"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FWDT"/>
         <value>29940</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="TRNIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="SLEEP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPHSHK9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="minPeriod"/>
         <value>0.0000000417</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="CRC5EE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="SWTXBufferSize"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="STSEL" alias="1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="STSEL" alias="2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="STSEL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="STSEL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTCLK" alias="SYSCLK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCON" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="VBUSVDIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV" alias="1:2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="SLPEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MSTEN" alias="Slave"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPTXEN15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="RESUMEIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV" alias="1:8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR1" settingAlias="INT4R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV" alias="1:4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MSSEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="OSCIOFCN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPSTALL2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_ENABLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPTXEN5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA0"/>
         <value>SLEEPN</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB13"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPSTALL8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPSTALL9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCSEL"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPITXI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB0"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="InternalClock"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITUR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPHSHK4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="VBUSVDIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPCONDIS15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPISGNEXT" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB0"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB14"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA1"/>
         <value>RESET</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RA4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="CRC5EF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="POSCMOD" alias="HS"/>
         <value>512</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="ClockSource"/>
         <value>FRC Oscillator</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="AllInterrupts"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MSSEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPHSHK14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPSTALL2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC9" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="customPR"/>
         <value>48000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UOTGSTAT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="LSTATEIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="UARTEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR8" settingAlias="ICM9R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="SOSC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="LVD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler2"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK"/>
         <value>Clock and PLL selections are not locked and may be modified</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIE" settingAlias="RESUMEIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB13" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="SWNMI" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS" alias="LPRC"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VCAP"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMPOL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="RSLP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="TRMT" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SPDIVRDY" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPTXEN14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB1"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="BaudRate"/>
         <value>57600</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="IGNTUR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB15"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIE" settingAlias="SOFIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPRXEN5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="ID"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS4096"/>
         <value>3072</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNFC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="WAKE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPCONDIS11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPSTALL5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DPPULUP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNFB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR5" settingAlias="RP24R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="TRMT" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPCONDIS12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="CORETIMER" registerAlias="CTI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPCONDIS12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="T1MSECIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="SIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UADDR" settingAlias="LSPDEN" alias="Full Speed"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="ENHBUF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VCAP"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB15" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPHSHK6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="SuspendHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="LVD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="WATCHDOG" registerAlias="WDTCON" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDMOD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="BaudRate"/>
         <value>19200</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR1" registerAlias="PR"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="OTGEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR2" registerAlias="PR"/>
         <value>27648</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BCFGFAIL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPSTALL5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR8" settingAlias="U3RXR"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="UOEMON"/>
         <value>inactive</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSource"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MSTEN" alias="Master"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB14" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="VBUSVDIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureFrcEnable"/>
         <value>NOTAVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="SWNMI" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UOTGCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPSTALL2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SPDIVRDY" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="ManufacturerString"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="IGNTUR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIE" settingAlias="URSTIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS8192"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="InternalClock"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPHSHK10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="URSTIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPHSHK9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="IDLEIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC9" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="RETEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCON" settingAlias="CLKSEL"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="RESUMEIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPTXEN3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="OVFDIS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1A" settingAlias="CNIE1A3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_ONE_CHAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNFA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UTXI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="SESVDIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_PRIMARY"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXISEL" alias="RX_1_2_BUF_FULL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="FRCRDY"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPSTALL10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCS" alias="PBCLK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNDIISRFunction"/>
         <value>ISR_Pin Module_CNDI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="HOSTEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="LSTATEIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="SBOREN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS" alias="1:1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS" alias="1:2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCON" settingAlias="PPBRST"/>
         <value>Ping-Pong Buffer Pointers are not reset</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS" alias="1:4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="OERR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS" alias="1:8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="DataBits"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UPWRC" settingAlias="USLPGRD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BCFGERR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="FRC"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS131072"/>
         <value>17</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIE" settingAlias="DFN8EE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="ACTVIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="InterruptMode"/>
         <value>Polling</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNBI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPRXEN14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR2" settingAlias="RP11R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="FUSBIDIO" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MODE32"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="OE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="ID" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNDI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="PDSEL" alias="8E"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX_RTS"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="LSTATE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UBDTP3" settingAlias="BDTPTRU" alias="enabled"/>
         <value>255</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="PDSEL" alias="8N"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="PDSEL" alias="8O"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB13" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="PLLSRC" alias="POSC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="UTEYE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="DataBits"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UADDR" settingAlias="LSPDEN"/>
         <value>Full Speed</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="TRNIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="SIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNAIISRFunction"/>
         <value>ISR_Pin Module_CNAI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNCIISRFunction"/>
         <value>ISR_Pin Module_CNCI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SYSUSBSPEED"/>
         <value>Low Speed Full Speed</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="JTAGEN" alias="ON"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="PDSEL" alias="9N"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX_CTS_RTS"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXINV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="TMR2_TNIISRFunction"/>
         <value>ISR_TMR2_TNI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXINV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1A"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="ACTIVE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMCNT" alias="16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="TRNIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MSTEN"/>
         <value>Master</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="USBSIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="POSC"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB15" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPRXEN11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="USOF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="BCDDevice"/>
         <value>0x100</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="LSTATEIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPRXEN11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UPWRC" settingAlias="USLPGRD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1B"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="IGNROV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR3" settingAlias="ICM3R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="EXTR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN1C"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="DISSDI" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FSEC"/>
         <value>2147483648</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DPPULUP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="PLLSRC" alias="FRC"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCS" alias="External"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="USBI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB0" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TGATE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TGATE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="packageId"/>
         <value>SOIC28</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPRXEN14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNAI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPIBRG" settingAlias="SPIBRG"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPSTALL7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSYNC" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="POR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPHSHK5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB14" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="OpMode"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="RTSMD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPTXEN1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDMONO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TNI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA3" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VSS4"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="UTEYE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPTXEN11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SMP"/>
         <value>Middle</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="Speed"/>
         <value>Full</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPCONDIS14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="ON"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SOSCHP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB11" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="CNSTYLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="SESVDIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UPWRC" settingAlias="UACTPND"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB2" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCS" alias="T2CK"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPHSHK12" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="CORETIMER" registerAlias="Compare"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet AVDD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="T1CK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPISTAT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPCONDIS9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BCFGERR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMCNT" alias="32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB1" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIE" settingAlias="ATTACHIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UTOK" settingAlias="PID" alias="SETUP (TX) token type transaction"/>
         <value>13</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockChange"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UBDTP2" settingAlias="BDTPTRH"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VSS4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="RODIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SPI1_SPITXIISRFunction"/>
         <value>ISR_SPI1_SPITXI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPHSHK15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCON" settingAlias="SE0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="HOSTEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="EXTR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS32768"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPRXEN6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="CRC5EE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureOscfdivEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB10" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="SerialNumberString"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="FRCRDY" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDMOD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="AutoAttach"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="DISSDI" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="CKE" alias="Idle to Active"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPRXEN11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB3" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="FRCRDY" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPTXEN11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureVcoDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCON" settingAlias="USBEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPCONDIS9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1024"/>
         <value>2560</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="PKTDIS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="POL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPITUREN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="PR32" settingAlias="PR32"/>
         <value>732</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPrescaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="WDTO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="ORNG"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="RTSMD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPHSHK15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR11" settingAlias="SDI2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="WDTO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="RESUMEIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet AVSS1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MCLKSEL"/>
         <value>PBCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SRXISEL" alias="Buffer is not empty"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS262144"/>
         <value>4608</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="CLKSEL" alias="REFCLKO"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="RIDLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR4" settingAlias="RP20R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="CNSTYLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCC" settingAlias="ODCC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="SESVDIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="ENHBUF"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UBDTP3" settingAlias="BDTPTRU"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="CLKSEL" alias="FRC"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name NMCLR"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MODE16" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCON" settingAlias="USBRST"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR3" settingAlias="RP16R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="ADDR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UPWRC" settingAlias="USLPGRD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="ADDR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="FlowControl"/>
         <value>None</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet NMCLR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MSSEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="PS37_5"/>
         <value>64</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR9" settingAlias="U2CTSR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="SPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPTXEN11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIR" settingAlias="BTOEF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNCONC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FPOR"/>
         <value>15</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name AVSS1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllPrescaler"/>
         <value>12:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPSTALL11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="callBackRate"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXINV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNCONB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SPIFE" alias="Frame Sync pulse coincides"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIR" settingAlias="ATTACHIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPRXEN10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPHSHK5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPCONDIS14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNCONA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="VREGS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SMP" alias="Middle"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="SWR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIE" settingAlias="CRC16EE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="PPBMode"/>
         <value>Full Ping Pong</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB4" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="OSCIOFCN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPTXEN1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="DevicePID"/>
         <value>0xA</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="callBackRate"/>
         <value>0.000015</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPTXEN14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPTXEN4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR5" settingAlias="OCFAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="CLKSEL" alias="PBCLK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="BRGH" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPIRXI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS128"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPSTALL3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA0"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VDD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="SetDescriptorHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXISEL" alias="TX_ONE_CHAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="TRMT" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="IGNROV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="SE0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockSource"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TWIP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIE" settingAlias="STALLIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="BCDUSB"/>
         <value>0x200</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="T1MSECIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="BTSEF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN" alias="Request Switch"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="OVFDIS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPHSHK6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="OVFDIS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CP" alias="OFF"/>
         <value>2147483648</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VCAP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UBDTP1" settingAlias="BDTPTRL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="UART3_UTXIISRFunction"/>
         <value>ISR_UART3_UTXI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="SPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPITXI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSCHG" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART3" registerAlias="USTA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="USOF" settingAlias="CNT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART2" registerAlias="USTA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPHSHK8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPSTALL14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB0" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNSTATA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllTwoStagePostScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPSTALL8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPHSHK15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UARTEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="FlowControl"/>
         <value>None</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNSTATB"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPCONDIS11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB1" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllEnable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPDC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPSTALL11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="SESVD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="STALLIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPSTALL6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNSTATC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPSTALL11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPRXEN9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNAI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPSTALL9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc AVDD1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="VREGS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="USBI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA2" alias="analog"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR6" settingAlias="TCKIAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VUSB3V3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="LPRC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="STXISEL" alias="Buffer is more than half empty"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPCONDIS2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UBDTP1" settingAlias="BDTPTRL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="CF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB5" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="Clock and PLL selections are locked"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="STXISEL" alias="Buffer is not Full"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSYNC"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPRXEN9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TGATE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPHSHK5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXISEL" alias="RX_1_2_BUF_FULL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIE" settingAlias="BTOEE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXISEL"/>
         <value>TX_ONE_CHAR</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXISEL"/>
         <value>TX_ONE_CHAR</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXINV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA3"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR9" settingAlias="U2RXR"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="BTOEF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="SWRXBufferSize"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCON" settingAlias="RUNDIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UARTEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPCONDIS1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIR" settingAlias="DFN8EF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="ACTVIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPHSHK2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPTXEN7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLMULT"/>
         <value>12x</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UART2_UTXIISRFunction"/>
         <value>ISR_UART2_UTXI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="PPBRST" alias="Ping-Pong Buffer Pointers are not reset"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Center frequency"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UBDTP1" settingAlias="BDTPTRL" alias="enabled"/>
         <value>127</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UCNFG1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="STXISEL" alias="Buffer is completely empty"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR10" settingAlias="U3CTSR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPSTALL9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPRXEN6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="IDLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV" alias="FRC/8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS512"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="POR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPRXEN7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV" alias="FRC/2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="T1MSECIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV" alias="FRC/1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV" alias="FRC/4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA0"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA1"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="STSRC" alias="USB"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR0" settingAlias="RP3R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="RETVR"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="OERR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FDEVOPT"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPSTALL14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIE" settingAlias="DMAEE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCSEL" alias="ON"/>
         <value>4096</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllFeedbackDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIROV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="RETRYDIS0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RTSMD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPTXEN14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="STALLIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPTXEN5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="ProductString"/>
         <value>Gun prototype testing tool</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="ClockFrequency"/>
         <value>250000.00000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSELB"/>
         <value>8192</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART3" registerAlias="UBRG"/>
         <value>312</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART2" registerAlias="UBRG"/>
         <value>103</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SRXISEL"/>
         <value>Last Word is Read</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TSYNC" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPTXEN4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="BTSEF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPRXEN6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ABAUD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPSTALL0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB4" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="SE0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="LSTATE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR7" settingAlias="ICM7R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="RETRYDIS0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX_CTS_RTS"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="BRGH" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ABAUD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPRXEN3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX_BCLK"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="SESVD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxPll"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR11" settingAlias="SS2INR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA1"/>
         <value>digital</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0A" settingAlias="CNIE0A0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB3" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ACTIVE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPTXEN7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RTSMD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC9"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="URXI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPTXEN12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN"/>
         <value>TX_RX</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="UEN"/>
         <value>TX_RX</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="OSCPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DPPULDWN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMCNT"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="T32" alias="32 Bit"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ANSELA" settingAlias="ANSA2"/>
         <value>analog</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="IGNROV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPCONDIS8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UERI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UseSosc"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="BTOEF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPCONDIS13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIE" settingAlias="IDLEIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SMP" alias="End"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPHSHK2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITBF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPICON"/>
         <value>99616</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="ANSELA"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="IGNTUR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="D-"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="SPLL"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISC"/>
         <value>512</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BOR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIR" settingAlias="BTSEF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR1" settingAlias="RP8R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TWIP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="TimerPeriod"/>
         <value>1048.576s</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPTXEN7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="SIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SRXISEL" alias="Last Word is Read"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="CORETIMER" name="CoreTimerPeriod"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISB"/>
         <value>27895</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS1048576"/>
         <value>20</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB8" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="FVBUSIO"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS2048"/>
         <value>2816</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="RedirectPrintf"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RSWRST"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSDIS" alias="VBUS line is not discharged"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPCONDIS0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART2" registerAlias="UTXREG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART3" registerAlias="UTXREG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TGATE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MODE32" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPSTALL0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="WDTS" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WINDIS" alias="OFF"/>
         <value>128</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPSTALL5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="CRC16EF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="OERR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="PWRCON" settingAlias="RETEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="prescaleDivisor"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP15"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLICLK" alias="FRC"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Maximum frequency deviation"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="LPBACK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="CNSTYLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="URXI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="PORIO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPRXEN10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SLPEN" alias="Device will enter Idle mode when a WAIT instruction is issued"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLICLK" alias="POSC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="CORETIMER" registerAlias="CTI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOTRIM" settingAlias="ROTRIM"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="STALLIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPRXEN0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="PIDEE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="SOFIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="RedirectPrintf"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIR" settingAlias="DMAEF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP14"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SRXISEL" alias="Buffer is Full"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="STALLIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="PS50_0"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="STXISEL" alias="Complete"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPCONDIS3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS4096"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx3"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="SLPEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx2"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR2" settingAlias="ICM1R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="PGx1"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="WDTO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="SLPEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="URXI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPHSHK7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="TransferTerminatedHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="WATCHDOG" registerAlias="WDTCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR5" settingAlias="RP23R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="PullUp"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DMPULDWN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="ACTVIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR0" settingAlias="RP1R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="POSC_ERRATA_WORKAROUND"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPIRXI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIROVEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="TRISA"/>
         <value>12</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="SIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="CLKSEL" alias="SYSCLK"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="UTEYE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATC" settingAlias="LATC9" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="IREN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_RODIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB11"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB10"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="CORETIMER" name="CoreTimerFrequency"/>
         <value>1.2E7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB15"/>
         <value>SS1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB14"/>
         <value>SDI1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB13"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="IESO" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN"/>
         <value>36864</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="CLKSEL" alias="FRC"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="SWRXBufferSize"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DPPULDWN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMPOL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TCON" settingAlias="T32"/>
         <value>32 Bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FICD" settingAlias="JTAGEN"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UADDR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="USBSIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR4" settingAlias="RP19R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CP" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPRXEN8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPRXEN8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="CNSTYLE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXISEL" alias="RX_3_4_BUF_FULL"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIE" settingAlias="BTSEE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPSTALL0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN0A"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSDIS"/>
         <value>VBUS line is not discharged</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="PIDEE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UTOK"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIR" settingAlias="TRNIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="SESENDIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCS" alias="PBCLK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPostscalerOptions"/>
         <value>[1:256, 1:64, 1:32, 1:16, 1:8, 1:4]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="IREN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS65536"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMSYPW"/>
         <value>One-Clock</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="OERR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="ADDEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="ADDEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP5"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="T2CK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIROVEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN0B"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="localClockFreq"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="SOFIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="OSWEN"/>
         <value>Switch is Complete</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UPWRC" settingAlias="UACTPND" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="FRCDIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllClock"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DPPULUP"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="ALTI2C" alias="ON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP6"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS8192"/>
         <value>3328</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="ICS" alias="NONE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="CNSTYLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNEN0C"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXBF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="USBSIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX_RTS"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="WDTO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPSTALL15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP7"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIR" settingAlias="CRC16EF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="clockSourceSelect"/>
         <value>PBCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePoscErrataWorkaround"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB6" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPHSHK13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR7" settingAlias="ICM5R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPTXEN0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UERI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_FRC"/>
         <value>8000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPCONDIS11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPSTALL6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSDIS" alias="VBUS line is discharged through a resistor"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP8"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="SESVD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="BRGH" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSCHG" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP12"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SOSCRDY"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="SESENDIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNDI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB7" alias="set"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="CMR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV" alias="1:32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPHSHK8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="SLEEP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP13"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP11"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0" alias="clear"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="WDTS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="CMR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS" alias="1:256"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UART2_UERIISRFunction"/>
         <value>ISR_UART2_UERI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXDA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXDA"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP10"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS16384"/>
         <value>3584</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="WATCHDOG" name="clockSourceSelect"/>
         <value>CLOCK_LPRC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="WDTO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFC" settingAlias="CNFC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="REFCLKI"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPSTALL3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV" alias="1:16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC"/>
         <value>SPLL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="CKE" alias="Active to Idle"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="ACTVIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="timerExtPinSelection"/>
         <value>FALSE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UPWRC" settingAlias="UACTPND" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="LPRCRDY" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPCONDIS14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="LPRCRDY"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROSEL" alias="SOSC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="localClockFreq"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXBF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="DISSDO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR7"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="PllPostscaler"/>
         <value>1:4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="requestedPeriod"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_SYSCLK"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="ErrorHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIE" settingAlias="TRNIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR12" settingAlias="CLCINBR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR6"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TGATE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="SESENDIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FCKSM" alias="CSDCME"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="SESEND"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXINV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="NMICNT"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="timerExtPinSelection"/>
         <value>FALSE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="SetConfigurationHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TCON" settingAlias="ON"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="ON"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="D\+"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA4"/>
         <value>set</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPostscalerClock"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="SLPEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR5"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="PPBRST" alias="Resets all Ping-Pong Buffer Pointers to the even BD banks"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SLPEN"/>
         <value>Device will enter Idle mode when a WAIT instruction is issued</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FCKSM" alias="CSDCMD"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPHSHK4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="STSRC"/>
         <value>USB</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR9"/>
         <value>655360</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="requestedPeriod"/>
         <value>0.000015</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="VBUS"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPRXEN1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="ON"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPRXEN8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUA"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="RXINV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="RXINV"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPITUR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS" alias="1:64"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR8"/>
         <value>134217728</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPRXEN5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR1" settingAlias="RP6R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPCONDIS3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMSYNC"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPTXEN6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="SWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPHSHK8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPIRXI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV" alias="1:64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="CNPUB"/>
         <value>16384</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCON" settingAlias="WDTCLRKEY"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPrescalerClock"/>
         <value>96000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS256"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="ACTVIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="VBUSVD" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEP9"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPHSHK1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPSTALL6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet VDD5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="ATTACHIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATA"/>
         <value>16</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLMULT" alias="2x"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="UART3_UERIISRFunction"/>
         <value>ISR_UART3_UERI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="SESEND" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPRXEN5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX_BCLK"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="SESVDIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TGATE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="SOSCHP" alias="OFF"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="OTGEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPRXEN2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockFBDivisor"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UpdatePllPrescalerOptions"/>
         <value>[12:1, 8:1, 6:1, 4:1, 3:1, 2:1]</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLMULT" alias="3x"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPCONDIS6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="WakeupHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPIBRG"/>
         <value>47</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA3"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="CRC16EF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="FVBUSIO" alias="OFF"/>
         <value>32768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="BRGH" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLMULT" alias="4x"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPCONDIS9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="SESENDIF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNBI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPHSHK12" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="CF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPINR3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXINV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="ABAUD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="ABAUD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SSEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPCONDIS2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPTXEN0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="EnableSPIControl"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllPostScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPCONDIS0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPSTALL10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BCFGFAIL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TWDIS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPRXEN2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllScaler"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB5" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UEN" alias="TX_RX"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS16"/>
         <value>1024</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLMULT" alias="6x"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TWIP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="SOFHandler"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="StatusTO"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPHSHK14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPTXEN10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="DISSDO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="IREN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPCONDIS15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCA" settingAlias="ODCA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPTXEN3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="CMR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="DPPULDWN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRMT" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATB"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPTXEN13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="TMR2" registerAlias="TMR32"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR3" settingAlias="RP14R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOTRIM"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="SOSCPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCON" settingAlias="HOSTEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_OE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UADDR" settingAlias="LSPDEN" alias="Low Speed"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="ID" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="RCDIV" alias="FRC/256"/>
         <value>7</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="DFN8EF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="DIVSWEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="SESEND" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="UOEMON" alias="active"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLMULT" alias="8x"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="LATC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="CKP" alias="Idle:High, Active:Low"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS32"/>
         <value>1280</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIR" settingAlias="ATTACHIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="COSC" alias="FRCDIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPCONDIS6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATA" settingAlias="LATA1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS512"/>
         <value>2304</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SPLLRDY" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="UARTEN"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="UARTEN"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="LPBACK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB15"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB14"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB13"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR3" settingAlias="ICM4R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockChange"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPSTALL13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS64"/>
         <value>1536</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPHSHK0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UBDTP2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB11"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc RB10"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="SESVDIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CF" alias="No Clock Failure"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL" alias="9N"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRMT" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPTXEN10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="prescaleDivisor"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="LSTATEIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="CF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="SESENDIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPISGNEXT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SPLLRDY" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VUSB3V3"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UBDTP3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL" alias="8N"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL" alias="8O"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISC" settingAlias="TRISC9"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL" alias="8E"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPIROVEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UBDTP3" settingAlias="BDTPTRU" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP0" settingAlias="LSPD0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPTXEN10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="ROEN"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB5" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="ACTVIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB2" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPCONDIS3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="trisUserSetRB14"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="EPTXEN0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXISEL" alias="RX_ONE_CHAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS524288"/>
         <value>4864</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="MODE32" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONA" settingAlias="CNSTYLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UERI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="LPRC"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UBDTP1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA3" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockEnable"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TCON" settingAlias="SIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="STSRC" alias="SOSC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPSTALL10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TCON" settingAlias="SIDL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name AVDD1"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B8" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="IREN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPHSHK9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN" alias="PS75_0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SS1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXBRK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPISGNEXT" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXISEL" alias="RX_3_4_BUF_FULL"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPSTALL3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SOSCRDY" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="USBEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPRXEN7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPSTALL7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPCONDIS1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB15" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPIRXI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPSTALL1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPTXEN9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="FRMERR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPRXEN2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPIBUF" settingAlias="SPIBUF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="VBUSVDIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcEnable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SPI1_SPIRXIISRFunction"/>
         <value>ISR_SPI1_SPIRXI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMSYNC" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet VSS4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPCONDIS10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPCONDIS7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN" alias="BOR2"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNSTATC" settingAlias="CNSTATC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN" alias="BOR3"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="System Module" registerAlias="FICD"/>
         <value>24</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN" alias="BOR0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="BOREN" alias="BOR1"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPITXI" settingAlias="enable"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPTXEN13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS128"/>
         <value>1792</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPITXI" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UIR" settingAlias="RESUMEIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPCONDIS10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="RESUME" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SRMT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLODIV"/>
         <value>1:4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UERI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="TimerFrequency"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="OTGEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="ORNGPOL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS" alias="SOSC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="SPIFE"/>
         <value>Frame Sync pulse precedes</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Pin Module_CNBIISRFunction"/>
         <value>ISR_Pin Module_CNBI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB6"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP5" settingAlias="EPCONDIS5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMERREN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="SOSCSEL" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc AVSS1"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="DMAEE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="timerMaxCount"/>
         <value>4294967295</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS" alias="1:64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB9"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR11" settingAlias="SCK2INR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC"/>
         <value>SPLL</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="Transceiver"/>
         <value>Internal</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPRXEN4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPIRXI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPHSHK10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPSTALL13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB14" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UTOK" settingAlias="PID" alias="IN (RX) token type transaction"/>
         <value>9</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="LVD"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPCONDIS4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPSTALL4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="DFN8EF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA2" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="URXI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="FRCDIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllCpuDivScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="URXI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="DMAEE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAuxClockPostscaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UOTGIE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB14"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPTXEN6" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="POSCMOD" alias="EC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="POL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TMR" settingAlias="TMR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB7" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TMR" settingAlias="TMR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FSEC" settingAlias="CP"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPCONDIS4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPCONDIS13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPSTALL4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPTXEN3" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UERI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="WAKE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPITUREN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="CLKLOCK" alias="Clock and PLL selections are not locked and may be modified"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UERI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="POSCRDY"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="ATTACHIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="timerMaxCount"/>
         <value>65535</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="PDSEL"/>
         <value>8N</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="PDSEL"/>
         <value>8N</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="LPBACK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="SIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="TimerFrequency"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB6"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="POR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UEIR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB7"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB8"/>
         <value>SCK1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="SESENDIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB9"/>
         <value>SDO1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB2"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCONC" settingAlias="CNSTYLE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="POSCRDY" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB4"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="MASK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RB5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="MASK"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="TMR1_TIISRFunction"/>
         <value>ISR_TMR1_TI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FICD" settingAlias="JTAGEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FNOSC" alias="PRI"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TCKPS" alias="1:256"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="DeviceVID"/>
         <value>0x4D8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB8"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPRXEN9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="SLPEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPUA" settingAlias="CNPUA1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPTXEN9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="IDIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPHSHK7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name RC9"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="PERR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMSYNC" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="SESVDIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPTXEN2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SOSCRDY" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="FRMERR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="PR" settingAlias="PR"/>
         <value>27648</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUC" settingAlias="CNPUC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="PR" settingAlias="PR"/>
         <value>45</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="CRC16EE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPCONDIS1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRA0"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="PORCORE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIR" settingAlias="PIDEF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS" alias="1:32"/>
         <value>5</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B8" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3"/>
         <value>output</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATA" settingAlias="CNSTATA0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UOTGIR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAutoTune"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="CDCDevice" name="AbstractManagementD1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="CDCDevice" name="AbstractManagementD2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS524288"/>
         <value>19</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPRXEN15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Interrupt Module" name="GlobalInterrupt"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BOR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPICON2"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB4"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="CORETIMER" registerAlias="Compare" settingAlias="Compare"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB3"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXBRK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS"/>
         <value>PS1048576</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="VBUSVDIF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN1C" settingAlias="CNIE1C9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureUsb"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPHSHK7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP15" settingAlias="EPTXEN15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="CORETIMER" registerAlias="CTI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR2" settingAlias="RP9R"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="ODCB" settingAlias="ODCB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIBUSY" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="USTA" settingAlias="TRMT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="USTA" settingAlias="TRMT"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="T32" alias="16 Bit"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPHSHK4" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="localClockFreq"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="RXBUFELM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="IDLE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB13" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="SIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP9" settingAlias="EPTXEN9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNBI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPCONDIS13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR2" settingAlias="RP10R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPRXEN7" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="ADDEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB11" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="LSPD0" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="CORETIMER" registerAlias="Count"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="RESUME" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UTXI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGCON" settingAlias="VBUSON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXDA" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="DataModeSelect"/>
         <value>16 bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGSTAT" settingAlias="VBUSVD" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP0" settingAlias="LSPD0" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TNI" settingAlias="flag"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="USB_USBIISRFunction"/>
         <value>USBDeviceTasks</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_DIVSWITCH"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="CKE"/>
         <value>Active to Idle</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FrcPostscaler"/>
         <value>1:1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="ATTACHIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="DIVSWEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="ADDEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="FWDTEN" alias="OFF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPHSHK1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIR" settingAlias="VBUSVDIF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB11" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllEnable"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="LPBACK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="LPBACK"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP11" settingAlias="EPHSHK11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="DFN8EE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="maxPeriod"/>
         <value>178.956970625</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FDEVOPT" settingAlias="FUSBIDIO" alias="OFF"/>
         <value>16384</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIBUSY" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNEN0C" settingAlias="CNIE0C9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SOSCEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="PORCORE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="POSCMOD" alias="NONE"/>
         <value>768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPRXEN4" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="SIDL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPHSHK1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureAvcoDivider"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UIE"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR1" registerAlias="TI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="CLKSEL" alias="SYSCLK"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP6" settingAlias="EPTXEN6" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SDI1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR2" registerAlias="TCON" settingAlias="TCKPS" alias="1:16"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4"/>
         <value>input</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB5" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPCONDIS10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FailSafe"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeatureClockSwitching"/>
         <value>AVAILABLE</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPRXEN1" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPSTALL7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="maxPeriod"/>
         <value>0.021845</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_LPRC"/>
         <value>32000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="POL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR5" settingAlias="RP21R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="SLPEN" alias="Device will enter Sleep mode when a WAIT instruction is issued"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="ON" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR0"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP8" settingAlias="EPTXEN8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB10" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="FeaturePllDisplayScaler"/>
         <value>UNSUPPORTED</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RC9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="PORCORE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="Ep0Size"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIE" settingAlias="PIDEE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="LPBOREN" alias="ON"/>
         <value>8</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="CORETIMER" registerAlias="CTI" settingAlias="enable"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="USBRST" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="CRC16EE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VUSB3V3"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS4"/>
         <value>512</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS2"/>
         <value>256</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB5"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR4" settingAlias="RP17R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB6"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPRXEN1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="TXBUFELM" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB7"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB8"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB1"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="PIDEF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FPOR" settingAlias="RETVR" alias="OFF"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR0" settingAlias="RP4R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="RXINV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB15" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="LOCK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="IDIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB14" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS8"/>
         <value>768</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPCONDIS4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="PORIO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="URXDA" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UTOK" settingAlias="PID" alias="OUT (TX) token type transaction"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFOPinsOutput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="SPI1" name="SCK1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB2"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPHSHK13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="SIDL" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP4" settingAlias="EPSTALL4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="UI_OSCTUN_SETTING"/>
         <value>Center frequency</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIROV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="LPBACK" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="STEN"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="UART2_URXIISRFunction"/>
         <value>ISR_UART2_URXI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS1024"/>
         <value>10</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDMONO" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="TMR2_TIISRFunction"/>
         <value>ISR_TMR2_TI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="IDLEIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNCI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTPS" alias="PS32768"/>
         <value>3840</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="UERRIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="DMAEF" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="PORIO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="TMR1" registerAlias="TCON" settingAlias="TECS" alias="T1CK"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="DISSDI"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMCNT" alias="1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMCNT" alias="2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="RXINV" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR7" settingAlias="ICM8R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMCNT" alias="4"/>
         <value>2</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXISEL" alias="RX_ONE_CHAR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMCNT" alias="8"/>
         <value>3</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR5"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="clockSourceSelect"/>
         <value>PBCLK</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="SLEEP" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIE" settingAlias="CRC5EE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR3"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON" settingAlias="PLLMULT" alias="24x"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS64"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="anselUserSetRB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="DMAEF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB15" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="LPRCRDY" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="DeviceClass"/>
         <value>CDC</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR4"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIROV" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIR" settingAlias="PIDEF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR2"/>
         <value>6</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet NMCLR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="WAKE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA4" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="WAKE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN0B" settingAlias="CNIE0B9"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB11" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB14" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="FERR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNFB" settingAlias="CNFB10" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="JSTATE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="TXBUFELM"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UCON" settingAlias="PKTDIS"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="Pin Module" registerAlias="RPOR1"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLKPinsInput"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="SWNMI"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB4" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UPWRC"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FWDT" settingAlias="SWDTPS" alias="PS262144"/>
         <value>18</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="IDIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEIE" settingAlias="DFN8EE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="TXBUFELM" alias="enabled"/>
         <value>31</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCCON" settingAlias="NOSC" alias="SOSC"/>
         <value>4</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="CLOCK_PBCLK"/>
         <value>24000000</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="CKP" alias="Idle:Low, Active:High"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="LATB" settingAlias="LATB0"/>
         <value>clear</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="USBEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UTXI" settingAlias="priority"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="UTXBRK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="CKP"/>
         <value>Idle:Low, Active:High</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCON" settingAlias="JSTATE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="POSCRDY" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC9" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet AVSS1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPHSHK13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="UTXEN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPRXEN13" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPSTALL1" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPRXEN14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="WDTS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR1" name="timerBitMode"/>
         <value>16 Bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR2" settingAlias="RP12R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="Parity"/>
         <value>None</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBF" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="BCFGERR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART3" registerAlias="UMODE"/>
         <value>32776</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPII" settingAlias="context"/>
         <value>OFF</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="UART3_URXIISRFunction"/>
         <value>ISR_UART3_URXI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="USB" name="EnableStatusTO"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="UART2" registerAlias="UMODE"/>
         <value>32776</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FWDT" settingAlias="WDTWIN"/>
         <value>PS25_0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="ORNGPOL"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="SPI1" registerAlias="SPIBUF"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNCONB" settingAlias="ON" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="GNMI" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCON" settingAlias="SLPDIV"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON" settingAlias="FRMPOL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc NMCLR"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="USB" registerAlias="UIR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="LOCK" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="STSEL" alias="2"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB14" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="STSEL" alias="1"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR5" settingAlias="OCFBR"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UTXREG" settingAlias="UTXREG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP1" settingAlias="EPTXEN1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UTXREG" settingAlias="UTXREG"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="CLKSTAT" settingAlias="SPLLRDY"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP12" settingAlias="EPHSHK12"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNBI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.RegisterKey" moduleName="INTERNAL OSCILLATOR" registerAlias="SPLLCON"/>
         <value>33882240</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNFA" settingAlias="CNFA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="SOFIE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="TMR2" name="timerBitMode"/>
         <value>32 Bit</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="Parity"/>
         <value>None</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="ioc VDD5"/>
         <value>none</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART2" registerAlias="UMODE" settingAlias="BRGH"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="UART3" registerAlias="UMODE" settingAlias="BRGH"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="FRMERR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="VendorDevice" name="VendorClass"/>
         <value>Generic</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FPOR" settingAlias="LPBOREN"/>
         <value>ON</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="INTERNAL OSCILLATOR" name="REFCLKOUT_TRIM"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="FCKSM"/>
         <value>CSECME</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP14" settingAlias="EPSTALL14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="UMODE" settingAlias="OVFDIS" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP2" settingAlias="EPHSHK2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="ORNGPOL" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="FRMERREN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA3" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="CORETIMER" name="CORETIMER_CTIISRFunction"/>
         <value>ISR_CORETIMER_CTI</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPRXEN10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART3" name="inputmode"/>
         <value>easysetup</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDB" settingAlias="CNPDB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="System Module" registerAlias="FOSCSEL" settingAlias="OSCIOFCN" alias="ON"/>
         <value>1024</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPOR0" settingAlias="RP2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART2" registerAlias="USTA" settingAlias="FERR" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RB1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="PERR" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEIR" settingAlias="CRC5EF"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB2" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="Custom Name VDD5"/>
         <value/>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="REFOCON" settingAlias="RSLP" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="WATCHDOG" registerAlias="WDTCON" settingAlias="ON"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="STEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TMR32" settingAlias="TMR32"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="TMR2" registerAlias="TNI" settingAlias="SubPriority"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPUB" settingAlias="CNPUB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UCNFG1" settingAlias="UOEMON" alias="inactive"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="iocUserSet RA0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="OSCTUN" settingAlias="TUN" alias="Minimum frequency deviation"/>
         <value>32</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="SOFIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UIE" settingAlias="UERRIE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB0" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RCON" settingAlias="WDTO"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP13" settingAlias="EPRXEN13" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="SPITUREN" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="INTERNAL OSCILLATOR" registerAlias="RNMICON" settingAlias="GNMI" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISB" settingAlias="TRISB1" alias="output"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="USTA" settingAlias="URXEN" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="UART2" name="inputmode"/>
         <value>easysetup</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RB0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA0"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="UART3" registerAlias="UMODE" settingAlias="WAKE" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA1"/>
         <value>enabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNPDC" settingAlias="CNPDC9" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA2"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet RA4"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UPWRC" settingAlias="USBPWR"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPICON2" settingAlias="AUDMONO" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="customNameUserSet AVDD1"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNEN1B" settingAlias="CNIE1B0"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="SPI1" registerAlias="SPISTAT" settingAlias="SPIRBE" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="TRISA" settingAlias="TRISA1" alias="input"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UEP3" settingAlias="EPRXEN3"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="RPINR2" settingAlias="ICM2R"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB15"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="CNSTATB" settingAlias="CNSTATB15" alias="enabled"/>
         <value>1</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="Pin Module" registerAlias="ANSELB" settingAlias="ANSB13" alias="digital"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB10"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="USB" registerAlias="UOTGIE" settingAlias="IDIE"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP7" settingAlias="EPCONDIS7" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB13"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB14"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.OptionKey" moduleName="USB" registerAlias="UEP10" settingAlias="EPHSHK10" alias="disabled"/>
         <value>0</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.CustomKey" moduleName="Pin Module" name="RB11"/>
         <value>disabled</value>
      </entry>
      <entry>
         <key class="com.microchip.mcc.core.tokenManager.SettingKey" moduleName="Pin Module" registerAlias="CNPDA" settingAlias="CNPDA2"/>
         <value>disabled</value>
      </entry>
   </tokenMap>
   <generatedFileHashHistoryMap class="java.util.HashMap">
      <entry>
         <file>mcc_generated_files\interrupt_manager.h</file>
         <hash>96ecb5e7609da5466a9540e7ee1c43d4bef0e835474de6b1042acaa7f224dde8</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_ch9.h</file>
         <hash>cf44001600593bb74481dfc2840650881d54f9d252e1ebc33d8a1058a85b7f5c</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_hal_pic32mm.h</file>
         <hash>a4ddf4333e36e63639c65259d1a2341af2fb05ccc29e490f9be898996dd9868c</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_device_config.h</file>
         <hash>bf1d7cf61686e868798ae6fcc6c4f93ce550768afec2e7f70d462655c1b8f168</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\spi1.h</file>
         <hash>d6a5878715feede95d48c29c1497dfe39cc788c5365bd4223fe04a8fa8da6dab</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_device_cdc.h</file>
         <hash>8ea273e3cdcdd17d3a7273b5f2418217ee3db7ea7ca19de718e37666f6ede9dd</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_device_cdc.c</file>
         <hash>780a4d8080c29d0be4acad6b5af5853c1de6372cf6b74c9312051d73d49ce22c</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\spi1.c</file>
         <hash>fdd289d57bc949c20b36e96fdc43ef14ef0bbf716ed9a5acd1d40d6058821118</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.c</file>
         <hash>b869da9398750a9d5f7764ac1612ad4e0bb4ede6ce03a3806977acb567675ead</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_descriptors.c</file>
         <hash>3390e9c327e98ce1e6aa4d3a26a586f24b34d00e983489844500db783b8b5335</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\mcc.h</file>
         <hash>52c0935c2660b23169373e20468f742c50e9ffcd53c5b5f6d2b85ac79defb89f</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\exceptions.h</file>
         <hash>c90f711f98aecea019c2a2c33b3e3a7149160e3025c8cd47493f91a041f5c114</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb.h</file>
         <hash>c85994b17b6cfddd1066b5a99d1f73dfd684890fc4f829247adb983afca3716e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart2.h</file>
         <hash>881583411109319807d53d4313c6fb573247a03a36a865cd800f366d6b7b72aa</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\tmr1.h</file>
         <hash>077e2cbb0a61f42552152eaa05c995c85239a1c9aad16f5feb5b4a1a0350eeb2</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\exceptions.c</file>
         <hash>8103ed30cc4e59631b37783dc989257f0b2a2c83ba2a55ebfa12c442cbf5865f</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart3.c</file>
         <hash>6bc2f0193c216a18596ccc580fd7866cef29cd480292b20071c86e4ff2eeef74</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\tmr2.h</file>
         <hash>a4bd3a33edf989c481a30ec8121a18723216c499abccc094febbae42c839b01a</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_device.c</file>
         <hash>65f3426d310cdd6ac210f7745d806b0089364316281793e7c9f9a7f29b2d3a07</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart2.c</file>
         <hash>0e80296b858971c0fd2a3009fef04e4e1484d754a98e1f61dc571185cbb10b67</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\tmr2.c</file>
         <hash>4dedbabec3c738cefa343197ac833cf6f951b0ee27c5c52d0c8843af903e013b</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_device.h</file>
         <hash>294fbc496c530f618cc1e8ec935045df2f309570e2115e7930211da6eec0f843</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_device_local.h</file>
         <hash>7dcf0276e9b9f3f533e68da755a4fc8c191cf5dd790f8dc4b9be973b3a645e2a</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_device_events.c</file>
         <hash>7418b13bc43e76d5bd1662942242323a73ccaa4899a1b14262b438ea61b2c02c</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.h</file>
         <hash>a3ea9bd0727321994a2372219d3b98946d01d5cd05d00a5d5543424133536319</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\tmr1.c</file>
         <hash>ebca7504db42a16733eac62ef48ea44ea7d6a61554cf7dece6cd1c8b9816776b</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_hal.h</file>
         <hash>4e4ccc67c8e238ad1033ff8b9d04be5e9f00ba01ee536ac25d203cba119fe24b</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\uart3.h</file>
         <hash>47f56c7588014a5bebf45bb4c1abc5e06fdec7d1e7cd14363ac77868713574f0</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\pin_manager.c</file>
         <hash>fb03c20d88ef6faa80040e280c90d8b518fead0c24346ba0ec9cf67d9a8d4e3e</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\coretimer.c</file>
         <hash>77f551c2e3ebcdfc05ad44ff5bdb2bd84d7a257b57f48dcfaf32337174c64092</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\coretimer.h</file>
         <hash>b7b306e6d56a222b0402e4be17dc596fbfbeab2dc65c86c84161e47f0d660561</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\interrupt_manager.c</file>
         <hash>0fd503a1f8f463b267444cd19b63dca82315bda80b9632605e7d4fc1324a085a</hash>
      </entry>
      <entry>
         <file>mcc_generated_files\usb\usb_common.h</file>
         <hash>86617caf86de4aaa4596cea9bd17678c049be0be66d8ab6d0a0fa994bbaee7cd</hash>
      </entry>
   </generatedFileHashHistoryMap>
</config>