=============================================================================
List of generated methods in project: vga2scart

THIS TEXT DESCRIPTION IS GENERATED BY THE TOOL. DO NOT MODIFY IT.
=============================================================================

Module "HSync"     (bean Capture)
   - HSync_GetCaptureValue -This method gets the last value captured by enabled timer (see implementation note in <General 
                Info>). The method does not return valid value after initialization or after <Reset> until new capture event 
                (even if the returned Error code is ERR_OK).
   - HSync_GetPinValue -The method reads the Capture pin value. The method is available only if it is possible to read the pin 
                value (usually not available for internal signals).

Module "HSyncTimeout" (bean FreeCntr)
   - HSyncTimeout_Reset -This method resets the timer-counter (sets to zero for up-counting HW or to appropriate value for 
                down-counting HW). The method is available only if the counter register can be set by software and the counter 
                is not shared.

Module "CSyncEn"   (bean BitIO)
   - CSyncEn_SetDir -Sets a pin direction (available only if the direction = _[input/output]_).
   - CSyncEn_GetVal -Returns the input/output value. If the direction is [input] then the input value of the pin is read and 
                returned. If the direction is [output] then the last written value is returned (see <Safe mode> property for 
                limitations). This method cannot be disabled if direction is [input].
   - CSyncEn_PutVal -The specified output value is set. If the direction is [input], the component saves the value to a memory 
                or a register and this value will be written to the pin after switching to the output mode (using 
                [SetDir(TRUE)]; see <Safe mode> property for limitations). If the direction is [output], it writes the value to 
                the pin. (Method is available only if the direction = _[output]_ or _[input/output]_).
   - CSyncEn_ClrVal -Clears (set to zero) the output value. It is equivalent to the [PutVal(FALSE)]. This method is available 
                only if the direction = _[output]_ or _[input/output]_.
   - CSyncEn_SetVal -Sets (to one) the output value. It is equivalent to the [PutVal(TRUE)]. This method is available only if 
                the direction = _[output]_ or _[input/output]_.

Module "CSyncInv"  (bean BitIO)
   - CSyncInv_GetVal -Returns the input/output value. If the direction is [input] then the input value of the pin is read and 
                returned. If the direction is [output] then the last written value is returned (see <Safe mode> property for 
                limitations). This method cannot be disabled if direction is [input].
   - CSyncInv_PutVal -The specified output value is set. If the direction is [input], the component saves the value to a memory 
                or a register and this value will be written to the pin after switching to the output mode (using 
                [SetDir(TRUE)]; see <Safe mode> property for limitations). If the direction is [output], it writes the value to 
                the pin. (Method is available only if the direction = _[output]_ or _[input/output]_).
   - CSyncInv_ClrVal -Clears (set to zero) the output value. It is equivalent to the [PutVal(FALSE)]. This method is available 
                only if the direction = _[output]_ or _[input/output]_.
   - CSyncInv_SetVal -Sets (to one) the output value. It is equivalent to the [PutVal(TRUE)]. This method is available only if 
                the direction = _[output]_ or _[input/output]_.

Module "VSync"     (bean Capture)
   - VSync_GetCaptureValue -This method gets the last value captured by enabled timer (see implementation note in <General 
                Info>). The method does not return valid value after initialization or after <Reset> until new capture event 
                (even if the returned Error code is ERR_OK).
   - VSync_GetPinValue -The method reads the Capture pin value. The method is available only if it is possible to read the pin 
                value (usually not available for internal signals).

Module "RgbStatus" (bean BitIO)
   - RgbStatus_GetVal -Returns the input/output value. If the direction is [input] then the input value of the pin is read and 
                returned. If the direction is [output] then the last written value is returned (see <Safe mode> property for 
                limitations). This method cannot be disabled if direction is [input].
   - RgbStatus_PutVal -The specified output value is set. If the direction is [input], the component saves the value to a 
                memory or a register and this value will be written to the pin after switching to the output mode (using 
                [SetDir(TRUE)]; see <Safe mode> property for limitations). If the direction is [output], it writes the value to 
                the pin. (Method is available only if the direction = _[output]_ or _[input/output]_).
   - RgbStatus_ClrVal -Clears (set to zero) the output value. It is equivalent to the [PutVal(FALSE)]. This method is available 
                only if the direction = _[output]_ or _[input/output]_.
   - RgbStatus_SetVal -Sets (to one) the output value. It is equivalent to the [PutVal(TRUE)]. This method is available only if 
                the direction = _[output]_ or _[input/output]_.

Module "Cpu"       (bean MC9S08QD4_8)
   - Cpu_EnableInt -Enables maskable interrupts
   - Cpu_DisableInt -Disables maskable interrupts

===================================================================================
