RF22

- Main Page
- Classes
- Files
- Examples

- Class List
- Class Hierarchy
- Class Members

Public Attributes | List of all members
RF22Mesh::MeshRouteDiscoveryMessage Struct Reference

`#include <RF22Mesh.h>`

## Public Attributes
MeshMessageHeader | header
| msgType = RF22_MESH_MESSAGE_TYPE_ROUTE_DISCOVERY_*
uint8_t | destlen
| Reserved. Must be 1.g.
uint8_t | dest
| The address of the destination node whose route is being sought.
uint8_t | route [RF22_MESH_MAX_MESSAGE_LEN-1]
| List of node addresses visited so far. Length is implcit.

## Detailed Description

Signals a route discovery request or reply At present only supports physical dest addresses of length 1 octet

The documentation for this struct was generated from the following file:

- RF22Mesh.h