RF22

- Main Page
- Classes
- Files
- Examples

- Class List
- Class Hierarchy
- Class Members

- All
- Functions
- Variables
- Enumerations
- Enumerator

- _
- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

Here is a list of all documented class members with links to the class documentation for each member:

### - s -

- send() : RF22
- sendNextFragment() : RF22
- sendto() : RF22Datagram
- sendtoWait() : RF22Mesh , RF22ReliableDatagram , RF22Router
- setBitOrder() : GenericSPIClass , HardwareSPIClass , SoftwareSPIClass
- setClockDivider() : GenericSPIClass , HardwareSPIClass , SoftwareSPIClass
- setCRCPolynomial() : RF22
- setDataMode() : HardwareSPIClass , SoftwareSPIClass , GenericSPIClass
- setFHChannel() : RF22
- setFHStepSize() : RF22
- setFrequency() : RF22
- setHeaderFlags() : RF22
- setHeaderFrom() : RF22
- setHeaderId() : RF22
- setHeaderTo() : RF22
- setMaxHops() : RF22Router
- setMode() : RF22
- setModeIdle() : RF22
- setModemConfig() : RF22
- setModemRegisters() : RF22
- setModeRx() : RF22
- setModeTx() : RF22
- setPins() : SoftwareSPIClass
- setPreambleLength() : RF22
- setPromiscuous() : RF22
- setRetries() : RF22ReliableDatagram
- setSyncWords() : RF22
- setThisAddress() : RF22Datagram
- setTimeout() : RF22ReliableDatagram
- setTxPower() : RF22
- setWutPeriod() : RF22
- source : RF22Router::RoutedMessageHeader
- spiBurstRead() : RF22
- spiBurstWrite() : RF22
- spiRead() : RF22
- spiWrite() : RF22
- startTransmit() : RF22
- state : RF22Router::RoutingTableEntry
- statusRead() : RF22