RF22

- Main Page
- Classes
- Files
- Examples

- Class List
- Class Hierarchy
- Class Members

Class List
Here are the classes, structs, unions and interfaces with brief descriptions:
[detail level 1 2]

GenericSPIClass | Base class for SPI interfaces
HardwareSPIClass | Encapsulate the Arduino hardware SPI interface
RF22 | Send and receive unaddressed, unreliable datagrams
ModemConfig | Defines register values for a set of modem configuration registers
RF22Datagram | RF22 subclass for addressed, unreliable messages
RF22Mesh | RF22 subclass for sending addressed, optionally acknowledged datagrams multi-hop routed across a network, with automatic route discovery
MeshApplicationMessage | Signals an application layer message for the caller of RF22Mesh
MeshMessageHeader | Structure of the basic RF22Mesh header
MeshRouteDiscoveryMessage |
MeshRouteFailureMessage | Signals a route failure
RF22ReliableDatagram | RF22 subclass for sending addressed, acknowledged, retransmitted datagrams
RF22Router | RF22 subclass for sending addressed, optionally acknowledged datagrams multi-hop routed across a network
RoutedMessage | Defines the structure of a RF22Router message
RoutedMessageHeader |
RoutingTableEntry | Defines an entry in the routing table
SoftwareSPIClass | Encapsulate a software SPI interface